;
; VCDS Label File
;
; Copyright © 2007-2009 Ross-Tech, LLC
;
; Skoda Octavia (1U)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 1U?-919-???-???
;
; includes measuring blocks, adaptation, coding, login and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1U-17.LBL
; 1Ux-919-xxx-17.LBL
; 1U0-920-xxx-17.LBL
;
; created on 29/Jun/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 11/Mar/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
;
003,0,General
003,1,Coolant,Temperature
;
020,0,Immobilizer - ID Block 1
020,1,Digit 1 && 2
020,2,Digit 3 && 4
020,3,Digit 5 && 6
020,4,Digit 7 && 8
;
021,0,Immobilizer - ID Block 2
021,1,Digit 9 && 10
021,2,Digit 11 && 12
021,3,Digit 13 && 14
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+02 = Seatbelt Warning active
C03,xx?xx: Country
C04,1 = Europe / 2 = USA / 3 = Canada/Mexico/Latin America
C05,4 = Great Britain (GB) / 5 = Japan / 6 = Saudi Arabia / 7 = Australia
C06,xxx?x: Cylinders
C07,4 = 4-Cylinders
C08,xxxxx?: Distance Impulse Number (K-Value)
C09,0 = Diesel Engines (excl. TDI 81kW from MY 1999+)
C10,2 = Other Engines (incl. TDI 81kW from MY 1999+)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,8 = Czech
;
A5,0,Service reminder - Maximum distance for oil change "OIL"
A5,5,Service reminder - Maximum distance for oil change (in 1000km)
A5,6,15 - 15.000km (Standard)
;
A6,0,Service reminder - Maximum distance "INSP 01"
A6,5,Service reminder - Maximum distance (in 1000km)
A6,6,30 - 30.000km (Standard)
;
A7,0,Service reminder - Maximum time "INSP 02"
A7,5,Service reminder - Maximum time (in 10 Days)
A7,6,37 - 370 Days (Standard)
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km.
A009,11, 
A009,12,NOTE: Perform Login first.
;
;
A10,0,Service reminder - Distance for oil change "OIL"
A10,5,Service reminder - Distance for oil change (in 1000km)
A10,6,15 - 15.000km (Standard)
;
A11,0,Service reminder - Distance "INSP 01"
A11,5,Service reminder - Distance (in 1000km)
A11,6,30 - 30.000km (Standard)
;
A12,0,Service reminder - Time "INSP 02"
A12,5,Service reminder - Time (in 10 Days)
A12,6,37 - 370 Days (Standard)
;
A016,0,Distance Impulse Number
;
A017,0,Distance Impulse Number
;
A021,0,Immobilizer - Key Adaptation
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,10,Oil Change (OEL),1000,km
RD,11,Inspection 1 (IN1),1000,km
RD,12,Inspection 2 (IN2),10,Days
;
RJ,0,0,Service Reset (Oil Service),,
RJ,0,1,10,15
;
RJ,1,0,Service Reset (Inspection),,
RJ,1,1,10,15
RJ,1,2,11,30
;
RJ,2,0,Service Reset (Oil Service & Inspection),,
RJ,2,1,10,15
RJ,2,2,11,30
RJ,2,3,12,37
;
