;
; VCDS Label File
;
; Audi A6 (4B)
;
; Component: Engine (#01) - AJP
;
; P/N: 4B0-907-557-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4B-01.LBL
; 06B-907-557-AJP.LBL  (1.8l E   @ 125 HP - AJP)
;
; created on 10/May/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 10/May/2008
;
; requires VCDS 803.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
000,0,Basic Function
000,1,Coolant Temperature,Specification: 170...204 (80..105 °C)
000,2,Engine Load,Specification: 18...50 (0.92...2.50 ms)
000,3,Engine Speed,Specification: 70...92 (700...920 RPM)
000,4,Supply Voltage,Specification: 142...206 (10.0...14.5 V)
000,5,Throttle Valve Angle,Specification: 0...12 (0.0...5.0 <°)
000,6,Idle Air Control,Specification: 123...133 (-3.0...+3.0 kg/h)
000,7,Idle Air Control (learned),Specification: 120...136 (-4.0....+4.0 kg/h)
000,8,Lambda Regulation (learned),Specification: 77...179 (-10.0...+10.0 %)
000,9,Lambda Regulation (learned - additive),Specification: 115...141 (-0.64...+0.64 ms)
000,10,Lambda Regulation (learned - multiplicative),Specification: 117...138 (-8.0...+8.0 %)
;
001,0,Basic Function
001,1,Engine Speed,,Specification (idle): 700...920 RPM
001,2,Engine Load,,Specification: 0.92...2.50 ms
001,3,Throttle Body Angle,,Specification (Idle): 0...5 <°\nSpecification (Load): 85...90  <°
001,4,Ignition Angle,,Specification: 6.0...12.0 °BTDC
;
002,0,Basic Function
002,1,Engine Speed,,Specification (idle): 700...920 RPM
002,2,Injection Period,(theoretical),Specification: 0.92...2.50 ms
002,3,Injection Period,(corrected),Specification: 2.0...5.0 ms
002,4,Intake Air Mass,,Specification: 2.0...4.0 g/s
;
003,0,Basic Function
003,1,Engine Speed,,Specification (idle): 700...920 RPM
003,2,Supply Voltage,,Specification: 10.0...14.5 V
003,3,Coolant,Temperature,Specification: 80...105 °C
003,4,Intake Air,Temperature,Specification: approx. outside Temperature
;
004,0,Idling Speed Stabilisation
004,1,Throttle Body Angle,,Specification: 0...5 <°
004,2,Intake Air Mass,(idle/learned),Specification: -1.7...1.7 g/s
004,3,Intake Air Mass,(load/learned),Specification: -1.7...1.7 g/s
004,4,Operating Mode,,Specification: Idle/Throttle/Enrich
;
005,0,Idling Speed Stabilisation
005,1,Engine Speed,(actual),Specification (idle): 700...920 RPM
005,2,Engine Speed,(specified),Specification: 700...920 RPM
005,3,Idle Regulation,,Specification: -10.0...+10.0 %
005,4,Intake Air Mass,,Specification: 2.0...4.0 g/s
;
006,0,Idling Speed Stabilisation
006,1,Engine Speed,,Specification (idle): 700...920 RPM
006,2,Idle Regulation,,Specification: -10.0...+10.0 %
006,3,Lambda,Regulation,Specification: -10.0...+10.0 %
006,4,Ignition Angle,,Specification: 6.0...12.0 °BTDC
;
007,0,Lambda Control
007,1,Lambda,Regulation,Specification: -10.0...+10.0 %
007,2,Lambda Probe,Voltage,Specification: +0.1...+1.1 V
007,3,Charcoal Filter,Solenoid Valve,Specification: 0.0...99.0 %
007,4,Lambda Correction,Factor,Specification: 0.3...1.2
;
008,0,Lambda learnt Values
008,1,Injection Period,(corrected),Specification: 2.0...5.0 ms
008,2,Lambda Regulat.,(learned - additive),Specification: -10.0...+10.0 %
008,3,Lambda Regulat.,(learned - multipl.),Specification: -8.0...+8.0 %
008,4,Fuel Tank,Venting
;
009,0,Lambda learnt Values
009,1,Engine Speed,,Specification (idle): 700...920 RPM
009,2,Lambda,Regulation,Specification: -10.0...+10.0 %
009,3,Lambda Probe,Voltage,Specification: +0.1...+0.3 and +0.7...+1.0 V
009,4,Lambda Regulat.,(learned - additive),Specification: -10.0...+10.0 %
;
010,0,Fuel Tank Breather
010,1,Charcoal Filter,Solenoid Valve,Specification: 0.0...99.0 %
010,2,Lambda Correction,Factor,Specification: 0.30...1.2
010,3,Charcoal Filter,Charge Level,Specification: -5.0...+45.0 %
010,4,Fuel Tank Venting,Purge Rate,Specification: 0.0...0.3 %
;
011,0,Fuel Consumption
011,1,Engine Speed,,Specification (idle): 700...920 RPM
011,2,Engine Load,,Specification: 0.92...2.50 ms
011,3,Vehicle Speed,,Specification: 0 km/h
011,4,Fuel Consumption,,Specification: 0.5...1.5 l/h
;
012,0,Fuel Consumtion (during Idling)
012,1,Engine Speed,,Specification (idle): 700...920 RPM
012,2,Supply Voltage,,Specification: 10.0...14.5 V
012,3,Fuel Consumption,,Specification: 0.5...1.5 l/h
012,4,Ignition Angle,,Specification: 6.0...12.0 °BTDC
;
013,0,Knock Control (Timing Retardation - Cylinder 1 - 4)
013,1,Timing Retardation,Cylinder 1,Specification: 0...12 °BTDC
013,2,Timing Retardation,Cylinder 2,Specification: 0...12 °BTDC
013,3,Timing Retardation,Cylinder 3,Specification: 0...12 °BTDC
013,4,Timing Retardation,Cylinder 4,Specification: 0...12 °BTDC
;
014,0,Knock Control (Timing Retardation - Cylinder 1 && 2)
014,1,Engine Speed,,Specification (idle): 700...920 RPM
014,2,Engine Load,,Specification: 0.92...2.50 ms
014,3,Timing Retardation,Cylinder 1,Specification: 0...12 °BTDC
014,4,Timing Retardation,Cylinder 2,Specification: 0...12 °BTDC
;
015,0,Knock Control (Timing Retardation - Cylinder 3 && 4)
015,1,Engine Speed,,Specification (idle): 700...920 RPM
015,2,Engine Load,,Specification: 0.92...2.50 ms
015,3,Timing Retardation,Cylinder 3,Specification: 0...12 °BTDC
015,4,Timing Retardation,Cylinder 4,Specification: 0...12 °BTDC
;
016,0,Knock Control (Sensor Signal - Cylinder 1 - 4)
016,1,Knock Sensor,Cylinder 1,Specification: 0.4...2.0 V
016,2,Knock Sensor,Cylinder 2,Specification: 0.4...2.0 V
016,3,Knock Sensor,Cylinder 3,Specification: 0.4...2.0 V
016,4,Knock Sensor,Cylinder 4,Specification: 0.4...2.0 V
;
017,0,Catalyst Converter Heating
017,1,Engine Speed,,Specification (idle): 700...920 RPM
017,2,Engine Load,,Specification: 0.92...2.50 ms
017,3,Energy Balance,Cat Heating
017,4,Ignition Angle,,Specification: 6.0...12.0 °BTDC
;
018,0,Altitude Correction
018,1,Engine Speed,,Specification (idle): 700...920 RPM
018,2,Engine Load,(bef. Correction),Specification: 0.92...2.50 ms
018,3,Engine Load,(aft. Correction)
018,4,Altitude Correction,Factor,Specification: -30...+20 %
;
019,0,Torque Reduction (only with automatic transmission)
019,1,Engine Speed,,Specification (idle): 700...920 RPM
019,2,Engine Load,,Specification: 0.92...2.50 ms
019,3,Ignition Angle,Retardation
019,4,Ignition Angle,,Specification: 6.0...12.0 °BTDC
;
020,0,Operating States
020,1,Engine Speed,,Specification (idle): 700...920 RPM
020,2,Selector Lever,Position,Display Range: Neutral/Gear ENG.
020,3,Air Conditioning,Operating Mode,Display Range: A/C High/Low
020,4,Air Conditioning,Status,Display Range: Compr. ON/OFF
;
021,0,Lambda Control
021,1,Engine Speed,,Specification (idle): 700...920 RPM
021,2,Engine Load,,Specification: 0.92...2.50 ms
021,3,Coolant,Temperature,Specification: 80...105 °C
021,4,Lambda Control,Operating Mode,Display Range: Reg. ON/OFF
;
023,0,Throttle Body Adaptation Information
023,1,Adaptation Status,,Specification: 100000
; 0xxxxx - Throttle Potentiometer adjustment with Idling Potentiometer not OK
; x1xxxx - Throttle Body Adaptation not OK
; xx1xxx - Learning process Max. Position Throttle Potentiometer not OK
; xxx1xx - Learning process Min. Position Throttle Potentiometer not OK
; xxxx1x - Learning process Max. Position Idling Potentiometer not OK
; xxxxx1 - Learning process Min. Position Idling Potentiometer not OK
023,2,Throttle Body,Min. Position,Specification: 72...95 %
023,3,Throttle Body,Emergency Stop,Specification: 67...83 %
023,4,Throttle Body,Max. Position,Specification: 18...54 %
;
024,0,Knock Control
024,1,Engine Speed
024,2,Engine Load,,Specification: 0.92...2.50 ms
024,3,Ignition Angle
024,4,Timing Retardation,Sum of Cyl. 1-4
;
025,0,Closed Loop Control
025,1,Operating Mode,,Specification: Idle/Throttle/Enrich
025,2,Phase Position,(Hall Sensor)
025,3,Operating Mode,,x-----0x = Intake Manifold Changeover OFF\nx-----x0 = Camshaft Timing Control OFF
025,4,Camshaft,Adjustment Angle,Specification (Normal): -3.0...+3.0 °KW\nSpecification (Adjusted): -15.0...+21.0 °KW
;
026,0,Closed Loop Control
026,1,Engine Speed,,Specification (idle): 700...920 RPM
026,2,Engine Load,,Specification: 0.92...2.50 ms
026,3,Operating Mode,,x-----0x = Intake Manifold Changeover OFF\nx-----x0 = Camshaft Timing Control OFF
26,4,Camshaft,Adjustment Angle,Specification (Normal): -3.0...+3.0 °KW\nSpecification (Adjusted): -15.0...+21.0 °KW
;
027,1,Operating Mode,,Specification: Idle/Throttle/Enrich
027,3,Coolant,Temperature,Specification: 80...105 °C
;
095,0,Basic Function
095,1,Engine Speed,,Specification (idle): 700...920 RPM
095,2,Engine Load,,Specification: 0.92...2.50 ms
095,3,Ignition Angle,,Specification: 6.0...12.0 °BTDC
095,4,Coolant,Temperature,Specification: 80...105 °C
;
098,0,Throttle Body Adaptation (Basic Setting)
098,1,Throttle Valve,Potentiometer,Specification: 0.5...4.9 V
098,2,Idling Positioner,Potentiometer
098,3,Operating Mode,,Specification: Idle/Throttle/Enrich
098,4,Adaption Status,,Specification: ADP OK\nDisplay Range: ADP OK/ADP RUN/ERROR
;
099,0,Lambda Control (Basic Setting)
099,1,Engine Speed
099,2,Coolant,Temperature,Specification: 80..105 °C
099,3,Lambda,Regulation,Specification: -10.0...+10.0 %
099,4,Status Lambda,Regulation,Display Range: Reg. ON/OFF
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine Control Unit (J220) Coding
C01,??xxx: Country/Emissions
C02,02 = Non EU-Member (MVEG I)
C03,04 = EU-Member (MVEG II)
C04,08 = China and CIS
C05,xx?xx: Drive/Additional Functions
C06,0 = Front-Wheel-Drive (FWD)
C07,2 = All-Wheel-Drive (AWD)
C08,xxx?x: Transmission
C09,0 = 5-Speed Manual Transmission
C10,3 = Automatic Transmission (01N)
C11,5 = Automatic Transmission (01V)
C12,xxxx?: Vehicle Type
C13,1 = Class B (e.g. Audi A4 / VW Passat)
C14,2 = Class C (e.g. Audi A6)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Idle Speed
A001,1,Engine Speed,(actual)
A001,2,Engine Speed,(specified)
A001,3,A/C Readiness,,Range: A/C-Low / A/C-High
A001,4,A/C Compressor,,Range: Compr.OFF/Compr.ON
; 
A091,0,Immobilizer Status
A091,5,Immobilizer Status (Read Only)
A091,6,0 = Immobilizer not matched (NEW)
A091,7,1 = Immobilizer disabled
A091,8,4 = Immobilizer matched (System OK)
;
