;
; VCDS Redirect File
;
; Copyright © 2007-2009 Ross-Tech, LLC
;
; Seat Leon/Toledo (1M)
;
; Component: A/C Heating Electronics (J255) (#01) - Climatronic
;
; P/N: 1M0-820-043-???
;
; includes measuring blocks, basic setting and coding
;
; created on 30/Jul/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 30/Aug/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
000,0,Flap Motors
000,1,Temperature Regulator Flap Motor (V68),Specified Value: 0
000,2,Central Air Flap Motor (V70),Specified Value: 0
000,3,Footwell/Defroster Flap Motor (V85),Specified Value: 0
000,4,Air Flow Flap Motor (V71),Specified Value: 0
;
B001,0,Potentiometer && Flap Alignment
B001,1, , , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
001,0,General
001,1,Comprossor,Shut-Off,Specification: 0 = Compressor Running (See Label File for more Details)
;  0 = Compressor Running
;  1 = Compressor OFF by Pressure Switch (F129): Refrigerant Pressure too High
;  3 = Compressor OFF by Pressure Switch (F129): Refrigerant Pressure too Low
;  6 = Compressor OFF by ECON Button
;  7 = Compressor OFF by OFF Button (via Fresh Air Blower Speed Buttons)
;  8 = Compressor OFF by Ambient Temperature below 3 °C (37 °F)
; 10 = Compressor OFF by Voltage below 9.5 V
; 12 = Compressor OFF by Engine OR Transmission Control Module
; 13 = Compressor OFF by Compressor Activation Delay)
; 14 = Compressor OFF by Pressure Switch (F129) 30 times activated
001,2,Spannung elektr.-,magnet. Kupplung,(N25)
001,3,Spannung,(Klemme 15)
001,4,Standzeit,,Zeitraum zwischen letztem Ausschalten und Wiedereinschalten der Zündung (Wertebereich: 0...240)
;
002,0,Temperature Regulator Flap Motor (V68/G92)
002,1,Measured Value,Potentiom. (G92),Range: 0...255\nTolerance (to Spec.): 3
002,2,Specified Value,Potentiom. (G92),Range: 0...255\nSpecification: 5...250
002,3,Flap Position,(Cooling),Specification: 5...50
002,4,Flap Position,(Heating),Specification: 190...250
;
003,0,Central Air Flap Motor (V70/G112)
003,1,Measured Value,Potentiom. (G112),Range: 0...255\nTolerance (to Spec.): 3
003,2,Specified Value,Potentiom. (G112),Range: 0...255\nSpecification: 5...250
003,3,Flap Position,Lower Stop,Specification: 5...50
003,4,Flap Position,Upper Stop,Specification: 190...250
;
004,0,Footwell/Defroster Flap Motor (V85/G114)
004,1,Measured Value,Potentiom. (G114),Range: 0...255\nTolerance (to Spec.): 3
004,2,Specified Value,Potentiom. (G114),Range: 0...255\nSpecification: 5...250
004,3,Flap Position,Lower Stop,Specification: 5...50
004,4,Flap Position,Upper Stop,Specification: 190...250
;
005,0,Air Flow Flap Motor (V71/G113)
005,1,Measured Value,Potentiom. (G113),Range: 0...255\nTolerance (to Spec.): 3
005,2,Specified Value,Potentiom. (G113),Range: 0...255\nSpecification: 5...250
005,3,Flap Position,Upper Stop,Specification: 5...30
005,4,Flap Position,Lower Stop,Specification: 210...250
;
006,0,Temperatures I && Photo Sensor
006,1,Calculated,Temperature,Calculated from temperature sensor (G89) and outside air temperature sensor (G17)
006,2,Fresh Air Duct,Temperature (G89)
006,3,Outside Air,Temperature (G17)
006,4,Sunlight Photo,Sensor (G107),Range: 0.0...100.0 % (equals 4.5...0.5 V)
;
007,0,Temperatures II
007,1,Center Vent (G191),Temperature
007,2,Footwell (G192),Temperature
007,3,Dash Panel (G56),Temperature 
007,4,Coolant,Temperature
;
008,0,Voltages
008,1,Fresh Air Blower,(V2 - specified),Display Range: 0 V = Blower Off / 3.6 V = Blower Speed 1 / 12 V = Blower Speed 7
008,2,Fresh Air Blower,(V2 - actual),Specification: ± 0.8 V to Specification (in Field 1)
008,3,Voltage,(Terminal 58d),Specification: 2.0...12.5 V
008,4,Parking Light,(Terminal 58),Range: 0 = inactive | 1 = active
;
009,0,Vehicle Data
009,1,Engine Speed
009,2,Vehicle Speed
009,3,Aux. Heating,,Range: 0 = inactive | 1 = active
;
010,1,Thermo Switch,Coolant Temp.,Specification: 0
; 0 = Thermo Switch open (Coolant Temperature OK)
; 1 = Thermo Switch closed (Coolant Temperature too High)
010,2,Compressor,Intervention
010,3,Pressure Switch,(F129)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Heating/Air Condition (J255) Coding
C01,00040 = 4-Cylinder Gasoline Engine (Left-Hand-Drive)
C02,00041 = 4-Cylinder Gasoline Engine (Right-Hand-Drive)
C03,00043 = 4-Cylinder Diesel Engine (Left-Hand-Drive)
C04,00044 = 4-Cylinder Diesel Engine (Right-Hand-Drive)
C05,00050 = 5-Cylinder Gasoline Engine (Left-Hand-Drive)
C06,00051 = 5-Cylinder Gasoline Engine (Right-Hand-Drive)
;
