;
; VCDS Label File
;
; Copyright © 2006-2010 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J234 - Airbag (#15) - 9.41
;
; P/N: 4E0-910-655-???
;
; includes measuring blocks, basic setting, coding, security access
;          and adaptation
;
; created on 22/Apr/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 26/May/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Igniter Status (Airbag && Tensioner)
001,1,Driver Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Passenger Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Driver Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Passenger Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
B001,0,Seat Occupied Recognition Control Module (J706) Basic Setting
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Igniter Status (Tensioner && Battery Disconnect)
002,1,Rear Left Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Rear Right Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Rear Center Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Battery Disconnect,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat Occupation && Belt Inquiry
003,1,Voltage supply,,Display Range: Correct/Signal too Low/Signal too High
003,2,Seat Occupation,Detection Passenger,Display Range: Child Seat/Light Adult/Medium Adult/Heavy Adult/Not Occup./Short to Ground/Short to Plus/Not Installed
003,3,Belt Inquiry,Driver,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Passenger,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry (Rear)
004,1,Belt Inquiry,Rear Left,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Right,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniter Status (Side Airbag)
005,1,Front Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Front Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Rear Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Rear Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
007,0,Igniter Status (Head Airbag)
007,1,Driver Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Passenger Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch Status
010,1,Key Switch,Passenger Airbag,Display Range: ON/OFF
010,2,Key Switch,(HW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
010,3,Key Switch,(SW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Igniter Status (Airbag Stage 2 && Knee Airbag)
011,1,Driver Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Passenger Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
016,0,Seat Occupation Recognition (J706)
016,1,Control Module,Serial: 1st/2nd digit
016,2,Control Module,Serial: 3rd/4th digit
016,3,Control Module,Serial: 5th digit
016,4,Control Module,Calibration
;
018,0,Seat Occupation Detection
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration Sensor
;
019,0,Workshop Codes
019,1,Workshop Code,(Last Coding),of seat occupation detection
019,2,Workshop Code,(Last 0 Calibration),of seat occupation detection
;
020,0,Power Supply
020,1,Voltage,(Terminal 15)
;
021,0,Igniter Resistance (Airbag && Tensioner)
021,1,Driver Airbag,Igniter,Specification: 2.1...5.6 Ohm
021,2,Passenger Airbag,Igniter,Specification: 1.6...5.6 Ohm
021,3,Driver Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
021,4,Passenger Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
;
022,0,Igniter Resistance (Tensioner && Battery)
022,1,Rear Left Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,2,Rear Right Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,3,Rear Center Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,4,Battery Disconnect,Igniter,Specification: 1.6...5.6 Ohm
;
025,0,Igniter Resistance (Side Airbag)
025,1,Front Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,2,Front Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,3,Rear Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,4,Rear Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
027,0,Igniter Resistance (Head Airbag)
027,1,Driver Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
027,2,Passenger Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
031,0,Igniter Resistance (Airbag Stage 2 && Knee Airbag)
031,1,Driver Airbag,Igniter (Stage 2),Specification: 2.1...5.6 Ohm
031,2,Passenger Airbag,Igniter (Stage 2),Specification: 1.6...5.6 Ohm
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Brake Electronics,,Specification: ABS 1
125,3,Immobilizer
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Instrument Cluster
225,2,Brake Electronics
225,3,Immobilizer
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Airbag 9.41 (J234) Coding
C01,0?xxxxx: Options I
C02,4 = without Knee Airbag (PR-4UE/4UF)
C03,5 = with Knee Airbag (PR-4UH/4UP)
C04,0x?xxxx: Stages
C05,3 = Standard
C06,0xx?xxx: Options II
C07,0 = without Passenger Airbag Shut-Off (PR-4UE/4UH+9P0/9P1)
C08,1 = with Passenger Airbag Shut-Off via Key Switch (PR-4UF/4UP+9P0/9P1)
C09,2 = with Passenger Airbag Shut-Off with Seat Occupation Detection (PR-4UH+9P5)
C10,0xxx?xx: Side Airbags
C11,7 = Front & Rear Side Airbags with Head Airbags (PR-4X4)
C12,0xxxx?x: Belt Inquiry
C13,0 = Standard
C14,0xxxxx?: Belt Tensioner
C15,5 = with electrically adjustable single seats (4-Seater / PR-5Z1)
C16,7 = without electrically adjustable single seats (5-Seater / PR-5Z0)
;
;
;---------------------------------------------------
;
; security access information
;
;---------------------------------------------------
;
;
S00,Airbag (J234) Security Access
S01,20324 = Seat Occupied Recognition Basic Setting/Zero Balancing
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A000,0,Seat Occupied Recognition Reset
A000,5,Seat Occupied Recognition Reset
A000,6,If a repair on the Seat Occupied Recognition
A000,7,has been performed a reset has to be performed too.
A000,8, 
A000,9,Prerequisites:
A000,10,* Seat in normal position.
A000,11,* Seat must NOT be occupied during the whole procedure.
A000,12,* Seatbelt must NOT be plugged in.
A000,13,* No faults in the system.
A000,14,* Interior temperature must be between 0 °C and 37 °C (32 °F and 98 °F).
A000,15, 
A000,16,NOTE: Perform Security Access first.
;
