;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; Audi A6 (4F)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 4F0-910-???-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4F-17.LBL
; 4F0-910-xxx-17.LBL
;
; includes measuring blocks, adaptation, coding, security access
;          selective output test and service reset
;
; created on 14/Jul/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 12/Oct/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring block
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,(1.2 bar)
001,4,Time
;
002,0,General
002,1,Mileage
002,2,Remote Clock,(Test Mode)
002,3,Tank Content
;
003,0,General
003,1,Coolant,Temperature
003,2,Standing Time
003,3,Dimming Signal,(Terminal 58d)
003,4,Dimming Signal,(Terminal 58s)
;
004,0,Supply Voltage && Outside Temperature
004,1,Supply Voltage,(Terminal 30)
004,2,Outside Temp.,(NTC)
004,3,Outside Temp.,(via CAN),from Climate Control
004,4,Outside Temp.,(Display)
;
005,0,Service Reminder
005,1,Distance since,Service exceeded,Unit: 100 km
005,2,Time since,Service exceeded,Unit: 1 day(s)
005,3,Remaining dist.,until Service,Unit: 100 km
005,4,Remaining time,until Service,Unit: 1 day(s)
;
006,1,Min. (M2) Oil Level,in Service Interval
006,2,Max. (M2) Oil Level,in Service Interval
006,3,Long Time Average,Oil Level Dif.,
006,4,Engine Hood,Contact,Display Range: Open/Closed
;
007,1,Min. (M3) Oil Level,in Service Interval
007,2,Max. (M3) Oil Level,in Service Interval
007,3,Fast Average,Oil Level Dif.,
;
010,0,Adaptation Channel 003
010,1,Adaptation,Channel
010,2,Consumption,Correction,See Adaptation Channel 003
;
011,0,Adaptation Channels 009 && 019
011,1,Adaptation,Channel
011,2,Mileage,,See Adaptation Channel 009
011,3,Adaptation,Channel
011,4,Remote Control,Clock Synchron.,See Adaptation Channel 019
;
012,0,Adaptation Channels 040 && 041
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 040
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 041
;
013,0,Adaptation Channels 042 && 043
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 042
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 043
;
014,0,Adaptation Channels 044 && 049
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 044
014,3,Adaptation,Channel
014,4,Minimum Time,to Service,See Adaptation Channel 049
;
015,0,Adaptation Channel 045
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 045
;
016,0,Adaptation Channels 047 && 048
016,1,Adaptation,Channel
016,2,Soot Entry,,See Adaptation Channel 047
016,3,Adaptation,Channel
016,4,Thermal Load,,See Adaptation Channel 048
;
019,0,Adaptation Channels 029 && 030
019,1,Adaptation,Channel
019,2,Fuel Gauge,Sender 2,See Adaptation Channel 029
019,3,Adaptation,Channel
019,4,Fuel Gauge,Sender 1,See Adaptation Channel 030
;
020,0,Adaptation Channel 035
020,1,Adaptation,Channel
020,2,Engine Speed,Threshold,See Adaptation Channel 035
;
021,0,Adaptation Channels 038 && 039
021,1,Adaptation,Channel
021,2,Oil Minimum,Detection Sensor,See Adaptation Channel 038
021,3,Adaptation,Channel
021,4,TOG,,See Adaptation Channel 039
;
026,0,Fuel Sender(s)
026,1,Fuel Sender 1,(Resistance)
026,2,Fuel Sender 1,(Tank Content)
026,3,Fuel Sender 2,(Resistance)
026,4,Fuel Sender 2,(Tank Content)
;
029,0,Wheel Circumference
029,1,Mean wheel,circumference,used for odometer
029,2,Max. wheel,circumference,used for speedometer
;
120,0,Connector Status I
120,1,Brake Fluid,Connector
120,2,Washer Fluid,Connector
120,3,Coolant Level,Connector
120,4,Oil Level,Connector
;
121,0,Connector Status II
121,1,Brake Pad Waer,Indicator Connect.
;
124,0,CAN-Databus Error Counter
124,1,CAN-Databus,Error Counter
;
125,0,CAN-Databus Communication (Powertrain)
125,1,CAN-Gateway,,Specification: Gateway 1
;
220,0,Miscellaneous
220,1,Sum of Fill,Level Differences
220,2,Count of summed,Fill Level Diff.
;
221,0,Miscellaneous
221,1,Theoretical,Service Interval,Increments: 1.000 km
221,2,Year Driving,Performance,Increments: 100 km
221,3,Short Time Average,Oil Level Dif.
221,4,After Totalling,Fill Level Values
;
222,0,Miscellaneous
222,1,Minimum Mileage,to Service,Increments: 1.000 km
222,2,Maximum Mileage,to Service,Increments: 1.000 km
222,3,Minimum Time,to Service,Increments: 1 month
222,4,Maximum Time,to Service,Increments: 1 month
;
223,0,Miscellaneous
223,1,Average Driving,Distance
;
224,1,Curr. (M2) Oil Level,in Service Interval
224,2,Error Counter,Component Prot.
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Instrument Cluster (J285) Security Access
S01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once before
A009,10,the current value is not over 100 km/62 mi.
A009,11,After changing the value can be corrected
A009,12,within the next 5 km/3 mi.
;
A019,0,Remote Clock
A019,5,Remote Clock
A019,6,Set the remote clock synchronization time.
A019,7, 
A019,8,0 = Remote Clock not installed
A019,9,1...50 = Synchronization Time (in minutes)
;
A029,0,Tank Characteristic (Fuel Level Sensor 2)
A029,5,Tank Characteristic (Fuel Level Sensor 2)
A029,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A029,7, 
A029,8,Standard Value: 128
A029,9,Value Range: 96...160 (-8.0...+8.0 l)
A029,10,Increments: 1 = 1 Ohm = 1/4 l
;
A030,0,Tank Characteristic (Fuel Level Sensor 1)
A030,5,Tank Characteristic (Fuel Level Sensor 1)
A030,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A030,7, 
A030,8,Standard Value: 128
A030,9,Value Range: 96...160 (-8.0...+8.0 l)
A030,10,Increments: 1 = 1 Ohm = 1/4 l
;
A031,0,Tank Characteristic (Wet Calibration)
;
A032,0,Tank Characteristic (Not detactable Tank Volume)
A032,5,Tank Characteristic (Not detactable Tank Volume)
A032,6,The tank volume which is not recordable by the fuel gauge
A032,7,sender(s). Make sure to enter this value before performing
A032,8,the "wet calibration" (Channel 031).
;
A033,0,Tank Characteristic (Full Calibration)
A033,5,Tank Characteristic (Full Calibration)
A033,6,Non-parallel shift of the tank characterictic above a readout of 1/2.
A033,7,To start the adaptation enter '65535' as new value.
A033,8, 
A033,9,Standard Value: 128
A033,10,Value Range: 112...144 (-4.0...+4.0 l)
A033,11,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
A035,9, 
A035,10,NOTE: Perform Security Access first.
;
A038,0,Oil Minimum Detection
A038,5,Oil Minimum Detection
A038,6,With this function the oil-minimum-warning at
A038,7,low oil level can be deactivated or activated.
A038,8,0 = Oil Minimum Detection not activated
A038,9,1 = Oil Minimum Detection activated
A038,10, 
A038,11,NOTE: Perform Security Access first.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
A039,7,0 = TOG Evaluation from the Instrument Cluster not activated
A039,8,1 = TOG Evaluation from the Instrument Cluster activated
A039,9, 
A039,10,NOTE: Perform Security Access first.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km/mi
A040,7, 
A040,8,NOTE: Adaptation channels 040-049 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 040-049 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km/mi
A042,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A042,8,00150 - flexible Service Intervals (15.000 km - with Longlife)
A042,9,or (if coded to miles)
A042,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A042,11,00090 - flexible Service Intervals (9.000 mi - with Longlife)
A042,12, 
A042,13,NOTE: Adaptation channels 040-049 must be
A042,14,entered and stored in the following order:
A042,15,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km/mi
A043,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A043,8,00300 - flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A043,11,00190 - flexible Service Intervals (19.000 mi - with Longlife)
A043,12, 
A043,13,NOTE: Adaptation channels 040-049 must be
A043,14,entered and stored in the following order:
A043,15,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 - fixed Service Intervals (w/o Longlife)
A044,8,00730 - flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 040-049 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 - fixed Service Intervals (w/o Longlife)
A045,7,2 - flexible Service Intervals (with Longlife)
A045,8, 
A045,9,NOTE: Adaptation channels 040-049 must be
A045,10,entered and stored in the following order:
A045,11,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display
A046,8, 
A046,9,NOTE: Adaptation channels 040-049 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 040-049 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 040-049 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 - fixed Service Intervals (w/o Longlife)
A049,8,00365 - flexible Service Intervals (Gasoline Engines with Longlife)
A049,9,00730 - flexible Service Intervals (Diesel Engines with Longlife)
A049,10, 
A049,11,NOTE: Adaptation channels 040-049 must be
A049,12,entered and stored in the following order:
A049,13,45 > 42 > 43 > 49 > 44 > 40 > 41 > 46 > 47 > 48
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,????xxx: Options
C02,+0001 = Quattro (2nd Tank Characteristic) / +0002 = Driver Information System (DIS) inactive
C03,+0004 = Vehicle with Clutch (NO Automatic) / +0008 = Second Tire Size Pair (only within first 100 km/61 mi)
C04,+0016 = Tire Pressure Monitoring installed / +0032 = Adaptive Air Suspension installed
C05,+0064 = Advanced Frontlighting System (AFS) installed / +0128 = Adaptive Cruise Control (ACC) installed
C06,+0256 = 70-Liter Fuel Tank (only Front-Wheel-Drive) / +1024 = Vehicle Symbol Avant/Wagon
C07,+2048 = Switch Option for Bord Computer Levels (MY 2006+)
C08,xxxx?xx: Country
C09,0 = Germany / 1 = Rest of World (Left-Hand-Drive) / 2 = USA / 3 = Canada
C10,4 = Great Britain / 5 = Japan (Left-Hand-Drive) / 6 = Arabian States
C11,7 = Australia / 8 = Rest of World (Right-Hand-Drive) / 9 = Japan (Right-Hand-Drive)
C12,xxxxx?x: Seatbelt Warning (< MY 2007 / 3-6 = MY 2005-2007)
C13,0 = No Seatbelt Warning  / 1 = Seatbelt Warning (EU-NCAP)
C14,2 = Seatbelt Warning (NAR Old) / 3 = Seatbelt Warning (NAR New)
C15,4 = Seatbelt Warning (EU-NCAP incl. Passenger) / 5 = Seatbelt warning (NAR Old incl. Passenger)
C16,6 = Seatbelt Warning (NAR New incl. Passenger)
C17,xxxxx?x: Seatbelt Warning (MY 2008 >)
C18,0 = Seatbelt Warning inactive
C19,5 = Seatbelt Warning EURO NCAP (incl. Passenger) active
C20,8 = Seatbelt Warning USA NAR (incl. Passenger) active
C21,xxxxxx?: Illumination & Washer Fluid Warning
C22,0 = Needles OFF and Scales OFF (Term. 15 ON / Term. 58 OFF) / 1 = Needles ON and Scales OFF (Term. 15 ON / Term. 58 OFF)
C23,2 = Needles OFF and Scales ON (Term. 15 ON / Term. 58 OFF) / 3 = Needles ON and Scales ON (Term. 15 ON / Term. 58 OFF)
C24,+5 = Washer Fluid Warning active
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T666,Chime/Buzzer/Gong
T694,Switch and Instrument Lighting
T798,Segment Test
T1150,Analog Indicators
T1298,Instrument Cluster Lamp Test
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,100,DIST
RD,43,Max Mileage to Service,100,DIST
RD,44,Max Time to Service,1,Days
RD,45,Oil Quality,1,
RD,47,Soot Quantity,100,DIST
RD,48,Thermal Load,100,DIST
RD,49,Min Time to Service,1,Days
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Change to Fixed Intervals (Kilometers),,ST_FIXED
RJ,1,1,45,1
RJ,1,2,42,80
RJ,1,3,43,80
RJ,1,4,44,365
RJ,1,5,49,365
;
; Change to flexible intervals (kilometers)
RJ,2,0,Change to Flexible Intervals (Kilometers),ST_DIESEL,ST_FLEXIBLE
RJ,2,1,45,2
RJ,2,2,42,150
RJ,2,3,43,300
RJ,2,4,44,730
RJ,2,5,49,730
;
; Change to flexible intervals (kilometers)
RJ,3,0,Change to Flexible Intervals (Kilometers),ST_GASOLINE,ST_FLEXIBLE
RJ,3,1,45,2
RJ,3,2,42,150
RJ,3,3,43,300
RJ,3,4,44,730
RJ,3,5,49,365
;
; Change to fixed intervals (miles)
RJ,4,0,Change to Fixed Intervals (Miles),,ST_FIXED
RJ,4,1,45,1
RJ,4,2,42,50
RJ,4,3,43,50
RJ,4,4,44,365
RJ,4,5,49,365
;
; Change to flexible intervals (miles)
RJ,5,0,Change to Flexible Intervals (Miles),ST_DIESEL,ST_FLEXIBLE
RJ,5,1,45,2
RJ,5,2,42,90
RJ,5,3,43,190
RJ,5,4,44,730
RJ,5,5,49,730
;
; Change to flexible intervals (miles)
RJ,6,0,Change to Flexible Intervals (Miles),ST_GASOLINE,ST_FLEXIBLE
RJ,6,1,45,2
RJ,6,2,42,90
RJ,6,3,43,190
RJ,6,4,44,730
RJ,6,5,49,365
;
