;
; VCDS Label File
;
; Copyright © 2010+ Ross-Tech, LLC
;
; Seat Arosa (6H) / VW Lupo (6E/6X)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 6X0-920-???-???
;
; includes measuring blocks, adaptation, coding,
;          login and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 6H-17.LBL
; 6X-17.LBL
; 6X0-920-xxx-17.LBL
;
; created on 06/Dec/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 21/Apr/2012
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Equipment
C02,+01 = Brake Pad Warning installed
C03,+02 = Seatbelt Warning installed
C04,+04 = Washer Fluid Warning installed
C05,xx?xx: Country
C06,0 = Germany (DE) / 1 = Europe (EU) / 2 = USA (US) / 3 = Canada (CDN)
C07,4 = Great Britain (GB) / 5 = Japan (JP) /6 = Saudi Arabia (SA) / 7 = Australia (AUS)
C08,xxx?x: Service Intervals
C09,0 = fixed Service Intervals without Oil Level/Temperature Sensor (PR-QG0)
C10,1 = flexible Service Intervals with Oil Level/Temperature Sensor (PR-QG1)
C11,2 = fixed Service Intervals with Oil Level/Temperature Sensor (PR-QG2)
C12,3 = without Service Intervals (USA/Canada)
C13,xxxx?: Engine Type (Distance Impulse Number)
C14,1 = 1.4l@55kW (4297)
C15,2 = 1.4l@44kW/1.6l@74kW Autom./2.0l@85kW/1.8l@110-132kW/1.9l@66-81kW TDI (3480)
C16,3 = 1.6l@74kW Manual/1.9l@50kW SDI (4078)
C17,4 = 1.9l@74-96kW TDI-PD (3599)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A02,0,Service Reminder
A02,5,Service Reminder
A02,6,Displayed Values:
A02,7,01 = Oil Service due
A02,8,10 = Inspection due
A02,9,11 = Oil Service & Inspection due
A02,10, 
A02,11,New Values:
A02,12,00 = Reset Oil Service & Inspection
A02,13,10 = Reset Oil Service
A02,14,01 = Reset Inspection
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A005,0,Service Reminder: Max. Distance to Oil Service "OIL"
A005,5,Service Reminder: Max. Distance to Oil Service "OIL" (in 1000 km/mi)
A005,6,15 = 15.000 km (Standard)
A005,7,or (if coded)
A005,8,10 = 10.000 mi (Standard)
;
A006,0,Service Reminder: Max. Distance to Inspection "INSP 01"
A006,5,Service Reminder: Max. Distance to Inspection "INSP 01" (in 1000 km/mi)
A006,6,30 = 30.000 km (Standard)
A006,7,or (if coded)
A006,8,20 = 20.000 mi (Standard)
;
A007,0,Service Reminder: Max. Time to Inspection "INSP 02"
A007,1,Max. Time
A007,2,Inspection
A007,3,in Month
A007,5,Service Reminder: Max. Time to Inspection "INSP 02" (in 1 Months)
A007,6,12 = Standard (12 Month)
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,7, 
A009,8,The distance can only be changed once until
A009,9,the current value is not over 100 km/62 mi.
A009,10, 
A009,11,NOTE: Perform Login first.
;
A010,0,Service Reminder: Distance to Oil Service "OIL"
A010,5,Service Reminder: Distance to Oil Service "OIL" (in 100 km/mi)
A010,6,150 = 15.000 km (Standard)
A010,7,or (if coded)
A010,8,100 = 10.000 mi (Standard)
;
A011,0,Service Reminder: Distance to Inspection "INSP 01"
A011,5,Service Reminder: Distance to Inspection "INSP 01" (in 100 km/mi)
A011,6,300 = 30.000 km (Standard)
A011,7,or (if coded)
A011,8,200 = 20.000 mi (Standard)
;
A012,0,Service Reminder: Time to Inspection "INSP 02"
A012,5,Service Reminder: Time to Inspection "INSP 02" (in 1 Days)
A012,6,360 = 360 Days (Standard)
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 9 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
A035,9, 
A035,10,Standard: 0
A035,11,Range: 0...1000 U/min
A035,12,Increments: 250 U/min
;
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Max. Distance to Oil Service "OIL",1000,DIST
RD,6,Max. Distance to Inspection "INSP 01",1000,DIST
RD,7,Max. Time to Inspection "INSP 02",1,Month(s)
RD,10,Remaining Distance to Oil Service "OIL",100,DIST
RD,11,Remaining Distance to Inspection "INSP 01",100,DIST
RD,12,Remaining Time to Inspection "INSP 02",1,Day(s)
;
RJ,0,0,Service Reset (Oil Service & Inspection),,
RJ,0,1,2,0
;
RJ,1,0,Service Reset (Oil Service),,
RJ,1,1,2,10
;
RJ,2,0,Service Reset (Inspection),,
RJ,2,1,2,1
;
RJ,3,0,Service Reset (Oil Service & Inspektion - Indivdual Channels/Kilometers),,
RJ,3,1,10,150
RJ,3,2,11,300
RJ,3,3,12,360
;
RJ,4,0,Service Reset (Oil Service - Indivdual Channels/Kilometers),,
RJ,4,1,10,150
;
RJ,5,0,Service Reset (Inspection - Indivdual Channels/Kilometers),,
RJ,5,1,10,150
RJ,5,2,11,300
;
RJ,6,0,Service Reset (Oil Service & Inspektion - Indivdual Channels/Miles),,
RJ,6,1,10,100
RJ,6,2,11,200
RJ,6,3,12,360
;
RJ,7,0,Service Reset (Oil Service - Indivdual Channels/Miles),,
RJ,7,1,10,100
;
RJ,8,0,Service Reset (Inspection - Indivdual Channels/Miles),,
RJ,8,1,10,100
RJ,8,2,11,200
;
