;
; VCDS Label File
;
; Copyright © 2009 Ross-Tech, LLC
;
; Audi A8 (4D)
;
; Component: J104 - Brake Electronics (#03) - Bosch 5.0 ABS/EDS/ASR
;
; P/N: 4D0-907-379-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4D-03.LBL
; 4D0-907-379-ABS.LBL (Bosch 5.0 ABS & ABS/EDS)
; 4D0-907-379-ASR.LBL (Bosch 5.0 ABS/EDS/ASR)
; 4D0-907-379-ESP.LBL (Bosch 5.0 ABS/EDS/ASR/ESP)
;
; created on 23/Mar/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 23/Mar/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right,Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0.0...255.0 km/h
;
002,0,Status Bits
002,1,Brake Light Switch,,Display Range: 0/1
002,2,Return Flow Pump,,Display Range: 0/1
002,3,Solenoid Valve,Relay,Display Range: 0/1
;
003,0,Traction Control (ASR)
003,1,Engine Speed
003,2,Engine Torque,,0.0 % = Schubphase\n20.0...30.0 % = Idle\n100.0 % = Maximum Torque
003,3,ASR-Button,,0 = Not Oper.\n1 = Operated
;
;
;---------------------------------------------------
;
; Codierung
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104/Bosch 5.0) Coding
C01,00000 = 2.8l 6-Cylinder with Manual Transmission (012)
C02,00001 = 2.8l 6-Cylinder with Automatic Transmission (01K)
C03,00002 = 3.7l 8-Cylinder with Automatic Transmission (01V)
C04,00003 = 2.8l 6-Cylinder with Automatic Transmission (01V)
;
