;
; VCDS Label File
;
; Copyright © 2011 Ross-Tech, LLC
;
; Audi A2 (8Z) / Audi A3 (8L) / Audi A4 (8D/8E) / Audi A6 (4B) / Audi A8 (4D)
;
; Component: R - Radio/Navigation System (#56) RNS-D
;
; P/N: ??0-035-192-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4B-56.LBL
; 4D-56.LBL
; 8D-56.LBL
; 8E-56.LBL
; 8L-56.LBL
; 8Z-56.LBL
; 4B0-035-192-RNSD-56.LBL
;
; created on 25/Apr/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 25/Apr/2011
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Speed Signal,recognized,Range: 0 = not recognized / 1 = recognized
001,2,Supply Voltage,(Terminal 30),Range: 0.0...20.0 V\nSpecification: 8.0...15.0 V
001,3,Illumination,(Terminal 58d)
001,4,Ignition Status,(Terminal S),Range: ON/OFF
;
002,0,Speaker/Line-Out
002,1,Speaker/Line-Out,Location/Type
002,2,Speaker/Line-Out,Status
002,3,Speaker/Line-Out,Location/Type
002,4,Speaker/Line-Out,Status
;
003,0,Antenna
003,1,Antenna Type,,Range: active/passive
003,2,Antenna
003,3,Antenna,Status
;
004,0,General
004,1,Amplifier,Output,0 = OK\n1 = Short to Ground
004,3,Telephone
004,4,Telephone,Mute Status,Range: ON/OFF
;
005,0,Communication Status CD-Changer (R41)
005,1,CD-Changer,(R41)
005,2,CD-Changer,Status
;
006,0,External Display
006,1,External Display
006,2,External Display,Status,Range: OK/n.OK
;
007,0,Production Diagnostics
007,1,System,Status,Specification: 255\n\n+001 = CAN-Communication Navigation System OK\n+002 = Current Draw for GPS-Antenna (10-30 mA) OK\n+004 = Terminal 15 (Ignition ON) recognized\n+008 = Backup-Light Switch recognized\n+016 = CAN-Communication Instrument Cluster OK\n+032 = Signal Wheel Impulse at least once recognized\n+064 = Wheel Impulse Adaptation OK\n+128 = Tire Circumference Adaptation OK
; +001 = CAN-Communication Navigation System OK
; +002 = Current Draw for GPS-Antenna (10-30 mA) OK
; +004 = Terminal 15 (Ignition ON) recognized
; +008 = Backup-Light Switch recognized
; +016 = CAN-Communication Instrument Cluster OK
; +032 = Signal Wheel Impulse at least once recognized
; +064 = Wheel Impulse Adaptation OK
; +128 = Tire Circumference Adaptation OK
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R/RNS-D) Coding
C01,00?xx: Speakers
C02,0 = Sound System (No passive Speakers)
C03,1 = 1 passive Speaker (Front Left for Bose Sound System with Telephone)
C04,2 = 2 passive Speakers (Front) and 2 active Speakers (Rear)
C05,5 = 2 passive Speakers (Front) and no active Speakers (Rear)
C06,00x?x: Sound System Correction
C07,0 = No Sound System (No Correction)
C08,1 = Sound System (Bose)
C09,00xx?: Configuration
C10,+1 = Active/Remote Supplied Antenna
C11,+2 = CD-Changer
C12,+4 = Secondary Display (Board Computer/Navigation)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Tire Circumference
A001,5,Tire Circumference
A001,6,The tire circumference is beeing adapted in "mm".
A001,7,A tire circumference list can be found here:
A001,8, 
A001,9,http://de.openobd.org/audi/rns.htm#reifen
;
A002,0,Wheel Impulse
A002,5,Wheel Impulse
A002,6,The Distance Impulse describes the amount
A002,7,of ABS Pulses per Wheel Revolution.
A002,8, 
A002,9,39 = Audi A2 (8Z) with 1.2l Economy
A002,10,43 = Audi A2 (8Z) with all other Engines
A002,11,45 = Audi A3 (8L) / Audi A4 (8D/8E) / Audi A6 (4B) / Audi A8 (4D)
;
A003,0,Production Diagnostics
A003,5,Production Diagnostics
A003,6,The Result of the Production Diagnostics is
A003,7,displayed in Measuring Value Block 007 Field 1.
A003,8, 
A003,9,0 = Production Diagnostics inactive
A003,10,1 = Production Diagnostics active
;
A004,0,Instrument Cluster Display
A004,5,Instrument Cluster Display
A004,6,RNS 4.0 & 4.1 (< CW 44/2001)
A004,7,0 = Monochrome Display
A004,8,1 = Color Display
A004,9, 
A004,10,RNS 4.2 (CW 45/2001 >)
A004,11,0 = Monochrome Display (< MY 2001)
A004,12,1 = Monochrome Display (MY 2002 >)
;
A005,0,Country
A005,5,Country
A005,6,0 = Europe (EU)
A005,7,1 = North American Region (NAR)
;
A006,0,Telematics
A006,5,Telematics
A006,6,1 = Telematics not installed
A006,7,3 = Telematics installed
;
A007,0,Options
A007,5,Options
A007,6,+1 = Card Reader installed
A007,7,+2 = Multi-Function-Steering-Wheel (MFSW) installed (through KW 45/2001 - RNS 4.2)
A007,8,+4 = TV-Tuner installed (from KW 45/2001 - RNS 4.2)
A007,9,+8 = Voice Control installed (from KW 45/2001 - RNS 4.2)
;
A009,0,Speakers/Model
A009,5,Speakers/Model
A009,6,Suppresses a Fault Code which would otherwise be stored when installed
A009,7,in Audi A4 Cabriolet (8H) Speakers are connected via a Capacitor.
A009,8, 
A009,9,0 = Audi A4 (8E) Limousine/Avant
A009,10,1 = Audi A4 (8H) Cabriolet
;
A099,0,Transport Mode
A099,5,Transport Mode
A099,6,0 = Transport Mode OFF
A099,7,1 = Transport Mode ON
;
