;
; VCDS Label File
;
; Copyright © 2007-2012 Ross-Tech, LLC
;
; Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia (1Z)
; VW Caddy (2K) / VW Eos (1F) / VW Golf/Jetta (1K/5M)
; VW Passat (3C) / VW Touran (1T)
;
; Component: J387 - Passenger Door Electronics (#52) MIN Generation 3
;
; P/N: ???-959-702-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-52.LBL
; 1Q-52.LBL
; 1T-52.LBL
; 42-52.LBL
; 8J-52.LBL
; 8P-52.LBL
; 1K0-959-702-MAX1.LBL
; 1K0-959-702-MAX2.LBL
; 1K0-959-702-MAX3.LBL
; 1K0-959-702-MIN1.LBL
; 1K0-959-702-MIN2.LBL
; 1K0-959-702-MIN3.LBL
;
; created on 21/Jul/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 13/Apr/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Window Regulator
001,1,WR-Button (E107),Passenger Door,Display Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
001,2,WR-Button (E81),Driver Door,Display Range: Auto Open/Auto Close/Manual Open/Manual Close/Not Oper.
001,3,Window Regulator,(V148),Specification: Ends Learned\nDisplay Range: Up/Down/Ends Learned/At Top/At Bottom/Pinch Protect/Over-Temp S/O
001,4,Thermal Protection,,Display Range: Active/Not Active
;
002,0,Window Regulator && General
002,1,Window Regulator,Comfort Control,Display Range: Open/Closed/Not Oper.
002,2,Window Regulator,Enabling,Display Range: Yes/No
002,3,Dimming,(Terminal 58d),Display Range: 0.0...100.0 %
002,4,Vehicle Speed
;
003,0,General
003,1,Voltage,(Terminal 30),Specification: 9.0...14.0 V
003,2,Databus,Condition,Specification: 2-Wire\nDisplay Range: 1-Wire/2-Wire
003,3,Ignition,(Terminal 15),Display Range: Terminal 15 On/Terminal 15 Off
003,4,S-Contact,,Display Range: Activated
;
004,0,General
004,1,Window Regulator,Position (V148),Display Range: 0.0...100.0 %
004,2,Internal,Illumination,Display Range: Enabled/Disabled
004,3,Interior Door,Handle Illumination,Display Range: 0.0...100.0 %/Not Installed
004,4,Ambient,Illumination,Display Range: 0.0...100.0 %/Not Installed
;
005,0,Central Locking
005,1,Locking Unit (F221),Passenger Door,Display Range: Locked/Unlocked/Safe
005,2,Contact Switch (F3),Passenger Door,Display Range: Door Open/Door Closed
005,3,Interior Locking,Button (E309),Display Range: Lock/Unlock/Not Oper./Not Installed
005,4,Key Switch,Passenger Door,Display Range: Open/Closed/Not Oper./Not Installed
;
006,0,Mirror I (Heating)
006,1,Mirror Selector,Switch (E48),Display Range: Left/Right/ON (Mirror Heater Switch)/OFF (Mirror Heater Switch)/Not Oper.
006,2,Mirror Heater,(Z5),Display Range: Active/Not Active/Not Installed
;
007,0,Mirror II (Adjustment)
007,1,Mirror Adjustment,Switch (E43),Range: Pos X+/Pos X-/Pos Y+/Pos Y-/Not Oper./Not Installed
;
008,1,Mirror Blinker,Passenger (L132),Range: Active/Not Active/Not Installed
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Door Electronics Passenger (J387) Coding
C01,+0000002 = Ambient Mirror Illumination installed
C02,+0000004 = Mirror Turn Signals installed
C03,+0000008 = Interior Door Handle Illumination installed
C04,+0000016 = Automatic Run active
C05,+0000032 = Mirror Heater installed
C06,+0000064 = Door Exit/Warning Light installed
C07,+0000128 = 5-Door Chassis
C08,+0000256 = Seat Memory installed
C09,+0000512 = Right Hand Steering
C10,+0001024 = Safe-Motor not installed
C11,+0002048 = Pinch Protection inactive
C12,+0004096 = Folding Mirrors installed (MY 2008+)
C13,+0008192 = Manually Operated Convertible Top installed
C14,+0131072 = Start/Stop Function installed (MY 2010+)
;
