;
; VAG-COM Label File
;
; Audi A2 (8Z) / Audi A4 (8E2/8E5) / Audi A6 (4B)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 8Z0-919-283-??
;
; includes measuring blocks, adaptation and coding
;
; created on 09/Apr/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 09/Apr/2006
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Distance (Rear)
001,1,Rear Left,Sensor (G203),Specification: 10...60 cm (255 cm = no obstacle recognized)
001,2,Rear Left Center,Sensor (G204),Specification: 10...160 cm (255 cm = no obstacle recognized)
001,3,Rear Right Center,Sensor (G205),Specification: 10...160 cm (255 cm = no obstacle recognized)
001,4,Rear Right,Sensor (G206),Specification: 10...60 cm (255 cm = no obstacle recognized)
;
002,0,Resulting Distance / Vehicle Speed && Voltage
002,1,Resulting,Distance Front,Specification: 0...120 cm (255 cm = no obstacle recognized)
003,2,Vehicle Speed,,Range: 0.0...255.0 km/h
002,3,Buzzer,,Range: Sound ON/Sound OFF
;
003,0,External Information
003,1,Voltage Supply
003,2,Reverese Gear,engaged,Range: Reverse: Yes/Reverse: No
003,3,Trailer hitched,,Range: Trailer: Yes/Trailer: No
;
004,0,Oscillation Time
004,1,Rear Left,Sensor (G203),Specification: max. 4.00 ms
004,2,Rear Left Center,Sensor (G204),Specification: max. 4.00 ms
004,3,Rear Right Center,Sensor (G205),Specification: max. 4.00 ms
004,4,Rear Right,Sensor (G206),Specification: max. 4.00 ms
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Communication (Comfort)
125,1,Instrument Cluster,(J285)
125,2,Steering Wheel,Electronics (J527)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,?xxxx: Trailer Hitch (0 = No / 1 = Yes)
C02,x?xxx: Transmission
C03,0 = Manual Transmission
C04,1 = Automatic Transmission
C05,xx?xx: Confirmation Sound (0 = No / 1 = Yes)
C06,xxx?x: Chassis
C07,0 = Limousine (Sedan) Rest of World
C08,1 = Avant (Wagon) Rest of World
C09,2 = Limousine (Sedan) North America
C10,3 = Avant (Wagon) North America
C11,4 = S-Variant Limousine (Sedan) Rest of World
C12,5 = S-Variant Avant (Wagon) Rest of World
C13,6 = S-Variant Limousine (Sedan) North America
C14,7 = S-Variant Avant (Wagon) North America
C15,8 = allroad
C16,xxxx?: Model
C17,2 = Audi A2 (8Z)
C18,4 - Audi A4 (8E)
C19,5 = Audi A4 Cabrio (8H)
C20,6 = Audi A6 (4B)

;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A01,0,Rear Buzzer Volume
A01,5,Rear Buzzer Volume
A01,6,Adaptation of the rear warning buzzer volume.
A01,7, 
A01,8,Display Range: 2...6
;
A02,0,Rear Buzzer Frequency
A02,5,Rear Buzzer Frequency
A02,6,Adaptation of the rear warning buzzer frequency.
A02,7, 
A02,8,Display Range: 0...4
;
