;
; VCDS Label File
;
; Copyright © 2011 Ross-Tech, LLC
;
; Audi A3 (8L) / VW Bora/Golf/Jetta (1J/9M)
;
: Component: J248 - Engine Electronics (# 01) - AGR / ALH (121 pin module)
;
; P/N: 038-906-012-???
;
; Includes Measuring Blocks, Basic Settings, Coding, Login and Adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 03-01.LBL
; 038-906-012-AGR.LBL  (1.9l TDI @  90 HP - AGR/ALH - from 05/1999)
;
; erstellt am 29.04.2005 von Sebastian Stange (Sebastian@Ross-Tech.com)
; letzte Änderung am 15.01.2009
;
: English content revisions:
; contributed by Mike Sauve www.alientech.net
; modified for Jetta, Golf 1999-2000 by Steve Tomasic www.steve_tomasic@hotmail.com
; Modified by Ross-Tech Feb 2004 to demonstrate Labels for Adaptation 
: Modified by Dana Smetanick 4/26/2011
;
; Requires VCDS 10.6.4 or newer
;
;
;
;---------------------------------------------------
;
; Measuring Blocks & Basic Settings
;
;---------------------------------------------------
;
;
000,0,Basic Functions - Switch to Basic Settings for Start of Injection
000,1,Engine speed (G28)  - Specification (Idle): 41...46 (861...950 RPM) | (Full Load): 138...148 (2900...3100 RPM)
000,2,Start of Injection - Specification (Idle): 12...75 (2 °ATDC ... 4 °BTDC) | (Full Load): 137...215 (8...14 °BTDC)
000,3,Throttle Position - Specification (Idle): 0 (0 %) | (Full Load): 255 (100 %)
000,4,Injected Quantity - Specification (Idle): 11...45 (2.2...9 mg/stroke) | (Full Load): 199...214 (39.8...42.8 mg/stroke)
000,5,Manifold pressure - Specification (Idle): 83...106 (920...1140 mbar) | (Full Load): 179...215 (1850...2250 mbar)
000,6,Atmospheric Pressure  (BARO metric) - Specification (Full Load) 183...224 (910...1110 mbar)
000,7,Coolant Temp. (G62) - Specification: 80...35 (80...110 °C)
000,8,Intake Manifold Temp. (G42). - Specification: 182...50 (10...100 °C)
000,9,Fuel Temp. (G81) - Specification: 91...201 (20...80°C)
000,10,Air Mass (EGR On - 2 Min. after start-up) - Specification (Idle): 69...111 (230...370 mg/H)
;
B000,0,Testing Dynamic Start of Injection
;
001,0,Injection Quantity
001,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
001,2,Injection Quantity,,Specification : 2.2...9.0 mg/H
001,3,Mod. Piston,Disp. (G149),Specification: 1.45...2.0 V
001,4,Coolant,Temperature (G62),Range: -40.5...+135.0 °C\nSpecification (Warm): 80.0...110.0 °C
;
002,0,Idle speed
002,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
002,2,Accel. Pedal Pos.,Sensor 1 (G79),Range: 0.0...100.0 %\nSpecification (Idle): 0.0 %\nSpecification (Full Load): 100.0 %
002,3,Operating,condition,Specification: \n1xx = A/C Switched On (Increased idle speed)\nx1x = Idle / Closed Throttle switch closed\nxx1 = A/C Compressor On
;
; 1xx = A/C Switched On (Increased idle speed)
; x1x = Idle / Closed Throttle switch closed
; xx1 = A/C Compressor On
;
002,4,Coolant,Temperature (G62),Range: -40.5...+135.0 °C\nSpecification (Warm): 80.0...110.0 °C
;
003,0,Exhaust Gas Recirculation (EGR) - Switch to Basic Settings for EGR test
003,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
003,2,Air Mass,Specified,Specification (Idle): 230...370 mg/H
003,3,Air Mass,Actual,Specification (Idle): 230...370 mg/H
003,4,EGR Solenoid,(N18),Specification: 40...75 % Duty cycle
;
B003,0,Exhaust Gas Recirculation (EGR) System Test at Idle
B003,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM
B003,2,Air Mass,Specified,Specification (Idle): 230...370 mg/H
B003,3,Air Mass,Actual,Specification (Idle): 230...370 mg/H
B003,4,EGR Solenoid,(N18),Specification: 40...75 % Duty cycle
;
004,0,Start of injection
004,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
004,2,Start of injection, Specified,Specification (Idle): 12...75 (2 °ATDC ... 4 °BTDC)\n(Full Load): 137...215 (8...14 °BTDC)
004,3,Start of injection, Actual,Specification (Idle): 12...75 (2 °ATDC ... 4 °BTDC)\n(Full Load): 137...215 (8...14 °BTDC)
004,4,Cold Start Injector,Duty cycle, Specification (Idle): 3...80 %\n(Full Load): 50...95 %
;
005,0,Starting Conditions
005,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
005,2,Start Injection,Quantity
005,3,Start Injection, Actual
005,4,Coolant,Temperature (G62),Range: -40.5...+135.0 °C\nSpecification (Warm): 80.0...110.0 °C
;
006,0,Cruise Control System (CCS) Switch positions
006,1,Vehicle Speed
006,2,Brake Pedal,Monitoring,Specification:\n1xx = Clutch Pedal Switch (F36) Open\nx1x = Brake Pedal Switch (F47) Open\nxx1 = Brake Light Switch (F) Closed
;
; 1xx = Clutch Pedal Switch (F36) Open
; x1x = Brake Pedal Switch (F47) Open
; xx1 = Brake Light Switch (F) Closed
;
006,3,Cruise Control, System (CCS),Specification:\nxxxxx1 = CCS Enabled / Switched On \nxxxx1x = CCS On and Memory Inactive \nxxx1xx = Acceleration \nxx1xxx = Resume \nx1xxxx = Brake Pedal Operated \n1xxxxx = Clutch Pedal Operated
;
; xxxxx1 = CCS Enabled / Switched On
; xxxx1x = CCS On and Memory Inactive
; xxx1xx = Acceleration
; xx1xxx = Resume
; x1xxxx = Brake Pedal Operated
; 1xxxxx = Clutch Pedal Operated
;
006,4,Cruise Control, System (CCS),Specification:\n0 = Vehicles With CCS - System Switched Off \n1 = Vehicles With CCS - System Switched On \n255 = Vehicles Without CCS \n \nNote: W/ Auto. Trans. it may be necessary \nto test drive exceeding the speed of \n30 km/h (19 mph) before voltage is supplied \nto the CCS switch.
;
; 0 = Vehicles With CCS - System Switched Off
; 1 = Vehicles With CCS - System Switched On
; 255 = Vehicles Without CCS
; Note: W/ Auto. Trans. it may be necessary to test drive exceeding the speed of 30 km/h (19 mph) before voltage is supplied to the CCS switch.
;
007,0,Temperatures
007,1,Fuel Temp. (G81),,Note: -5.4°C = Short Ckt. or G81 Inoperative \nBaseline with Ambient / Intake / ECT Temp. readings
;
; Note: -5.4°C = Short Ckt. or G81 Inoperative. Baseline with Ambient / Intake / ECT Temp. readings
;
007,2,N/A
007,3,Intake Air Temp., (G72),Note: 136.8°C = G72 Inoperative \nBaseline with Ambient / Fuel / ECT Temp. readings
;
; Note: 136.8°C = G72 Inoperative. Baseline with Ambient / Fuel / ECT Temp. readings
;
007,4,Coolant,Temperature (G62),Range: -40.5...+135.0 °C \nNote: 135.0 °C = Short Ckt or G62 Inoperative \nBaseline with Ambient / Intake / Fuel Temp. readings
;
; Note: 135.0 °C = Short Ckt or G62 Inoperative. Baseline with Ambient / Intake / Fuel Temp. readings
;
008,0,Injected Quantity (IQ) Limitation I (at WOT)
008,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
008,2,Torque Request,(Driver),Specification: (Full Load) 38.0...42.0 mg/H
008,3,Torque Limitation, via Speed / RPM, Specification: (Full Load) 35.5...36.5 mg/H
008,4,Smoke Limitation,,Specification (Full Load) 36.0...39.0 mg/H
;
009,0,Injected Quantity (IQ) Limitation II
009,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
009,2,Torque Request,(Cruise Control)
009,3,Transmission,Limitiation, Signal via Auto. Trans. during shift
009,4,N/A
;
010,0,Air System && Charge Pressure Control
010,1,Mass Air Flow,(Actual),Specification: (Idle): 230-370 mg/H \n (Full Load): 800...1100 mg/H
010,2,Air Pressure,(F96) BARO,Specification: 900...1100 mbar
010,3,Manifold Pressure,(Actual) MAP (G71),Specification (Full Load): 1700...2080 mbar
010,4,Accel. Pedal Pos.,Sensor 1 (G79),Range: 0.0...100.0 %\nSpecification (Idle): 0.0 %\nSpecification (Full Load): 100.0 %
;
011,0,Charge Pressure Control
011,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM\n(Full Load): 2900...3100 RPM
011,2,Boost,Specified, Specification (Full Load): 1850...1950 mbar
011,3,Boost,Actual,Specification (Full Load): 1850...2080 mbar
011,4,Charge Pressure,(N75) Solenoid,Specification: 45...95%
;
B011,0,Charge Pressure Control at Idle in Basic Setting
B011,1,Engine Speed,(G28),Specification: (Idle): 870...950 RPM
B011,2,Boost,Specified,Charge Pressure Control is \nalternately switched On and Off
B011,3,Boost,Actual,Charge Pressure Control is \nalternately switched On and Off
B011,4,Charge Pressure,(N75) Solenoid
;
012,0,Glow Plugs
012,1,N/A
012,2,Glow Period, Preheat
012,3,Supply,Voltage ECM
012,4,Coolant,Temperature (G62),Range: -40.5...+135.0 °C\nSpecification (Warm): 80.0...110.0 °C
;
013,0,I.Q. Idle Stabilization (Injection Quantity Deviation)
013,1,IQ Cylinder 1,,Specification: -2.0...+2.0 mg/H
013,2,IQ Cylinder 2,,Specification: -2.0...+2.0 mg/H
013,3,IQ Cylinder 3,,Specification: -2.0...+2.0 mg/H
013,4,IQ Cylinder 4,,Specification: -2.0...+2.0 mg/H
;
015,0,Fuel consumption
015,1,Engine speed
015,2,Injected Quantity, Actual
015,3,Fuel,Consumption
015,4,Injected Quantity, Driver Request
;
016,0,Auxiliary Heating
016,1,Generator Load
016,2,Auxiliary Heating,Shut-Off Conditions,Specification: \n1xxxxxxx = N/A \nx1xxxxxx = N/A \nxx1xxxxx = ECT (G62)/ IAT (G72) Faulty \nxxx1xxxx = Engine Start within 10 seconds \nxxxx1xxx = Engine Speed below 870/RPM \nxxxxx1xx - Battery voltage below 9 V \nxxxxxx1x = Generator (GEN) Inoperative \nxxxxxxx1 = ECT (G62) Exceeds 70...80 °C \nxxxxxxx1 = IAT (G72) Exceeds 5 °C
;
; 1xxxxxxx = N/A
; x1xxxxxx = N/A
; xx1xxxxx = ECT (G62)/ IAT (G72) Faulty
; xxx1xxxx = Engine Start within 10 seconds
; xxxx1xxx = Engine Speed below 870/RPM
; xxxxx1xx - Battery voltage below 9 V
; xxxxxx1x = Generator (GEN) Inoperative
; xxxxxxx1 = ECT (G62) Exceeds 70...80 °C
; xxxxxxx1 = IAT (G72) Exceeds 5 °C
;
016,3,Heating Element,Activation,Specification: \n1x - Relay for High Heat output (J360) on \nx1 - Relay for Low Heat output (J359) on
;
; 1x - Relay for High Heat output (J360) on
; x1 - Relay for Low Heat output (J359) on
;
016,4,Supply,Voltage ECM
;
017,0,Readiness Code
017,1,N/A
017,2,Specification:,x000xxxx
017,3,N/A
017,4,Specification:,0xxxxxxx
;
019,0,Quantity Adjuster
019,1,Mod. Piston (G149),Disp. Sensor,Specification: (Stop position Stop) 0.500...0.970 V
019,2,Mod. Piston (G149),Disp. Sensor,Specification: (Start position Stop) 4.150...4.740 V
019,3,N/A
019,4,N/A
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission,,Range: Transm. 1/Transm. 0
125,2,Brake Electronics,,(J104),Range: ABS 1/ABS 0\nSpecification: ABS 1
125,3,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
;
;
;---------------------------------------------------
;
; Adaptation
;
;---------------------------------------------------
;
;
A001,0,Injected Quantity (IQ)
A001,1,Engine Speed,(G28)
A001,2,IQ,, 3-5 mg/H
A001,3,Mod. Piston
A001,4,Coolant Temp
A001,5,Injected Quantity Increase to solve slowdown
A001,6,shudder problems. Check the injected quantity at idle with
A001,7,engine warm and all power consuming devices turned off.
A001,8,Note the original values prior to modification.
A001,9,
A001,10,Login - 11 with 12233 may be required first.
;
A002,0,Idle speed
A002,1,Engine Speed,,870...950 RPM
A002,2,Throttle Position
A002,3,Operating,Condition
A002,4,Coolant,Temperature
A002,5,Increase or decrease this to change idle speed
A002,6,Note the original values prior to modification.
;
A003,0,Exhaust Gas Recirculation (EGR)
A003,1,Engine Speed,, 870...950 RPM
A003,2,MAF (Specified),,230-370 mg/H
A003,3,MAF (Actual),,230-370 mg/H
A003,4,EGR Solenoid (N18),,40-75% Duty Cycle
A003,5,Exhaust Gas Recirculation (EGR) Modification
A003,6,Note the original values prior to modification.
A003,7,To reduce EGR to a minimum (for off-road use only!)
A003,8,increase the value. Typically 33768 is Max.
A003,9,
A003,10,To restore EGR to stock, set this channel to 32768
A003,11,Login - 11 with 12233 may be required first.
;
A004,0,Start of Injection - Modification is Strongly Discouraged
A004,1,Engine Speed,,870...950 RPM
A004,2,Specified Start,,2 °ATDC ... 4 °BTDC
A004,3,Actual Start,,2 °ATDC ... 3 °BTDC
A004,4,Cold Start Valve,, 3-80%
A004,5,Modification of this Channel is Strongly Discouraged!
A004,6,Note the original values prior to modification.
A004,7,Login - 11 with 12233 may be required first.
;
A005,0,Starting Conditions
A005,1,Engine Speed,,870...950 RPM
A005,2,Start Injection,Quantity
A005,3,Actual Start,Quantity
A005,4,Coolant,Temperature
A005,5,Starting Conditions
A005,6,This channel alters the Injected Quantity (IQ) allowed
A005,7,when starting. Temporary fix for poorly starting engine.
A005,8,Note the original values prior to modification.
A005,9,Login - 11 with 12233 may be required first.
;
;
;---------------------------------------------------
;
; Coding
;
;---------------------------------------------------
;
;
C00,Engine Electronics (J248) Coding
C01,00001 = Automatic Transmission
C02,00002 = Manual Transmission (FWD) Front Wheel Drive
C03,00003 = Manual Transmission (AWD) All-Wheel Drive
;
;
;---------------------------------------------------
;
; Login
;
;---------------------------------------------------
;
;
L00,Engine electronics (J248) Login
L01,11463 = Activate Cruise Control System(CCS)
L02,16167 = Deactivation Cruise Control System(CCS)
L03,12233 = Adaptation Enabling
;

