;
; VCDS Label File
;
; Copyright © 2004-2009 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J104 - Brake Electronics (#03)
;
; P/N: 4E0-910-517-???
;
; includes measuring blocks, login and coding
;
; created on 23/Sep/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modificationon on 06/Mar/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right,Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0.0...255.0 km/h
;
B001,0,Steering Angel Sensor (G85) Alignment
B001,1,Steering Angel,Sensor (G85), 
B001,2,Alignment, , 
B001,3,Alignment,Status,Specification: OK
B001,4, , , 
;
002,1,Brake test,switch
002,2,Brake light,switch
002,3,Parking,brake
002,4,ESP-button,(center console)
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,Sensor (G85),Display Range: -720.0...+720.0 °\nTolerance (when straight): ±5.0 °
005,2,Rotation Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
005,4,Transverse,Acceleration,Display Range: -25.0...+25.0 m/s²
;
006,1,Supply Voltage,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON = OK / OFF = not OK
006,3,Return Flow Pump,,Display Range: ON/OFF
006,4,Work Shop Code
;
007,0,Installation position - see labelfile (test applies only to room temperature)
; not OK => check brake temperature (test applies only to room temperature)
;        => Check installation of sensor (fully inserted, firmly screwed in)
;        => Check wheel bearing
;        => Check tolerance of axle
007,1,Front,Left,Display range: invalid/OK/not OK
007,2,Front,Right,Display range: invalid/OK/not OK
007,3,Rear,Left,Display range: invalid/OK/not OK
007,4,Rear,Right,Display range: invalid/OK/not OK
;
008,0,Direction of rotation
008,1,Front,Left,Display range: invalid/forward/reverse
008,2,Front,Right,Display range: invalid/forward/reverse
008,3,Rear,Left,Display range: invalid/forward/reverse
008,4,Rear,Right,Display range: invalid/forward/reverse
;
009,1,Brake test,switch 
009,2,Brake light,switch
009,3,Brake,pressure
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 0/Steer. ang. 1
125,2,Transmission,,Display Range: Transm. 1/Transm. 0
125,3,Engine,,Specification: Engine 1\nDisplay Range: Engine 0/Engine 1
125,4,Instrument Cluster,,Specification: Instruments 1\nDisplay Range: Instruments 0/Instruments 1
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Adaptive Cruise,Control (ACC)
126,2,CAN-Gateway
126,3,Electric Parking,Brake (EPB)
126,4,Level Control,System
;
;
;---------------------------------------------------
;
; login/coding-ii
;
;---------------------------------------------------
;
;
L00,Brake Electronics (J104/Bosch 5.7) Coding-II
L01,0?xxx: Chassis
L02,3 = Audi S8 (Short Wheel Base)
L03,5 = Audi A8 (Short Wheel Base)
L04,6 = Audi A8 (Long Wheel Base)
L05,0x?xx: Brakes
L06,1 = 2FNR 42 AL 18" (PR-1LJ)
L07,2 = 2FNR 42 AL 17" (PR-1LL)
L08,4 = FNRG-60 16" (PR-1LG)
L09,7 = Brembo M6 AL 19" (PR-1LW)
L10,0xx?x: Engine
L11,2 = 10 Cyl. Gasoline
L12,3 = 12 Cyl. Gasoline OR 6/8 Cyl. Gasoline/Diesel with Brembo M6 AL 19" (PR-1LW)
L13,5 = 6/8 Cyl. Diesel w/o Brembo M6 AL 19" (PR-1LW)
L14,6 = 6 Cyl. Diesel (Long Wheel Base)
L15,9 = 6/8 Cyl. Gasoline w/o Brembo M6 AL 19" (PR-1LW)
L16,0xxx?: Transmission
L17,7 = Automatic (09E/09L)
L18,9 = Multitronic (01J)
L19, 
L20,Note: After Login/Coding-II has been carried out you need to recode the Control Module.
L21, 
L22,40168 = Basic Settings Enabling (i.e. mandatory prior to Steering Angle Sensor Alignment)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104/Bosch 5.7) Coding
C01,000?xxx: Chassis
C02,1 = Audi S8 (Short Wheel Base)
C03,7 = Audi A8 (Long Wheel Base)
C04,8 = Audi A8 (Short Wheel Base)
C05,000x?xx: Brakes
C06,3 = FNRG-60 16" (PR-1LG)
C07,5 = 2FNR 42 AL 17" (PR-1LL)
C08,6 = 2FNR 42 AL 18" (PR-1LJ)
C09,7 = Brembo M6 AL 19" (PR-1LW)
C10,000xx?x: Engine
C11,2 = 10 Cyl. Gasoline
C12,3 = 12 Cyl. Gasoline OR 6/8 Cyl. Gasoline/Diesel with Brembo M6 AL 19" (PR-1LW)
C13,5 = 6/8 Cyl. Diesel w/o Brembo M6 AL 19" (PR-1LW)
C14,6 = 6 Cyl. Diesel (Long Wheel Base)
C15,9 = 6/8 Cyl. Gasoline w/o Brembo M6 AL 19" (PR-1LW)
C16,000xxx?: Transmission
C17,7 = Automatic (09E/09L)
C18,9 = Multitronic (01J)
C19, 
C20,Note #1: Coding is accepted after a specific Login has been carried out.
C21,Note #2: After successful Coding the Steering Angle Sensor Alignment needs to be carried out.
;
