;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; VW Passat (3B)
;
; Component: J217 - Transmission (#02) - 5-Speed Automatic Transmission 01V
;
; P/N: 01V-927-733-???
;
; includes measuring blocks, coding and adaptation
;
; created on 16/Mar/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 20/Aug/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Engine Speed
001,2,Transmission,Input Speed (G182)
001,3,Transmission,Output Speed (G195)
001,4,Current Gear,,Range: 1m/1/2/3/4/5/R
;
002,0,General
002,1,Current Program,,Range: S0/DS/WL/TT/AS/GR
; DS = Dynamisches Shift Program active
; WL = Warm-Up Program active
; TT = TipTronic Recognition active
; AS = Anti-Slip-Regulatiopn (ASR) active
002,2,Accel. Pedal,Position,Range (Idle): 0.0...1.0 %\nRange (Load): 99.0...100.0 %
002,3,Transmission,Output Speed (G195)
002,4,Current Gear,,Range: 1m/1/2/3/4/5/R
;
003,0,General
003,1,Brake Light,Switch (F)
003,2,Shift Lock,Solenoid (N110),Range: PN active/PN not active
003,3,Vehicle Speed
003,4,Supply Voltage,(Terminal 15),Specification: 10.0...16.0 V
;
004,0,General
004,1,Transmission Fluid,Temperature (G93),-50.0 °C = Short to Ground\n-180.0 °C = Open/Short to Plus
004,2,Selector Lever,Position (F125),Range: P/R/N/D/S/Z1/Z2/Z3
004,3,Multi-Function,Switch (F125),P = 1000\nR = 0100\nN = 1110\nD = 1011\nS = 0111\nZ3 = 1111\nZ2 = 1010\nZ1 = 1100
004,4,On-Board-Diag.,(OBD) Information,Range 0 = No / 1 = Yes\n\n?xxx = Malfunction Display active\nx?xx = Trip complete\nxx?x = Transmission Wam-Up complete\nxxx? = Engine Start recognized
;
005,0,Solenoid Valves
005,1,Solenoid Valve 1,(N88),O = not active\nX = active (D = Gear 3/4)
005,2,Solenoid Valve 2,(N89),O = not active / X = active
005,3,Solenoid Valve 3,(N90),O = not active / X = active
005,4,Current Gear,,Range: 1m/1/2/3/4/5/R
;
006,0,Pressure Control Valves (Specified Current)
006,1,Pressure Control,Valve 1 (N215),Range: 0.000...2.000 A
006,2,Pressure Control,Valve 2 (N216),Range: 0.000...2.000 A
006,3,Pressure Control,Valve 3 (N217),Range: 0.000...2.000 A
;
007,0,Pressure Control Valve (Specified Current) && Torque Converter
007,1,Transmission Fluid,Temperature (G93),-50.0 °C = Short to Ground\n-180.0 °C = Open/Short to Plus
007,2,Pressure Control,Valve 4 (N218),Range: 0.000...2.000 A
007,3,Torque Converter,Clutch,Range: TC Open/TC Control/TC Closed
007,4,Torque Converter,Slip Speed,Specification (at "TC Open"): 0 RPM\nSpecification (at "TC Control"): 20...120 RPM\nSpecification (at "TC Closed"): 0...20 RPM
;
008,0,
008,1,Kick-Down,Switch (F8),Range: Operated/Not Oper.
008,2,Accel. Pedal,Position,Range (Idle): 0.0...1.0 %\nRange (Load): 99.0...100.0 %
008,3,Deceleration,Signal,Range: No Display/Deceleration
;
009,0,
009,1,Engine Torque
009,2,Engine Speed
009,3,Accel. Pedal,Position,Range (Idle): 0.0...1.0 %\nRange (Load): 99.0...100.0 %
009,4,Transmission,Input Torque
;
010,0,
010,1,Torque Increase in,Torque Converter
010,2,Engine Speed
010,3,Current Gear,,Range: 1m/1/2/3/4/5/R
010,4,Vehicle,Acceleration
;
011,0,
011,1,Selector Lever,Position (F125),Range: P/R/N/D/S/Z1/Z2/Z3
011,2,Tiptronic Switch,(F189) Gate Status,Range: No Display/M-Shift
011,3,Tiptronic Switch,(F189) Status,Range: No Display/Up-Shift/Down-Shift
;
012,0,
012,1,Surface,Recognition,E = Flat Surface\nB = Hill
012,2,Dynamic Index
012,3,Driving Resistance,Index
012,4,Driving,Evaluation
;
013,0,
013,1,Standard Torque,via CAN
013,2,Engine Code Digit,via CAN
013,3,Transmission Coding,in Engine
013,4,CAN-Data Version
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
084,0,Advanced Control Module Identification V
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Range: Engine 1/Engine 0\nSpecification: Engine 1
125,2,Brake Electronics,(J104),Range: ABS 1/ABS 0\nSpecification: ABS 1
125,3,Steering Wheel,Electronics (J527),Range: St. Wheel 1/St. Wheel 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Transmission (J217) Coding
C01,Non-DBW (Drive-by-Wire) Cars:
C02,00000 = Standard (DSP active)
C03,00010 = Standard (DSP inactive)
C04, 
C05,DBW (Drive-by-Wire) Cars:
C06,0?xxx: Tiptronic Installation
C07,0 = Tiptronic Buttons/Paddels not installed
C08,1 = Tiptronic Buttons/Paddels installed
C09,0x?xx: Tiptronic Strategy
C10,0 = Old Strategy (Shifts to first Gear when braked to Standstill)
C11,1 = New Strategy (Automatic Up/Down Shift before RPM Limit & Down Shift at Kick-Down)
C12,0xx?x: Dynamic Shift Program (DSP)
C13,0 = Dynamic Shift Program (DSP) active
C14,1 = Dynamic Shift Program (DSP) inactive
C15,0xxx?: Region/Powertrain
C16,1 = All-Wheel-Drive (Rest of World)
C17,2 = All-Wheel-Drive (North American Region)
C18,3 = Front-Wheel-Drive (Rest of World)
C19,4 = Front-Wheel-Drive (North American Region)
;
