;
; VAG-COM Label File
;
; Audi A4 (8E)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 8E0-953-549-???
;
; includes measuring blocks, coding and adaptation
;
; created on 26/Sep/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 03/Jun/2006
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Ignition,switch,Display range: 12345 (1=P-contact/2=S-contact/3=term. 75/4=term. 15/5=term. 50)
001,2,Signal light,,Display range: not activated/left/right
001,3,Light horn,,Display range: not activated/activated
001,4,High beam,,Display range: not activated/activated
;
002,1,Horn,,Display range: not activated/activated
002,2,Wiping front,,Display range: not activated/interval step 1/step 1/step 2
002,3,Interval,steps,Display range: step 1/step 2/step 3/step 4
002,4,Washing,front,Display range: not activated/activated
;
003,1,Wiping rear,,Display range: not installed/not activated/activated
003,2,Washing rear,,Display range: not installed/not activated/activated
003,3,Board computer,,Display range: not installed/button reset/button on/button down
003,4,[N/A]
;
004,0,Cruise control switch
004,1,Cruise control,,Display range: on/off
004,2,Cruise control,-SET-,Display range: not activated/activated
004,3,Cruise control,,Display range: not activated/accelerating/decelerating/stored Off/Resume
004,4,[N/A]
;
005,0,Steering wheel (M-equipment)
005,1,Tip down,,Display range: not installed/not activated/activated
005,2,Tip up,,Display range: not installed/not activated/activated
005,3,Steering wheel,heater,Display range: not installed/on/off
005,4,Sensor,[°C],127 = open circuit / 248 = not installed
;
006,0,Multi-function steering wheel
006,1,Communication,,Display range: OK/not OK
006,2,Electronic,version
006,3,Malfunction,recognized?,Display range: yes/no
006,4,[N/A]
;
007,0,Multi-function buttons
007,1,Button 1,,Display range: not activated/activated
007,2,Button 2,,Display range: not activated/activated
007,3,Button 3,,Display range: not activated/activated
007,4,Button 4,,Display range: not activated/activated
;
008,0,Multi-function buttons
008,1,Button 5,,Display range: not activated/activated
008,2,Button 6,,Display range: not activated/activated
008,3,[N/A]
008,4,[N/A]
;
009,0,Inputs via Comfort CAN-bus
009,1,Diming,,Display range: diming value
009,2,Right hand,steering,Display range: yes/no
009,3,Left,heated seat,Display range: off/step
009,4,Right,heated seat,Display range: off/step
;
010,0,Inputs via Comfort CAN-bus
010,1,M-path,Tiptronic,Display range: not activated/activated
010,2,[N/A]
010,3,[N/A]
010,4,[N/A]
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
125,0,CAN-Databus communication (Comfort)
125,1,Instrument,cluster
125,2,Central comfort,electric
125,3,Climate control
125,4,[N/A]
;
126,0,CAN-Databus communication (Comfort) - Door control modules
126,1,driver,side
126,2,passenger,side
126,3,rear,left,only with electrical power windows
126,4,rear,right,only with electrical power windows
;
127,0,CAN-Databus communication (Comfort)
127,1,Radio
127,2,Telephone
127,3,Voice activation,input
127,4,[N/A]
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,0?xxx: Steering Wheel
C02,0 = Standard (without Multifunction)
C03,1 = 3-Spoke Steering Wheel (Sport Steering Wheel)
C04,2 = Multifunction Steering Wheel with Radio Control
C05,3 = Multifunction Steering Wheel with Radio/Telephone Control
C06,4 = Multifunction Steering Wheel with Radio/Telephone/Voice Control
C07,5 = Multifunction Steering Wheel with Radio/Voice Control
C08,0x?xx: Options
C09,+1 = Tiptronic
C10,0xx?x: Board Computer & Cruise Control
C11,0 = Board Computer & Cruise Control not installed
C12,1 = Board Computer installed
C13,2 = Cruise Control installed
C14,4 = Board Computer & Cruise Control installed
C15,0xxx?: Rear Wiper (Chassis)
C16,1 = Rear Wiper not installed (Sedan/Cabriolet)
C17,2 = Rear Wiper installed (Avant)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A081,0,Learned Values (Vehicle Data)
A081,5,Learned Values (Vehicle Data)
A081,6,To start the process for vehicle data (VIN)
A081,7,learning enter/save 00111 as new value.
;
