;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Audi A4 (8D) / Audi A6 (4B) / VW Passat (3B)
;
; Component: J104 - Brake Electronics (#03) - Bosch 5.3 ABS/EDL/ASR/ESP
;
; P/N: 8D0-907-389-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4D-03.LBL
; 4Z-03.LBL
; 8D0-907-389.LBL (Bosch 5.3 ABS/EDL/ASR/ESP)
;
; includes measuring blocks, basic setting, coding and login
;
; created on 21/Jan/2006 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modificationon on 17/Jul/2012
;
; requires VCDS 11.2.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right,Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0.0...255.0 km/h
;
B001,0,Steering Angle Sensor (G85) Alignment
B001,1,Steering Angle,Sensor (G85), 
B001,2,Alignment, , 
B001,3,Alignment,Status,Specification: OK
B001,4, , , 
;
002,0,Switches && Buttons
002,1,Brake Test Switch,,Display Range: 0/operated
002,2,Brake Light Switch,,Display Range: 0/operated
002,3,Parking Brake,Button,Display Range: 0/operated
002,4,ESP-Passive,Button,Display Range: 0/operated
;
B002,0,Brake System Bleeding
B002,1,Status, , 
B002,2, , , 
B002,3, , , 
B002,4, , , 
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
B003,0,Activate ESP System/Function Test
B003,1,Status, , 
B003,2, , , 
B003,3, , , 
B003,4, , , 
;
004,1,Standing Time
004,2,EDL-T Flag,,Display Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,Sensor (G85),Display Range: -720.0...+720.0 °\nTolerance (when straight): ±5.0 °
005,2,Rotation Rate,,Display Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
005,4,Transverse,Acceleration,Display Range: -25.0...+25.0 m/s²
;
006,1,Supply Voltage,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON = OK / OFF = not OK
006,3,Return Flow Pump,,Display Range: ON/OFF
006,4,Work Shop Code
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 0/Steer. ang. 1
125,2,Transmission,,Display Range: Transm. 1/Transm. 0
125,3,Engine,,Specification: Engine 1\nDisplay Range: Engine 0/Engine 1
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Brake Electronics - Bosch 5.3 (J104) Login
L01,0?xxx: Chassis
L02,5 = Audi A8 (4D)
L03,7 = Audi A6 (4B)
L04,9 = Audi A4 (8D) / VW Passat (3B)
L05,0x?xx: Brakes
L06,3 = FNRG-60 (Teves/ATE) [PR-1LA/1LG] 
L07,4 = FN2/HP2 (Dual-Piston) [PR-1LX]
L08,5 = FN3 (Teves/ATE) [PR-1LB/1LF/1LT]
L09,6 = C54 (Lucas) [PR-1LZ]
L10,0xx?x: Engine
L11,5 = 4/6/8 Cyl. Diesel
L12,7 = 4/5 Cyl. Gasoline
L13,9 = 6/8/12 Cyl. Gasoline
L14,0xxx?: Transmission
L15,3 = Manual with Low Range (only Audi A6 Allroad)
L16,5 = Manual
L17,7 = Automatic (01N/01V)
L18,9 = Multitronic (01J)
L19, 
L20,Note #1: After Login/Coding-II has been carried out you need to recode the Control Module.
L21,Note #2: For Audi A8 (4D) always use 4 as Selection for Brakes.
L22, 
L23,40168 = Basic Settings Enabling (i.e. mandatory prior to Steering Angle Sensor Alignment)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics - Bosch 5.3 (J104) Coding
C01,0?xxx: Chassis
C02,4 = Audi A4 (8D) / VW Passat (3B)
C03,6 = Audi A6 (4B)
C04,8 = Audi A8 (4D)
C05,0x?xx: Brakes
C06,1 = C54 (Lucas) [PR-1LZ]
C07,2 = FN3 (Teves/ATE) [PR-1LB/1LF/1LT]
C08,3 = FN2/HP2 (Dual-Piston) [PR-1LX]
C09,4 = FNRG-60 (Teves/ATE) [PR-1LA/1LG] 
C10,0xx?x: Engine
C11,5 = 4/6/8 Cyl. Diesel
C12,7 = 4/5 Cyl. Gasoline
C13,9 = 6/8/12 Cyl. Gasoline
C14,0xxx?: Transmission
C15,3 = Manual with Low Range (only Audi A6 Allroad)
C16,5 = Manual
C17,7 = Automatic (01N/01V)
C18,9 = Multitronic (01J)
C19, 
C20,Note #1: Coding is accepted after a specific Login has been carried out.
C21,Note #2: After successful Coding the Steering Angle Sensor Alignment needs to be carried out.
C22,Note #3: For Audi A8 (4D) always use 3 as Selection for Brakes.
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,Bosch ESP 5.3
;
