;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; Audi A3 (8P) / Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia II (1Z)
; VW Eos (1F) / VW Golf/Jetta (1K/5M) / VW Touran (1T)
;
; Component: J104 - Brake Electronics (#03) - ABS MK60 (FWD)
;
; P/N: 1K0-614-517-???
;
; includes measuring blocks, basic setting, coding and security access
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1K-03.LBL
; 2K-03.LBL
; 1K0-614-517-MK60-A.LBL (MK60 AWD)
; 1K0-614-517-MK60-F.LBL (MK60 FWD)
; 1K0-907-379-MK60-A.LBL (MK60 AWD)
; 1K0-907-379-MK60-F.LBL (MK60 FWD)
; 1K0-907-379-MK70.LBL   (MK70)
;
; created on 10/Mar/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 25/May/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Range: 0.0...255.0 km/h
;
B001,0,Brake System Bleeding
B001,1,System Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
003,0,Switches and Warning Lights
003,1,Brake Light,Switch (F),Range: Not Oper./Operated
003,2,Brake System,Warning L. (K118),Range: ON/OFF
003,3,ABS,Warning L. (K47),Range: ON/OFF
003,4,ASR/ESP,Warning L. (K155),Range: ON/OFF
;
004,0,Steering Angle / Lateral Acceleration / Rotation Rate
004,1,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
004,2,Lateral Acc.,Sensor (G200),Specification: ± 1.5 m/s²
004,3,Rotation Rate,,Specification: ± 2.5 °/s
;
005,0,Brake Pressure && Steering Angle Sensor Status
005,1,Brake Pressure,Sensor (G201),Specification: ± 7.0 bar
005,2,Steering Angle,Sensor Condition,Range: Initialised/N. Initialised/Implausible
;
006,0,Longitudinal Acceleration & Vacuum System
006,1,Long. Accel.,Sensor (G251),Specification: ± 1.5 m/s²
;
007,0,ASR/ESP Button
007,1,ASR/ESP Button,(E256),Display Range: Operated/Not Oper.
;
010,0,Additional Functions
010,1,Trailer,Stabilization
010,2,Brake Wiping,(Front),Range: ON/OFF
010,3,Driver's Door,Status,Range: Open/Closed
010,4,Revers Gear,Status,Range: Reverse: No/Reverse: Yes
;
011,0,Speed Encoder Errors (Front Left)
;
012,0,Speed Encoder Errors (Front Right)
;
013,0,Speed Encoder Errors (Rear Left)
;
014,0,Speed Encoder Errors (Rear Right)
;
016,0,Tire Pressure Monitoring (TPMS) I
016,1,Mileage at,last Warning
;
017,0,Tire Pressure Monitoring (TPMS) II
017,1,Mileage at,last Initialization
;
018,0,Tire Pressure Monitoring (TPMS) III
018,1,TPMS Button,Status (E492),Range: Operated/Not Oper.
018,2,Parking Brake,Status,Range: Activated/Not Activated
;
031,0,Tire Pressure Monitoring (TPMS) IV
; 0 = Nothing Learned
; 1 = Only 1st Threshold powered
; 2 = Only 2nd Threshold powered
; 3 = Only 1st Threshold rolling
; 4 = Only 2nd Threshold rolling
; 5 = 1st Threshold powered and rolling
; 6 = 1st Threshold powered and 2nd Threshold rolling
; 7 = 2nd Threshold powered and 1st Threshold rolling
; 8 = 2nd Threshold powered and rolling (Optimal)
031,1,Speed Ranges I
; 5?xxx = Speed Range 1 ( 15 -  70 km/h)
; 5x?xx = Speed Range 2 ( 70 - 100 km/h)
; 5xx?x = Speed Range 3 (100 - 130 km/h)
; 5xxx? = Speed Range 4 (130 - 160 km/h)
031,2,Speed Ranges II
; 5?xxx = Speed Range 5 (160 - 190 km/h)
; 5x?xx = Speed Range 6 (190 - 220 km/h)
; 5xx?x = Speed Range 7 (220 - 250 km/h)
031,3,Curve/Wheel,Recognition
; 5?x00 = Curve Recognition (0 = No Curve / 1 = Left or Right Curve learned / 2 = Complete Curve learned)
; 5x?00 = Wheel Recognition (0 = inactive / 1 = activ)
;
B042,0,Tire Pressure Monitoring System (TPMS) Reset
B042,1,Tire Pressure,Monitoring System
B042,2, , , 
B042,3,Reset Status
B042,4, , , 
;
B060,0,Adjustment of Steering Angle Sensor (G85)
B060,1,Adjustment
B060,2,Adjustment,Status
B060,3,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
;
B063,0,Adjustment of Lateral Acceleration Sensor (G200)
B063,1,Adjustment
B063,2,Adjustment,Status
B063,3,Lateral Acc.,Sensor (G200),Specification: ± 1.5 m/s²
;
B066,0,Adjustment of Brake Pressure Sensor (G201)
B066,1,Adjustment
B066,2,Adjustment,Status
B066,3,Brake Pressure,Sensor (G201),Specification: ± 7.0 bar
;
B069,0,Adjustment of Longitudinal Acceleration Sensor (G251)
B069,1,Adjustment
B069,2,Adjustment,Status
B069,3,Long. Accel.,Sensor (G251),Specification: +/- 1.5 m/s²
;
B093,0,Activate ESP System/Function Test
B093,1,System/Function,Test
B093,2,System/Function,Test Status
B093,3, , , 
B093,4, , , 
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine,,Specification: Engine 1\nRange: Engine 1/Engine 0
125,2,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nRange: Steer. ang. 1/Steer. ang. 0
125,4,Transmission,,Range: Transm. 1/Transm. 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Instrument Cluster,(J285),Specification: Instruments 1\nRange: Instruments 1/Instruments 0
126,2,CAN-Gateway,(J533),Specification: Gateway 1\nRange: Gateway 1/Gateway 0
126,3,Immobilizer,,Specification: Immobilizer 1\nRange: Immobilizer 1/Immobilizer 0
126,4,Steering Aid,(J500),Specification: Steering 1\nRange: Steering 1/Steering 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding - MK60 FWD
C01,Tire Pressure Monitoring:
C02,+0000000 = Tire Pressure Monitoring active
C03,+0016384 = Tire Pressure Monitoring inactive
C04, 
C05,Note #1: See production codes on car data plate.
C06,Note #2: Coding is the sum of the individual options.
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Brake Electronics (J104) Security Access
S01,15082 = Adaptation Enabling
S02,40168 = Basic Setting Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A056,0,Trailer Stabilization
A056,3,Stabilization,Status
A056,5,Trailer Stabilization
A056,6,0 = Trailer Stabilization inactive
A056,7,1 = Trailer Stabilization active
;
A058,0,Hill Hold Assist (HHA)
A058,3,Hill Hold,Assist Status
A058,5,Hill Hold Assist (HHA)
A058,6,0 = Hill Hold Assist (HHA) inactive (PR-UG0)
A058,7,1 = Hill Hold Assist (HHA) "normal"
A058,8,2 = Hill Hold Assist (HHA) "early" (Start with low RPMs)
A058,9,3 = Hill Hold Assist (HHA) "late" (Start with high RPMs and slipping Clutch)
;
A059,0,Hill Hold Assist (HHA): Engine Type
A059,5,Hill Hold Assist (HHA): Engine Type
A059,6,Only valid for 1K0-614-517-R/S!
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,ABS/ESP MK60-AT
;
