;
; VCDS Label File
;
; Copyright © 2005-2009 Ross-Tech, LLC
;
; VW Golf (1J)
;
; Component: Engine (#01) - BJS
;
; P/N: 022-906-032-???
;
; includes measuring blocks, coding and readiness
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 02-01.LBL
; 022-906-032-BJS.LBL  (3.2l E   @ 241 HP - BJS)
;
; created on 27/Jul/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 30/Apr/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Engine Speed
001,2,Coolant,Temperature,Specification: 80.0...110.0 °C
001,3,Lambda Control,Bank 1
001,4,Lambda Control,Bank 2
;
002,0,Basic Functions (Mass Air Flow)
002,1,Engine Speed
002,2,Engine Load
002,3,Injection Timing
002,4,Mass Air Flow
;
003,0,Basic Functions (Mass Air Flow)
003,1,Engine Speed
003,2,Mass Air Flow
003,3,Throttle Position,Sensor (G187)
003,4,Ignition,Timing Angle
;
004,0,Basic Functions
004,1,Engine Speed
004,2,Supply Voltage,,Specification: 12.0...15.0 V
004,3,Coolant,Temperature,Specification: 80.0...110.0 °C
004,4,Intake Air,Temperature
;
005,0,Basic Functions
005,1,Engine Speed
005,2,Engine Load
005,3,Vehicle Speed
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,Basic Functions
006,1,Engine Speed
006,2,Engine Load
006,3,Intake Air,Temperature
006,4,Altitude,Correction Factor
;
008,0,Basic Functions
008,1,Brake Condition,,Display Range: Operated/Not Oper.
008,2,Vacuum Pump,Condition,Display Range: Pump ON/Pump OFF
008,3,Brake Booster,Pressure
;
010,0,Ignition
010,1,Engine Speed
010,2,Engine Load
010,3,Throttle Position,Sensor (G187)
010,4,Ignition,Timing Angle
;
011,0,Ignition
011,1,Engine Speed
011,2,Coolant,Temperature,Specification: 80.0...110.0 °C
011,3,Intake Air,Temperature
011,4,Ignition,Timing Angle
;
014,0,Ignition (Misfire Recognition - Total)
014,1,Engine Speed
014,2,Engine Load
014,3,Misfire,(total),Specification: 0
014,4,Misfire,Recognition,Display Range: Disabled/Enabled
;
015,0,Ignition (Misfire Recognition - Cylinder 1-3)
015,1,Misfire Counter,Cylinder 1
015,2,Misfire Counter,Cylinder 2
015,3,Misfire Counter,Cylinder 3
015,4,Misfire,Recognition,Display Range: Disabled/Enabled
;
016,0,Ignition (Misfire Recognition - Cylinder 4-6)
016,1,Misfire Counter,Cylinder 4
016,2,Misfire Counter,Cylinder 5
016,3,Misfire Counter,Cylinder 6
016,4,Misfire,Recognition,Display Range: Disabled/Enabled
;
018,0,RPM/Load Barriers
018,1,Lower,RPM Barrier
018,2,Upper,RPM Barrier
018,3,Lower,Load Barrier,
018,4,Upper,Load Barrier,
;
020,0,Ignition (Timing Retardation Cylinder 1-4)
020,1,Timing Retardation,Cylinder 1
020,2,Timing Retardation,Cylinder 2
020,3,Timing Retardation,Cylinder 3
020,4,Timing Retardation,Cylinder 4
;
021,0,Ignition (Timing Retardation Cylinder 5-8)
021,1,Timing Retardation,Cylinder 5
021,2,Timing Retardation,Cylinder 6
;
022,0,Ignition (Timing Retardation Cylinder 1 && 2)
022,1,Engine Speed
022,2,Engine Load
022,3,Timing Retardation,Cylinder 1
022,4,Timing Retardation,Cylinder 2
;
023,0,Ignition (Timing Retardation Cylinder 3 && 4)
023,1,Engine Speed
023,2,Engine Load
023,3,Timing Retardation,Cylinder 3
023,4,Timing Retardation,Cylinder 4
;
024,0,Ignition (Timing Retardation Cylinder 5 && 6)
024,1,Engine Speed
024,2,Engine Load
024,3,Timing Retardation,Cylinder 5
024,4,Timing Retardation,Cylinder 6
;
026,0,Ignition (Knock Control Cylinder 1-4)
026,1,Voltage,Cylinder 1
026,2,Voltage,Cylinder 2
026,3,Voltage,Cylinder 3
026,4,Voltage,Cylinder 4

027,0,Ignition (Knock Control Cylinder 5-8)
027,1,Voltage,Cylinder 5
027,2,Voltage,Cylinder 6
;
028,0,Ignition (Knock Sensor Test - Short Trip)
028,1,Engine Speed
028,2,Engine Load
028,3,Coolant,Temperature,Specification: 80.0...110.0 °C
028,4,Result,,Display Range: Test ON/Test OFF/Sys. OK/Sys. not OK\nSpecification: Sys. OK
;
030,0,Lambda Control (Sensor Status)
030,1,Bank 1,Sensor 1
; 1xxxx - Lambda Sensor Control Cyl. 1 active
; x1xxx - Catalytic Converter Venting active
; xx1xx - Lambda Sensor Heating on
; xxx1x - Lambda Sensor ready
; xxxx1 - Lambda Control active
030,2,Bank 1,Sensor 2
; 1xxx - Enabling P Factor
; x1xx - Lambda Sensor Heating on
; xx1x - Lambda Sensor ready
; xxx1 - Lambda Control active
030,3,Bank 2,Sensor 1
; 1xxxx - Lambda Sensor Control Cyl. 1 active
; x1xxx - Catalytic Converter Venting active
; xx1xx - Lambda Sensor Heating on
; xxx1x - Lambda Sensor ready
; xxxx1 - Lambda Control active
030,4,Bank 2,Sensor 2
; 1xxx - Enabling P Factor
; x1xx - Lambda Sensor Heating on
; xx1x - Lambda Sensor ready
; xxx1 - Lambda Control active
;
031,0,Lambda Control (Lambda Sensor Voltages)
031,1,Lambda Sensor,B1-S1 (actual)
031,2,Lambda Sensor,B1-S1 (specified)
031,3,Lambda Sensor,B2-S1 (actual)
031,4,Lambda Sensor,B2-S1 (specified)
;
032,0,Lambda Control (Mixture Adaptation)
032,1,Adaptation (Idle),Bank 1 Sensor 1
032,2,Adaptation (Partial),Bank 1 Sensor 1
032,3,Adaptation (Idle),Bank 2 Sensor 1
032,4,Adaptation (Partial),Bank 2 Sensor 1
;
033,0,Lambda Control
033,1,Lambda Control,Bank 1 Sensor 1
033,2,Sensor Voltage,Bank 1 Sensor 1
033,3,Lambda Control,Bank 2 Sensor 1
033,4,Sensor Voltage,Bank 2 Sensor 1
;
034,0,Lambda Control (Aging Check Bank 1)
034,1,Engine Speed
034,2,Catalytic Converter,Temperature
034,3,Dynamic Factor,Bank 1 Sensor 1
034,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK\nSpecification: B1-S1 OK
;
035,0,Lambda Control (Aging Check Bank 2)
035,1,Engine Speed
035,2,Catalytic Converter,Temperature
035,3,Dynamic Factor,Bank 2 Sensor 1
035,4,Result,Lambda Aging,Display Range: Test ON/Test OFF/B2-S1 not OK/B2-S1 OK\nSpecification: B2-S1 OK
;
036,0,Lambda Control (Sensor Readiness - After Catalyst)
036,1,Sensor Voltage,Bank 1 Sensor 2
036,2,Result,Lambda Availability,Display Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK\nSpecification: B1-S2 OK
036,3,Sensor Voltage,Bank 2 Sensor 2
036,4,Result,Lambda Availability,Display Range: Test ON/Test OFF/B2-S2 not OK/B2-S2 OK\nSpecification: B2-S2 OK
;
037,0,Lambda Control (Delta Lambda Bank 1)
037,1,Engine Load
037,2,Sensor Voltage,Bank 1 Sensor 2
037,3,Delta Lambda,Bank 1 Sensor 2
037,4,Result,,Specification: Test ON/Test OFF/B1-S1 OK/B1-S1 n.OK\nSpecification: B1-S1 OK
;
038,0,Lambda Control (Delta Lambda Bank 2)
038,1,Engine Load
038,2,Sensor Voltage,Bank 2 Sensor 2
038,3,Delta Lambda,Bank 2 Sensor 2
038,4,Result,,Specification: Test ON/Test OFF/B2-S1 OK/B2-S1 n.OK\nSpecification: B2-S1 OK
;
039,0,Lambda Control (Sensor Exchange)
039,1,Mass Air Flow
039,2,Sensor Voltage,Bank 1 Sensor 2
039,3,Sensor Voltage,Bank 2 Sensor 2
039,4,Result,Sensor Exchange,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK\nSpecification: Syst. OK
;
041,0,Lambda Sensor Heating Bank 1
041,1,Resistance,Bank 1 Sensor 1
041,2,Heater Condition,,Display Range: Htg. S1 OFF/Htg. S1 ON
041,4,Heater Condition,,Display Range: Htg. S2 OFF/Htg. S2 ON
;
042,0,Lambda Sensor Heating Bank 2
042,1,Resistance,Bank 2 Sensor 1
042,2,Heater Condition,,Display Range: Htg. S1 OFF/Htg. S1 ON
042,4,Heater Condition,,Display Range: Htg. S2 OFF/Htg. S2 ON
;
043,0,Lambda Sensor Aging Bank 1
043,1,Engine Speed
043,2,Catalytic Converter,Temperature
043,3,Lambda Voltage,Bank 1 Sensor 1
043,4,Result,Aging,Display Range: Test ON/Test OFF/B1-S2 OK/B1-S2 n.OK\nSpecification: B1-S2 OK
;
044,0,Lambda Sensor Aging Bank 2
044,1,Engine Speed
044,2,Catalytic Converter,Temperature
044,3,Lambda Voltage,Bank 2 Sensor 1
044,4,Result,Aging,Display Range: Test ON/Test OFF/B2-S2 OK/B2-S2 n.OK\nSpecification: B2-S2 OK
;
046,0,Catalytic Conversion Test Bank 1
046,1,Engine Speed
046,2,Catalytic Converter,Temperature
046,3,Catalytic,Conversion
046,4,Result,Cat. Conversion,Display Range: Test ON/Test OFF/CatB1 OK/CatB1 n.OK\nSpecification: CatB1 OK
;
047,0,Catalytic Conversion Test Bank 2
047,1,Engine Speed
047,2,Catalytic Converter,Temperature
047,3,Catalytic,Conversion
047,4,Result,Cat. Conversion,Display Range: Test ON/Test OFF/CatB2 OK/CatB2 n.OK\nSpecification: CatB2 OK
;
050,0,Engine Speed Increase
050,1,Engine Speed,(actual)
050,2,Engine Speed,(specified)
050,3,A/C Readiness,,Display Range: A/C-Low / A/C-High
050,4,A/C Compressor,,Display Range: Compr.OFF/Compr.ON
;
051,0,Engine Speed Increase (Gear shifts)
051,1,Engine Speed,(actual)
051,2,Engine Speed,(specified)
051,3,Selected Gear,,Display Range: P or N = 0/Gear = 1 - 6/R = 7
051,4,Supply Voltage,,Specification: 12.0...15.0 V
;
052,0,Engine Speed Increase
052,1,Engine Speed,(actual),Specification (Idle): 640...740 RPM\nSpecification (Load): 3000...3500 RPM\nDisplay Range: 640...6800 RPM
052,2,Engine Speed,(specified)
052,3,A/C Readiness,,Display Range: A/C-Low / A/C-High
;
053,0,Engine Speed Increase (Generator Load)
053,1,Engine Speed,(actual)
053,2,Engine Speed,(specified)
053,3,Supply Voltage,,Specification: 12.0...15.0 V
;
054,0,Idle Speed Stabilization
054,1,Engine Speed
054,2,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Throttle Position,Sensor (G79)
054,4,Throttle Position,Sensor (G187)
;
055,0,Idle Speed Stabilization
055,1,Engine Speed
055,2,Idle Regulator
055,3,Idle Stabilization,Self-Adaptation
055,4,Operating,Condition,00xxx1 = A/C Compressor ON\n00xx1x = Gear engaged\n00x1xx = A/C Readiness ON\n001xxx = Rear Window Heater ON
;
056,0,Idle Speed Stabilization
056,1,Engine Speed,(actual)
056,2,Engine Speed,(specified)
056,3,Idle Regulator
056,4,Operating,Condition,00xxx1 = A/C Compressor ON\n00xx1x = Gear engaged\n00x1xx = A/C Readiness ON\n001xxx = Rear Window Heater ON
;
057,0,Idle Speed Stabilization (Air Condition)
057,1,Engine Speed,(actual)
057,2,Engine Speed,(specified)
057,3,A/C Compressor,,Display Range: Compr.OFF/Compr.ON
057,4,A/C Compressor,Pressure
;
058,0,Engine Mounting
058,1,Engine Speed
058,2,Engine Load
;
060,0,Electronic Throttle Adaptation
060,1,Throttle Position,Sensor (G187)
060,2,Throttle Position,Sensor (G188)
060,3,Adaptation,Steps Counter,Specification: 0
060,4,Result,Throttle Valve Adp.,Display Range: ADP RUN/ADP OK/ADP ERROR\nSpecification: ADP OK
;
061,0,Electronic Throttle
061,1,Engine Speed
061,2,Supply Voltage,,Specification: 12.0...15.0 V
061,3,Throttle Position,Sensor (G187)
061,4,Operating,Condition,00xxx1 = A/C Compressor ON\n00xx1x = Gear engaged\n00x1xx = A/C Readiness ON\n001xxx = Rear Window Heater ON
;
062,0,Electronic Throttle
062,1,Throttle Position,Sensor (G187)
062,2,Throttle Position,Sensor (G188)
062,3,Throttle Position,Sensor (G79)
062,4,Accelerator Pedal,Position  (G185)
;
063,0,Electronic Throttle (Kick-Down Adaptation)
063,1,Throttle Position,Sensor (G79)
063,2,Kick-Down,Adaptation Value
063,3,Kick-Down,Switch,Display Range: Kick Down
063,4,Kick-Down,Adaptation,Display Range: ADP RUN/ADP OK/ADP ERROR\nSpecification: ADP OK
;
064,0,Throttle Valve Potentiometer Adaption Values
064,1,Potentiometer 1,Lower Adaptation
064,2,Potentiometer 2,Lower Adaptation
064,3,Emergency Air Gap,Potentiometer 1
064,4,Emergency Air Gap,Potentiometer 2
;
066,0,Cruise Control System
066,1,Vehicle Speed,(current)
066,2,Pedal Settings
; ----1xxx - Cruise control system active
; ----x1xx - Clutch depressed (always 1 in automatic transmission)
; ----xx1x - Brake depressed (brake pedal switch)
; ----xxx1 - Brake depressed (brake light switch)
066,3,Vehicle Speed,(specified)
066,4,Switch Settings
; ----1xxx - CCS slide handle on RES or RES button on multi-function steering wheel pressed
; ----x1xx - SET button pressed
; ----xx1x - CCS slide handle on OFF (not engaged or engaged)/OFF button on multi-function steering wheel pressed
; ----xxx1 - CCS slide handle on OFF
;
070,0,Emission Reduction (TEV - Basic Setting)
070,1,Evap. Emissions,Sol. Valve (Open),Specification: 0...100 %
070,2,Lambda Control
070,3,Evap. Emissions,Sol. Valve (Flow)
070,4,Result,,Display Range: Test ON/Test OFF/TEV OK/TEV not OK
;
071,0,Exhaust Reduction (Basic Setting: Leak Diagnostic System)
071,1,Reed Contact,Condition,Display Range: Reed Open/Reed Closed
071,2,Malfunction Display,,Display Range: minor leak/significant leak/Open circuit
071,3,Diagnostic Status,,Display Range: System test/Measurement end
071,4,Result,Leak Test,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
072,1,Reed Contact,Condition
072,2,Malfunction,Message
072,4,Result
;
073,1,Opening angle,of TVV
073,2,Flush rate
073,3,Load factor
073,4,TE-Fuel portion
;
077,0,Emission Reduction (Bank 1)
077,1,Engine Speed
077,2,Mass Air Flow
077,3,Air Mass from,Sec. Air Inj. Bank 1
077,4,Result,,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK
;
078,0,Emission Reduction (Bank 2)
078,1,Engine Speed
078,2,Mass Air Flow
078,3,Air Mass from,Sec. Air Inj. Bank 2
078,4,Result,,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK
;
079,1,Engine Speed
079,2,Engine Load
079,3,Flap Bank 1
079,4,Flap Bank 2
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,VIN & IMMO-ID
;
082,0,Advanced Control Module Identification III
;
086,0,Readiness Code I
086,1,Readiness Bits
086,2,Cycle Flags
086,3,Cycle Flags
086,4,Cycle Flags
;
087,0,Readiness Code II
087,1,Readiness Bits
087,2,Error Flags
087,3,Error Flags
087,4,Error Flags
;
088,0,Readiness Code III
088,1,Cycle Flags
088,2,Cycle Flags
088,3,Cycle Flags
;
089,1,Distance Driven,with MIL on
089,2,Tank Condition,,Display Range: OK/too low
;
090,0,Continuous Camshaft Adjustment (Bank 1 - Exhaust)
090,1,Engine Speed
090,2,Duty Cycle
090,3,Adjustment Bank 1,(specified)
090,4,Adjustment Bank 1,(actual)
;
091,0,Continuous Camshaft Adjustment (Bank 1 - Intake)
091,1,Engine Speed
091,2,Duty Cycle
091,3,Adjustment Bank 1,(specified)
091,4,Adjustment Bank 1,(actual)
;
093,0,Continuous Camshaft Adjustment (Bank 2 - Intake)
093,1,Engine Speed
093,2,Duty Cycle
093,3,Adjustment,(specified)
093,4,Adjustment,(actual)
;
094,0,Continuous Camshaft Adjustment (Intake)
094,1,Adjustment,Bank 1
094,2,Adjustment,Bank 2
094,3,Result Bank 1,,Display Range: Test OFF/Test ON/System OK/System Not OK
094,4,Result Bank 2,,Display Range: Test OFF/Test ON/System OK/System Not OK
;
095,0,Performance Increase (Intake Manifold Change Over)
095,1,Engine Speed,,Specification: 650...6500 RPM
095,2,Engine Load,,Specification: 0...100 %
095,3,Coolant,Temperature,Specification: 80.0...110.0 °C
095,4,Switch-Over,Staus,Display Range: IMC-V ON/IMC-V OFF
;
096,0,Continuous Camshaft Adjustment (Exhaust)
096,1,Adjustment,Bank 1
096,2,Adjustment,Bank 2
096,3,Result Bank 1,,Display Range: Test ON/Test OFF/System OK/System Not OK\nSpecification: System OK
096,4,Result Bank 2,,Display Range: Test ON/Test OFF/System OK/System Not OK\nSpecification: System OK
;
098,0,Continuous Camshaft Adjustment (Exhaust - Bank 2)
098,1,Engine Speed
098,2,Engine Load
098,3,Adjustment,(specified)
098,4,Adjustment,(actual)
;
099,0,Lambda Control Shut-Off (Basic Setting)
099,1,Engine Speed
099,2,Lambda Control,Bank 1
099,3,Lambda Control,Bank 2
099,4,Lambda Control,Status,Display Range: O2-Reg.OFF/O2-Reg.ON
;
100,0,Readiness Code
100,1,Readiness Bits,,see labelfile
; 1xxxxxxx - Exhaust Gas Recirculation (EGR)
; x1xxxxxx - Sensor heater
; xx1xxxxx - Oxygen sensors
; xxx1xxxx - A/C system
; xxxx1xxx - Secondary Air Injection (AIR) system
; xxxxx1xx - Activated charcoal system
; xxxxxx1x - Catalytic converter heater
; xxxxxxx1 - Catalytic converter
100,2,Coolant,Temperature,Specification: 80.0...110.0 °C
100,3,Time since,Engine Start
100,4,OBD-Status,,see labelfile
; 1-xxxxxx - MIL warning lamp on
; x-1xxxxx - Complete distance
; x-x1xxxx - At least one malfunction detected
; x-xx--1x - Heating cycle ended
; x-xx--x1 - Heating cycle not possible
;
101,0,Fuel Injection
101,1,Engine Speed
101,2,Engine Load
101,3,Injection Timing
101,4,Mass Air Flow
;
102,0,Fuel Injection
102,1,Engine Speed
102,2,Coolant,Temperature,Specification: 80.0...110.0 °C
102,3,Intake Air,Temperature
102,4,Injection Timing
;
104,0,Start Adaption Values
104,1,Start Engine,Temperature
104,2,Temperature,Adaptation Factor 1
104,3,Temperature,Adaptation Factor 2
104,4,Temperature,Adaptation Factor 3
;
105,0,Cylinder Shut-Off
105,1,Engine Speed
105,2,Engine Load
105,3,Coolant,Temperature,Specification: 80.0...110.0 °C
105,4,Status,Cylinder Shut-Off,Display Range: ON/OFF
;
107,0,Lambda Control
107,1,Engine Speed
107,2,Lambda Control,Bank 1 (average)
107,3,Lambda Control,Bank 2 (average)
107,4,Result,Lambda Control,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK\nSpecification: Syst. OK
;
110,0,Load/Full Throttle Enrichment
110,1,Engine Speed
110,2,Coolant,Temperature,Specification: 80.0...110.0 °C
110,3,Injection Timing
110,4,Throttle Position,Sensor (G187)
;
112,0,Exhaust Gas Temperature
112,1,Exhaust Gas,Temperature Bank 1
112,3,Exhaust Gas,Temperature Bank 2
;
113,0,Load/Full Throttle Enrichment
113,1,Engine Speed
113,2,Engine Load
113,3,Throttle Position,Sensor (G187)
113,4,Athmospheric,Pressure
;
120,0,Traction Control (ASR)
120,1,Engine Speed
120,2,Engine Load,(specified)
120,3,Engine Load,(actual)
120,4,Status,,Specification: ASR OFF/ASR ON
;
122,0,Transmission
122,1,Engine Speed
122,2,Engine Load,(specified)
122,3,Engine Load,(actual)
122,4,Status,,Display Range: Engine interv./No engine interv.
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Transmission,,Display Range: Transm. 1/Transm. 0
125,2,Brake Electronics,,Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,3,Instrument Cluster,,Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
;
126,0,CAN-Databus Powertrain (Communication)
126,3,Airbag,,Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
;
130,0,Map Cooling
130,1,Engine Outlet,Temperature
;
131,0,Map Cooling
131,1,Engine Outlet,Temperature
;
134,0,Temperatures
134,1,Oil Temperature
134,2,Ambient,Temperature
134,3,Intake Air,Temperature
134,4,Engine Outlet,Temperature
;
137,0,Air Condition Requirements
137,1,A/C Readiness,,Display Range: A/C-Low / A/C-High
137,2,A/C Compressor,,Display Range: Compr.OFF/Compr.ON
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine Control Module (J220) Coding
C01,0000132 - Manual Transmission
C02,0000133 - Automatic Transmission (02E / DSG)
;
;
;---------------------------------------------------
;
; readiness
;
;---------------------------------------------------
;
;
O,022-906-032-BJS
;
