;
; VCDS Label File
;
; Copyright © 2008 Ross-Tech, LLC
;
; Audi A4 (8K) / Audi A5 (8K) / Audi A6 (4F) / Audi A8 (4E) / Audi Q7 (4L)
;
; Component: R199 - Media Player (#0E/#1E/#2E) - Audi Music Interface (AMI) MOST
;
; P/N: 4E0-035-785-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4E0-035-785.LBL - Audi Music Interface (AMI) MOST
; 8T0-035-785.CLB - Audi Music Interface (AMI) CAN
;
; includes measuring blocks, adaptation and long coding
;
; created on 06/Jul/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 03/Nov/2008
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Voltages
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Voltage Status,,0000xxx1 = Term. S active\n0000xx1x = Term. 15 active\n0000x1xx = Term. X active\n00001xxx = Term. 50 active
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
002,4,Send Diode,Temperature
;
003,0,MOST-Databus
003,1,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
004,0,MOST-Databus
004,1,System Status
004,2,MMI Status
;
005,0,MOST-Databus
005,1,Hardware Instance
005,2,Ring Break,Diagn. Wire Level,0 = low\n1 = high
;
006,0,Freeze Frame Data
006,1,Unlearn Counter,& Mileage
006,2,Mileage
;
007,0,Freeze Frame Data
007,1,Time Indic. Bit,Time Stamp
007,2,Time Stamp
007,3,Time Stamp
;
016,0,Used Drivers
016,1,Used Drivers,,See Label File
; 00000000 00010000
; 00000000 xxxxxxx? = Aux (Driver for 3.5mm Connector active)
; 00000000 xxxxxx?x = DAP UART (Driver iPod active)
; 00000000 xxxxx?xx = DAP USB-MC (Driver for USB-Drive active)
; 00000000 xxxx?xxx = DAP MTP (Driver for USB with Media Transfer Protocol active)
; 00000000 xxx?xxxx = DSP
; 00000000 xx?xxxxx = DAP Bluetooth Audio Streaming (Driver for MP3 Player via Bluetooth active)
; 00000000 x?xxxxxx = DAP Next 1
; 00000000 ?xxxxxxx = DAP Next 2
;
017,0,Adapter Cable
017,1,Adapter Cable,,00000000 xxxxxxx? = No Cable connected\n00000000 xxxxxx?x = AUX (3.5mm Connector Cable connected)\n00000000 xxxxx?xx = DAP UART (iPod Cable connected)\n00000000 xxxx?xxx = DAP USB-MC (USB Cable connected)\n00000000 xxx?xxxx = DAP MTP (USB-Cable for Player with Media Transfer Protocol connected)\n00000000 xx?xxxxx = Zune (Microsoft MP3 Player connected)\n00000000 x?xxxxxx = Standard Cable\n00000000 ?xxxxxxx = Bluetooth Audio Streaming (Bluetooth Dongle connected)
;
018,0,Codec
018,1,Used Codec,,00000000 00xxxxx? = No Codec used\n00000000 00xxxx?x = MP3\n00000000 00xxx?xx = MP3-Pro\n00000000 00xx?xxx = WMA\n00000000 00x?xxxx = OGG\n00000000 00?xxxxx = AAC
;
019,0,Power Supply for External Player
019,1,Ext. Player Power,Supply Status
019,2,Ext. Player,Power Supply,Range: 0.0..25.5 V\nStandard: ~5.0 V
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A20,0,
;1
A20,1,
;N/A
A20,2,
;N/A
A20,3,
;N/A
A20,4,
;N/A
;
A21,0,
;0
A21,1,
;00000000 00000000
A21,2,
;0
A21,3,
;N/A
A21,4,
;N/A
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
;
;---------------------------------------------------
;
; long coding (supported by firmware >= 0800)
;
;---------------------------------------------------
;
;
; {Country}
LC,00,0~7,00,Default (Delivery)
LC,00,0~7,01,Rest of World (RoW)
LC,00,0~7,02,North American Region (NAR)
LC,00,0~7,03,Japan (JP)
LC,00,0~7,04,China (CN)
LC,00,0~7,05,Russia (RUS)
LC,00,0~7,06,South Korea (KR)
;
