;
; VCDS Label File
;
; Copyright © 2008-2011 Ross-Tech, LLC
;
; Seat Ibiza (6L) / Skoda Fabia/Roomster (6Y/5J) / VW Polo (9N)
;
; Component: J301 - Climate Control (#08) - Climatic
;
; P/N: 6?0-820-045-???
;
; includes measuring blocks and basic setting
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 5J-08.LBL
; 6L-08.LBL
; 6Y-08.LBL
; 6Q0-820-045.LBL
;
; created on 16/Feb/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 08/Feb/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage,(Terminal 15)
001,2,Fresh Air Blower,(V2) Position,Switch Position & Voltage Specification\n\n1 = 0.0 V\n1 = 3.0...4.5 V\n2 = 5.0...7.0 V\n3 = 7.5...10.0 V\n4 = 10.5...14.0 V
001,3,Coolant Fan,(Stage 1),Range: ON/OFF
001,4,Coolant Fan,(Stage 2),Range: ON/OFF
;
B001,0,Flap Motor Basic Setting
B001,1,Temp. Regulator,Flap Motor (V68),Specification: 0
B001,2,Outside/Recirc.,Air Flap (V154),Specification: 0
B001,3, , , 
B001,4, , , 
;
002,1,Compressor Load,,Range: 0.0...100.0 %
002,2,Refrigerant,Pressure (G65),Specification: 2.0...32.0 bar 
002,3,Comprossor,Shut-Off,Specification: 0/6/7 (See Label File)
;  0 = Compressor Running
;  1 = Compressor OFF by Pressure Switch (F129): Refrigerant Pressure too High
;  2 = Compressor OFF by Pressure Switch (F129): Refrigerant Pressure too Low
;  3 = Compressor OFF by Missing Engine Speed Signal
;  6 = Compressor OFF by ECON Button
;  7 = Compressor OFF by OFF Button (via Fresh Air Blower Speed Buttons)
;  8 = Compressor OFF by Ambient Temperature below 3 °C (37 °F)
; 10 = Compressor OFF by Voltage below 9.5 V
; 11 = Compressor OFF by Coolant Temperature too High
; 12 = Compressor OFF by Engine OR Transmission Control Module (Compressor Load Limitation)
; 14 = Compressor OFF by Evaporator Temperature too Low
; 16 = Evaporator Temperature Sensor (G263) faulty OR Coolant Fan not working
002,4,Temperature (G263),Evaporator
;
003,1,Temperature at,Floor Outlet (G192)
003,2,Temperature at,Center Outl. (G191)
003,3,Temperature at,A/C Panel (G56)
003,4,Heat Exchanger,Deactivation,Range: ON/OFF
;
004,0,Motor for Outside/Recirculated Air Flap (V154) / Potentiom. (G143)
004,1,Potentiom. (G143),(actual),Range: 0...255\nTolerance (to Specification): ± 2
004,2,Potentiom. (G143),(specified),Range: 0...255
004,3,Stop/Learned,(Fresh Air),saved after Basic Setting (Specification: 150...250)
004,4,Stop/Learned,(Recirculated),saved after Basic Setting (Specification: 5...100)
;
005,0,Motor for Temperature Regulator Flap (V68) / Potentiom. (G92)
005,1,Potentiom. (G92),(actual),Range: 0...255\nTolerance (to Specification): ± 2
005,2,Potentiom. (G92),(specified),Range: 0...255
005,3,Stop/Learned,(Heating),saved after Basic Setting (Specification: 150...250)
005,4,Stop/Learned,(Cooling),saved after Basic Setting (Specification: 5...100)
;
006,1,Engine Speed
006,2,Idle Speed,Increase,Range: ON/OFF
006,3,Vehicle Speed,,Range: 0...255 km/h
006,4,Reverse Gear,engaged,Range: Reverse OFF/Reverse ON
;
007,1,Standing Time
007,2,Status,Terminal X,Range: ON/OFF
007,3,Dimming,(Terminal 58d),Range: 0.0...100.0 %
007,4,Auxiliary,Heater (Z35),Range: ON/OFF
;
008,1,Outside Air,Temperature (G17)
008,2,Coolant,Temperature (G62)
008,3,Coolant Temperat.,"too High",Range: ON (Coolant Temperature not OK)/OFF (Coolant Temperature OK)
008,4,Compressor Load,Limitation,Range: ON/OFF
;
080,0,Advanced Control Module Identification I
;
