;
; VAG-COM Label File
;
; Audi A6 (4B)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 4B0-919-???-???
;
; includes measuring blocks, adaptation, coding, login
;          and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4B-17.LBL
; 4Z-17.LBL
; 4B0-919-xxx-17.LBL
; 4B0-920-xxx-17.LBL
;
; created on 02/Oct/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 01/Jan/2008
;
; requires VAG-COM 610.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
020,0,Immobilizer - ID Block 1
020,1,Digit 1 && 2
020,2,Digit 3 && 4
020,3,Digit 5 && 6
020,4,Digit 7 && 8
;
021,0,Immobilizer - ID Block 2
021,1,Digit 9 && 10
021,2,Digit 11 && 12
021,3,Digit 13 && 14
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...4
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = Not Locked / 1 = Locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+01 = Brakepad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,+16 = Secondary Display (Radio/Navigation) active
C06,xx?xx: Country
C07,1 = Europe / 2 = USA
C08,3 = Canada/Mexico/Latin America
C09,4 = Great Britain (GB) / 5 = Japan
C10,6 = Saudi Arabia / 7 = Australia
C11,xxx?x: Cylinders
C12,4 = 4-Cylinders
C13,5 = 5-Cylinders
C14,6 = 6-Cylinders
C15,xxxx?: Engine
C16,0 = TDI-Engine
C17,2 = 6-Cylinder Gasoline Engine
C18,3 = 8-Cylinder Gasoline Engine
;
;
;---------------------------------------------------
;
; login information
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A02,0,Service Reminder
A02,5,Service Reminder
A02,6,Displayed Values:
A02,7,01 = Oil Service Due
A02,8,10 = Inspection Due
A02,9,11 = Oil Service and Inspection Due
A02,10, 
A02,11,New Values:
A02,12,00 = Reset Oil Service and Inspection
A02,13,01 = Reset Oil Service
A02,14,10 = Reset Inspection
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A4,0,Language for error messages and navigation
A4,5,Language for error messages and navigation
A4,6,1 - German
A4,7,2 - English
A4,8,3 - French
A4,9,4 - Italian
A4,10,5 - Spanish
A4,11,6 - Portuguese
A4,12,8 - Czech
;
A5,0,Service reminder - Maximum distance for oil change "OIL"
A5,5,Service reminder - Maximum distance for oil change (in 1000km)
A5,6,15 - 15.000km (Standard)
;
A6,0,Service reminder - Maximum distance "INSP 01"
A6,5,Service reminder - Maximum distance (in 1000km)
A6,6,30 - 30.000km (Standard)
;
A7,0,Service reminder - Maximum time "INSP 02"
A7,5,Service reminder - Maximum time (in 10 Days)
A7,6,37 - 370 Days (Standard)
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km.
A009,11, 
A009,12,NOTE: Perform Login first.
;
A10,0,Service reminder - Distance for oil change "OIL"
A10,5,Service reminder - Distance for oil change (in 1000km)
A10,6,15 - 15.000km (Standard)
;
A11,0,Service reminder - Distance "INSP 01"
A11,5,Service reminder - Distance (in 1000km)
A11,6,30 - 30.000km (Standard)
;
A12,0,Service reminder - Time "INSP 02"
A12,5,Service reminder - Time (in 10 Days)
A12,6,37 - 370 Days (Standard)
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 96...160 (-8.0...+8.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Maximum Distance to Oil Change (OEL),1000,km
RD,6,Maximum Distance to Inspection (IN1),1000,km
RD,7,Maximum Time to Inspection (IN2),10,Days
RD,10,Distance to Oil Change (OEL),1000,km
RD,11,Distance to Inspection (IN1),1000,km
RD,12,Time to Inspection (IN2),10,Days
;
RJ,0,0,Service Reset (OIL &  INSP),,
RJ,0,1,2,0
;
RJ,1,0,Service Reset (OIL),,
RJ,1,1,2,10
;
RJ,2,0,Service Reset (INSP),,
RJ,2,1,2,1
;
