;
; VCDS Label File
;
; Copyright © 2004+ Ross-Tech, LLC
;
; Audi A4 (8E)
;
; Component: J393 - Central Module Comfort System (#46) - MAX/USA
;
; p/n: 8E0-959-433-???
;
; includes measuring blocks, coding, adaptation and selective output test
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8E-46.LBL
; 8E0-959-433-MAX.LBL
; 8E0-959-433-MIN.LBL
;
; created on 26/Sep/2004 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 09/Jul/2012
;
; requires VCDS 11.11.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Driver's Side
001,1,Driver's Side,Key Switch,Display Range: Open/Closed/Not Oper.
001,2,Central Locking,Button,Display Range: Locking/Unlocking/Not Oper.
001,3,Driver's Side,Lock Status,Display Range: Locked/Unlocked
001,4,Driver's Side,Safe Status,Display Range: Safe/Not Safe
;
002,0,Driver Side/Passenger Side
002,1,Driver's Side,Key Switch,Display Range: Open/Closed/Not Oper.
002,2,Passenger Side,Key Switch,Display Range: Open/Closed/Not Oper.
002,3,Passenger Side,Lock Status,Display Range: Locked/Unlocked
002,4,Passenger Side,Safe Status,Display Range: Safe/Not Safe
;
003,0,Rear Right/Left (Return Messages)
003,1,Rear Right,Lock Status,Display Range: Locked/Unlocked
003,2,Rear Right,Safe Status,Display Range: Safe/Not Safe
003,3,Rear Left,Lock Status,Display Range: Locked/Unlocked
003,4,Rear Left,Safe Status,Display Range: Safe/Not Safe
;
004,0,Door Contacts (Rotary Traps)
004,1,Door Contact,Driver's Side,Display Range: Door Open/Door Closed
004,2,Door Contact,Passenger Side,Display Range: Door Open/Door Closed
004,3,Door Contact,Rear Right,Display Range: Door Open/Door Closed
004,4,Door Contact,Rear Left,Display Range: Door Open/Door Closed
;
005,1,Trunk Lid,Release Button,Display Range: Operated/Not Oper.
005,2,Trunk Lid,Contact Switch,Display Range: Lid Open/Lid Closed
005,3,Soft-Touch,Trunk Lid Release,Display Range: Operated/Not Oper.
005,4,Engine Hood,Contact Switch,Display Range: Lid Open/Lid Closed
;
006,1,Interior Light,,Display Range: ON/OFF
006,2,Window Regulator,Relief Relay,Display Range: Relay ON/Relay OFF
006,3,Comfort System,,Display Range: Open/Closed/Not Oper.
006,4,Luggage,Compartment Light,Display Range: ON/OFF
;
007,1,Key Number,(Memory Position),0 = Not Operated\n1-4 = Key Number
007,2,Remote Control,Command,0 = Not Operated\n1 = Open\n2 = Close\n3 = Open Rear Lid\n4 = Panic Button
007,3,Adapted Key,Memory Positions,Display Range: 0 = Not Occupied / 1 = Occupied\n\n?xxx = Key 1\nx?xx = Key 2\nxx?x = Key 3\nxxx? = Key 4
007,4,Parking Brake,,Display Range: Operated/Not Oper.
;
008,1,Vehicle Speed
008,2,Immobilizer,(Key recognized),Display Range: Yes/No
008,3,Radio Ground,Contact recognized,Display Range: Recognized/No/Not Installed
008,4,Rear Windshield,broken,Display Range: Recognized/No/Not Installed
;
009,1,Control Module,Coding
009,2,Control Module,Coding
009,3,Thermal,Protection,Display Range: 0 = Not Active/1 = Active\n\n?xxx = Driver's Door\nx?xx = Passenger Door\nxx?x = Rear Right\nxxx? = Rear Left
009,4,Window Regulator,Standardized,Display Range: 0 = Not Stand./1 = Stand.\n\n?xxx = Driver's Door\nx?xx = Passenger Door\nxx?x = Rear Right\nxxx? = Rear Left
;
010,1,Driver's Door,(Door Contact),Display Range: Door Open/Door Closed
010,2,Interior Monitoring,Deactivation Button,Display range: operated/Not Oper./Not Installed
010,3,Inclination Sensor,Deactivation Button,Display range: operated/Not Oper./Not Installed
010,4,Back-Up Light,,Display Range: ON/OFF
;
011,0,Window Regulator Buttons
011,1,Driver's Side,,Display Range: auto. open/auto. close/man. open/man.close/Not Oper.
011,2,Driver's Side,for Pass. Side,Display Range: auto. open/auto. close/man. open/man. close/Not Oper.
011,3,Driver's Side,for Rear Right,Display Range: auto. open/auto. close/man. open/man. close/Not Oper.
011,4,Driver's Side,for Rear Left,Display Range: auto. open/auto. close/man. open/man. close/Not Oper.
;
012,0,Mirror System
012,1,Mirror Adjustment,Switch,Display Range: Pos. X+/Pos. X-/Pos. Y+/Pos. Y-/Not Oper.
012,2,Mirror Selection,Switch,Display Range; Left/Right/Fold-Out/Not Oper.
012,3,Mirror Disengage,Switch,Display Range: Disengaged/Engaged/Not Installed
012,4,Heated Mirror,Driver's Side,Display Range: ON/OFF
;
013,1,Window Regulator,Button Pass. Side,Display Range: auto. open/auto. close/man. open/man. close/Not Oper.
013,2,Child Safety Switch,,Display Range: ON/OFF
013,3,Central Locking,Button Pass. Side,Display Range: locking/unlocked/Not Oper. (China only)
013,4,Heated Mirror,Passenger Side,Display Range: ON/OFF
;
014,0,Window Regulator && Central Locking Buttons (Rear)
014,1,Window Regulator,Button Rear Right,Display Range: auto. open/auto. close/man. open/man. close/Not Oper./Not Installed
014,2,Window Regulator,Button Rear Left,Display Range: auto. open/auto. close/man. open/man. close/Not Oper./Not Installed
014,3,Central Locking,Button Rear Right,Display Range: locking/unlocking/Not Oper. (China only)
014,4,Central Locking,Button Rear Left,Display Range: locking/unlocking/Not Oper. (China only)
;
015,1,Supply Voltage,(Terminal 30)
015,2,Status,Terminal 15,Display Range: Term. 15 On/Term. 15 Off
015,3,Status,S-Contact,Display Range: Activated/Not Oper.
015,4,Comfort-BUS,Condition,Display Range: 1-Wire/2-Wire
;
016,1,Rear Central,Locking Button,Display Range: locking/unlocking/not operated (USA only)
016,2,Driver Side Lock,(Return Message),Display Range: locked/unlocked
016,3,Trunk Key Switch,,Display Range: open/closed/not operated
016,4,Glas Type,,Display Range: 0 = Normal/1 = Insulated\n\n?xxx = Driver's Door\nx?xx = Passenger Door\nxx?x = Rear Right\nxxx? = Rear Left
;
017,0,Inclination Sensor
017,1,Tilt X-Axis
017,2,Tilt Y-Axis
017,3,Byte Status
;
125,0,CAN-Databus Communication (Comfort)
125,1,Door Control Mod.,Driver's Side,Specification: Dr. Door 1
125,2,Door Control Mod.,Passenger Side,Specification: Pas. Door 1
125,3,Door Control Mod.,Rear Left,Specification: 
125,4,Door Control Mod.,Rear Right,Specification: 
;
126,0,CAN-Databus Communication (Comfort)
126,1,Steering Wheel,Electronics,Specification: St. Wheel 1
126,2,Central Electronics,,Specification: Cent Elec 1
126,3,Climatronic,,Specification: A/C 1
126,4,Instrument Cluster,,Specification: Instruments 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C0,Comfort System (J393) Coding
C1,+00001 - GB-Alarm (not USA)
C2,+00002 - Confirmation Anti-Theft Warning System (Blink)
C3,+00004 - Selective Central Locking (SCL)
C4,+00008 - Anti-Theft Warning System
C5,+00016 - Rear Lid Release Locking at 5 km/h
C6,+00032 - Central Locking at 15 km/h (or 10 mph)
C7,+00064 - Comfort Function via Remote Control (not USA)
C8,+00128 - Right Hand Drive (RHD)
C9,+00256 - Avant
C10,+00512 - Confirmation Close via Remote (1x Blink)
C11,+01024 - Confirmation Anti-Theft Warning Sytem Horn Activation
C12,+02048 - Door-/Window Regulator Logic
C13,+04096 - Thatcham Anti-Theft Warning (not USA)
C14,+08192 - No Safe-Function 
C15,+16384 - Side Windows with Insulated Glass
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A61,0,Variants Reduction
A61,5,Variants Reduction
A61,6,+1 = Rear Mechanical Window Regulators (PR-4R5) installed 
A61,7,+2 = Footwell Lights (PR-QQ1) installed
A61,8,+4 = Fuel Tank Lid/Flap Release Button (PR-4K2/4K8) installed
;
A62,0,Comfort Functions
A62,5,Comfort Functions
A62,6,+001 - Comfort closing via remote for window regulators (not USA)
A62,7,+002 - Comfort opening via remote for window regulators (not USA)
A62,8,+004 - Comfort closing via lock cylinder for window regulators
A62,9,+008 - Comfort opening via lock cylinder for window regulators
A62,10,+016 - Comfort closing via remote for sunroof (not USA)
A62,11,+032 - Comfort opening via remote for sunroof (not realized)
A62,12,+064 - Comfort closing via lock cylinder for sunroof
A62,13,+128 - Comfort opening via lock cylinder for sunroof (not realized)
;
A63,0,Glass Variant
A63,5,Glass Variant
A63,6,0 = Standard Glass installed
A63,7,1 = Isolating Glass installed
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1565,Trunk Light (W3)
T332,Fuel Tank Lid/Flap Release Button
T1699,Motor for Central Locking: Rear Lid (V53)
T1134,Alarm Horn (H12)
T2225,Lamp for Central Locking
T1338,Signal "Doors not closed"
;
