;
; VAG-COM label file 3D0-907-135.lbl
;
; VW Phaeton (3D) - up to and including model year 2005 (fully tested with 2004 W12 Phaeton NAR and ROW)
;
; component: Roof Electronics -J528-  (#38)
;
; p/n: 3D0 907 135 B Component: Dachmodul 0605  Coding: 0000015 (NAR and ROW Phaeton)
; p/n: 3W0 907 135 C Component: Dachmodul 0703  Coding: 0000157 (Bentley Continental GT - not tested)
;
; includes measured value blocks, coding, and adaptation
;
; by Michael Moore (Moore@ross-tech.com) 'PanEuropean' on the VW Vortex forum.
; tested on a 2004 W12 Phaeton - not all blocks may show on other vehicles.
;
; last modified: 22/July/2005 (Michael)
;  - coding information clarified to avoid confusion between heat reflecting and heat insulating glass.
;                29/November/2005 (Michael) - measuring block data enhanced.
;                13/December 2005 (Michael) - production codes added to coding section.
;                                           - refer to build sticker in spare tire well or owner manual.
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
;Remark: Data exists many blocks, but it is not fully documented
;
;
001,0,Power Supply to Controller
001,1,Battery,Voltage,Voltage measured at roof controller.
001,2,Not Used
001,3,Not Used
001,4,Not Used
;
002,0,Cabin Dome Lights
002,1,Front Cabin,Switch E326,Position of Front Cabin Dome Light Switch.
002,2,Front Cabin W1,% Illumination
002,3,Rear Cabin,Switch E327,Position of Rear Cabin Dome Light Switch.
002,4,Rear Cabin W43,% Illumination
;
003,0,Front Seat (Driver and Front Passenger) Reading Lights
003,1,Driver Reading,Switch E457/E458
003,2,Not Used
003,3,Driver Lamp W19,% Illumination
003,4,Passenger Lamp W13,% Illumination
;
004,0,Rear Seat Reading Lights
004,1,Left Rear,Switch E454/E456
004,2,Not Used
004,3,Left Rear Seat,% Illumination
004,4,Right Rear Seat,% Illumination
;
005,0,Interior Rear View Mirror Position Sensor (for cars with memory mirror)
005,1,Horizontal Position,Sensor G353
005,2,Horizontal Position,Sensor G353
005,3,Vertical Position,Sensor G354
005,4,Vertical Position,Sensor G354
;
006,0,Unknown
;
007,0,Sunroof Switches
007,1,Sunroof Blind,Button
007,2,Sunroof Switch,E8
007,3,Not Used
007,4,Not Used
;
008,0,Automatic Day Night Interior Mirror (Auto-Dimming Mirror)
; REMARK - need to get full width text from VAS 5052
008,1,Y7 EC mirror in,inside mirror, (voltage)
008,2,Not Used
008,3,E386 Button for,anti dazzle mirror,Mirror dark - button active. Mirror light - button not active.
008,4,E386 Button for,anti dazzle mirror,Mirror dark - button active. Mirror light - button not active.
;
009,0,Sunroof
009,1,Unknown
009,2,Sunroof,Status
009,3,Sunroof,Installed,Indicates if a sunroof is installed.
009,4,Not Used
;
010,0,Interior Monitoring (Anti-Theft)
010,1,K-Wire,Status
010,2,Monitoring,Status
010,3,Monitoring,Installed
010,4,Not Used
;
011,0,Rain and Light Sensor
011,1,K-wire,Status
011,2,Rain sensor,Status
011,3,Light sensor,Status
011,4,Auto light control,Installed
;
012,0,G355 Humidity Sensor (IR sensor facing forward on interior mirror mounting arm)
012,1,Temperature,sensor
012,2,Reference,temperature
012,3,Air,temperature
012,4,Air humidity,frequency
;
013,0,G355 Humidity Sensor (IR sensor facing forward on interior mirror mounting arm)
013,1,Voltage,supply
013,2,Not Used
013,3,N340 Heater,for sensor
013,4,N340 Heater,return message
;
014,0,Unknown
014,3,Not Used
014,4,Not Used
;
015,0,Electrical Supply
015,1,Terminal 30,SW
015,2,Not Used
015,3,unknown
015,4,Terminal 58D,Term 30 SW status
;
016,0,*This measuring block returns an error message.
;
017,0,Unknown
;
017,2,Not Used
017,3,Not Used
017,4,Not Used
;
018,0,Control Module Temperatures
; REMARK - need to get full width text from VAS 5052
018,1,J528 Module,temperature
018,2,Rear module,temperature
018,3,Door switch,for front E459
018,4,Rear door switch,number 2 E456
;
019,0,*Next measuring block used is 025
;
025,0,Unknown
;
025,2,Not Used
025,3,Not Used
025,4,Not Used
;
026,0,*Next measuring block used is 032
;
032,0,Ultrasonic Interior Monitoring
;
033,0,Ultrasonic sensors for anti-theft warning (Cabin Monitoring)
; REMARK - need to get full width text from VAS 5052
033,1,G209 Ultrasonsic,Security Sensor,active
033,2,G209 Ultrasonsic,Security Sensor,disabled
033,3,Not Used
033,4,Not Used
;
034,0,Ultrasonic sensors for anti-theft warning (Cabin Monitoring)
; REMARK - need to get full width text from VAS 5052
034,1,
034,2,
034,3,
034,4,
;
035,0,Unknown Counts
;
036,0,*Next measuring block used is 048
;
048,0,Unknown - Status Messages (On-Off)
;
049,0,Unknown - Status Messages (On-Off)
;
050,0,Unknown - Status Messages (On-Off)
;
051,0,Unknown - Status Messages (On-Off)
;
052,0,Unknown - Status Messages (On-Off)
;
053,0,*Next measuring block used is 080
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,*Block 80 is the last block used by this controller.
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Phaeton Roof Electronics (J528) Coding - Refer to production code sticker in spare tire well
C01,xxxxx?? - Sum up all the applicable codes to get the correct number
C02,
C03,+00 - Solar reflecting safety glass on cabin windows (4KV, NOT 4KC!)
C04,+01 - Automatic headlight control (tunnel symbol on light switch 8K7 or 8K9)
C05,+02 - Inside rear view mirror with memory capability (motorized interior mirror 4L9)
C06,+04 - Cabin interior anti-theft monitoring (7AL)
C07,+08 - Standard glass sunroof (without solar electrical generating panels 3FE)
C08,+16 - Solar power generating glass sunroof (3FR)
C09,+24 - Heat insulating glass on cabin windows (Production Code 4KC - NOT 4KV!)
C10,+32 - No sunroof at all (solid steel roof 3FA)
;
;REMARK: Do not confuse 4KC (warmeschutzglas) with 4KV (infrared glass). Add 24 to the code
;        only if the car is NOT equipped with infrared reflecting glass.
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
;Remark: Channels 11, 12, 13 are used, but the function of these is unknown.
;No other channels are used.
;
;Channel 11 value = 58474
;Channel 12 value = 8824
;Channel 13 value = 13520
;
;Above values taken from a 2004 W12 North American Phaeton.
;
;
;
