;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; Audi TT Coupe/Roadster (8N)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 8N?-920-9??-??
;
; includes measuring blocks, adaptation, coding, login and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8N-17.LBL
; 8Nx-919-xxx-17.LBL (             >> 8N-Y-050 000)
; 8Nx-920-xxx-17.LBL (8N-Y-050 001 >>             )
;
; created on 24/Feb/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 22/Apr/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Outside,Temperature
;
003,0,General
003,1,Coolant,Temperature
003,2,Standing Time
003,3,Dimming Signal,(Terminal 58d)
003,4,Dimming Signal,(Terminal 58s)
;
010,0,Adaptation Channels 30 && 09
010,1,Adaptation,Channel
010,2,Fuel Gauge,Sender 1,See Adaptation Channel 30
010,3,Adaptation,Channel
010,4,Mileage,,See Adaptation Channel 09
;
011,0,Adaptation Channels 04 && 03
011,1,Adaptation,Channel
011,2,Language,,See Adaptation Channel 04
011,3,Adaptation,Channel
011,4,Consumption,Correction,See Adaptation Channel 03
;
012,0,Adaptation Channels 40 && 41
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 40
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 41
;
013,0,Adaptation Channels 42 && 43
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 42
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 43
;
014,0,Adaptation Channel 44
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 44
;
015,0,Adaptation Channels 45 && 46
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 45
015,3,Adaptation,Channel
015,4,Total,Consumption,See Adaptation Channel 46
;
020,0,Immobilizer (ID Block 1)
020,1,Digit 1 && 2
020,2,Digit 3 && 4
020,3,Digit 5 && 6
020,4,Digit 7 && 8
;
021,0,Immobilizer (ID Block 2)
021,1,Digit 9 && 10
021,2,Digit 11 && 12
021,3,Digit 13 && 14
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...4
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)
; 4 - New Customer Service / Delivery Condition (Replacement Instrument Cluster)
; 5 - Customer Service locked / Adaptation Data Programmed in Customer Service
; 6 - Immobilizer adapted / Normal Function Condition
; 7 - Key Adaptation active
;
024,0,Immobilizer III
024,1,Lock-Time,Instrument Cluster
024,2,Lock-Time,Engine (ECU)
024,3,Lock-Time,Emergency Unlock
024,4,Lock-Time,Transponder
;
025,0,Immobilizer IV (Communication)
025,1,Immobilizer,Communication,0 = No Communication\n1 = via CAN-Databus\n2 = via W-Line
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Specification: Engine 1\nRange: Engine 0/Engine 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+01 = All-Wheel-Drive (AWD) / Quattro (Extended Fuel Tank)
C03,+02 = Seatbelt Warning active
C04,+04 = Manual Transmission (02M)
C05,+16 = Secondary Display (Radio/Navigation - w/o CAN-Databus Display)
C06,xx?xx: Country
C07,0 = Germany (D) / 1 = Rest of World (RoW - Left-Hand-Drive)
C08,2 = United States of America (USA) / 3 = Canada (CA)
C09,4 = Great Britain (GB) / 5 = Japan (JP - Left-Hand-Drive)
C10,6 = Saudi Arabia (SA) / 7 = Australia (AUS)
C11,8 = Rest of World (Right-Hand-Drive) / 9 = Japan (JP - Right-Hand-Drive)
C12,xxx?x: Engine/Cylinders
C13,4 = 4-Cylinder Engine
C14,6 = 6-Cylinder Engine
C15,xxxx?: Engine Type
C16,2 = Gasoline Engine
C17,4 = Turbo Charged Engine
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
L02, 
L03,Prior to Key Learning or adapting a used replacement
L04,Instrument Cluster the Vehicle specific PIN/SKC (Login)
L05,of the replacement Instrument Cluster has to be used
L06,to enable the adaptation.
L07,You'll find the PIN/SKC on the Key Tag of the additional
L08,Key (of the Donor Car) or you can acquire it through your
L09,responsible Distribution Center or Importer.
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 00000 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 5 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
A009,11, 
A009,12,NOTE: Perform Login first.
;
A019,0,Additional Features
A019,5,Additional Features
A019,6,?xxxx: Illumination
A019,7,0 = Needle and Scale only active at "Light ON"
A019,8,1 = Needle already active at "Ignition ON"
A019,9,2 = Scale already active at "Ignition ON"
A019,10,3 = Scale (2nd Map) and Needle at "Ignition ON" active
A019,11, 
A019,12,xxx?x - Outside Temperature
A019,13,0 - not active / 1 - active
A019,14, 
A019,15,xxxx? - Remote Clock
A019,16,0 - not active / 1 - clock active
;
A021,0,Immobilizer - Key Adaptation
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This is a parallel shift of the tank characteristic.
A030,7, 
A030,8,Standard: 128
A030,9,Range: 96...160 (-8.0...+8.0 l)
A030,10,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Resolution: 1 = 100 km
A040,7, 
A040,8,NOTE: Adaptation channels 40-46 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Resolution: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-46 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 1000 km/mi
A042,7,00015 = Standard (15.000 km)
A042,8,or (if coded to miles)
A042,9,00010 = Standard (10.000 mi)
A042,10, 
A042,11,NOTE: Adaptation channels 40-46 must be
A042,12,entered and stored in the following order:
A042,13,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 1000 km/mi
A043,7,00015 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,00030 = flexible Service Intervals (30.000 km - with Longlife)
A043,9,or (if coded to miles)
A043,10,00010 = fixed Service Intervals (10.000 mi - USA - w/o Longlife)
A043,11,00019 = Gasoline Engines with flexible Service Intervals (19.000 mi - with Longlife)
A043,12, 
A043,13,NOTE: Adaptation channels 40-46 must be
A043,14,entered and stored in the following order:
A043,15,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-46 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
A045,8, 
A045,9,NOTE: Adaptation channels 40-46 must be
A045,10,entered and stored in the following order:
A045,11,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display.
A046,8, 
A046,9,NOTE: Adaptation channels 40-46 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 44 > 40 > 41 > 46
;
A050,0,Immobilizer - Vehicle Data Learning
A050,5,Immobilizer - Vehicle Data Learning
;
A060,0,CAN-Databus Powertrain (Installation List)
A060,5,CAN-Databus Powertrain (Installation List)
A060,6,00000 = Engine and Instrument Cluster (IMMO-II)
A060,7,01025 = Engine and Instrument Cluster (IMMO-III)
A060,8,01027 = Engine and Auto. Transm. and Instrument Cluster (IMMO-III)
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,1000,DIST
RD,43,Max Mileage to Service,1000,DIST
RD,44,Max Time to Service,1,Days
RD,45,Oil Quality,1,
RD,46,Total Consumption,100,DIST
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Change to Fixed Intervals (Kilometers),,ST_FIXED
RJ,1,1,45,1
RJ,1,2,42,15
RJ,1,3,43,15
RJ,1,4,44,365
;
; Change to flexible intervals (kilometers)
RJ,2,0,Change to Flexible Intervals (Kilometers),,ST_FLEXIBLE
RJ,2,1,45,2
RJ,2,2,42,15
RJ,2,3,43,30
RJ,2,4,44,730
;
; Change to fixed intervals (miles)
RJ,3,0,Change to Fixed Intervals (Miles),,ST_FIXED
RJ,3,1,45,1
RJ,3,2,42,10
RJ,3,3,43,10
RJ,3,4,44,365
;
; Change to flexible intervals (miles)
RJ,4,0,Change to Flexible Intervals (Miles),,ST_FLEXIBLE
RJ,4,1,45,2
RJ,4,2,42,10
RJ,4,3,43,19
RJ,4,4,44,730
;
