;
; VCDS Label File
;
; Copyright © 2010 Ross-Tech, LLC
;
; VW Fox (5Z)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 5Z0-920-???-???
;
; includes measuring blocks, adaptation, coding and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 5Z-17.LBL
; 5Z0-920-xxx-17.LBL
;
; created on 11/Aug/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 05/Dec/2010
;
; requires VCDS 10.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...4
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)\n\n1 = End of Assembly Line: NEW (Delivery Condition of New Instrument Cluster)\n2 = End of Assembly Line: VIN adapted\n3 = End of Assembly Line: ECU adapted\n4 = Customer Service: NEW (Delivery Condition of Replacement Instrument Cluster)\n5 = Customer Service: Instrument Cluster adapted\n6 = Customer Service: Keys adapted (Normal Condition)\n7 = Customer Service: Key Adaptation active
;
024,0,Immobilizer III (Lock Time)
024,1,Lock-Time,Instrument Cluster
024,2,Lock-Time,Engine (ECU)
024,3,Lock-Time,Emergency Unlock
024,4,Lock-Time,Transponder
;
025,0,Immobilizer IV (Communication)
025,1,Immobilizer,Communication,0 = No Communication\n1 = via CAN-Databus\n2 = via W-Line
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Range: Engine 0/Engine 1\nSpecification: Engine 1
125,3,Brake Electronics,(J104),Range: ABS 0/ABS 1\nSpecification: ABS 1
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Airbags,(J234),Range: Airbag 0/Airbag 1\nSpecification: Airbag 1
126,3,Steering Aid,(J500),Range: Steering 1/Steering 0\nSpecification: Steering 1
;
225,0,CAN-Databus TimeOut (Powertrain)
225,1,Engine
225,3,Brake Electronics,(J104)
;
226,0,CAN-Databus Kommunikation (Powertrain)
226,2,Airbags,(J234)
226,3,Steering Aid,(J500)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Equipment
C02,00 = No Additional Equipment
C03,02 = Seatbelt Warning installed
C04,x?xxx: Country
C05,0 = Germany (DE)
C06,1 = Europe (EU)
C07,4 = Great Britain (GB)
C08,xxx?x: Engine
C09,3 = 3-Cylinder Motor
C10,4 = 4-Cylinder Motor
C11,xxxx?: Distance Impulse Number
C12,1 = Tires 155/80 R13
C13,1 = Tires 185/60 R14
C14,2 = Tires 165/70 R14
C15, 
C16,Note: Seatbelt Warning cannot be deactivated in all cases.
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,7, 
A009,8,The distance can only be changed once until
A009,9,the current value is not over 100 km/62 mi.
;
A021,0,Immobilizer (Key Adaptation)
A021,3,Key Count
A021,5,Immobilizer (Key Adaptation)
A021,6,Prior to Adapting new Keys the Adaptation has to be enabled by
A021,7,logging in using the Immobilizer PIN/SKC. The Adaptation Value
A021,8,is the number of all Keys to be adapted (Maximum 8).
A021,9,After Saving the Adaptation Value the first Key is adapted.
A021,10,Proceed until all Keys are adapted:
A021,11,- Switch the Ingnition OFF and take out the Key.
A021,12,- Switch the Ignition ON using the next Key.
A021,13,- The Immobilizer Lamp should light up for 2 Seconds and then switch OFF.
A021,14,- The Key is now adapted.
;
;A025,0,
; 
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 9 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 108...148 (-5.0...+5.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
A035,9, 
A035,10,Standard: 0
A035,11,Range: 0...1000 U/min
A035,12,Increments: 250 U/min
;
A050,0,Immobilizer (Vehicle Data learning)
A050,1,Status
A050,5,Immobilizer (Vehicle Data learning)
A050,6,Please enter the Immobilizer PIN/SKC of the Engine Control Module (OLD PIN/SKC).
A050,7,After that the Learning Process is being initiated the new Immobilizer Control
A050,8,Module adopts the Vehicle-Identification-Number (VIN) and Immobilizer
A050,9,Identification (IMMO-ID) of the Vehicle (from the OLD Engine Control Module).
A050,10,Once the Adaptation is done switch the Ignition OFF for about 2 Minutes.
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RM,0,Service Reset not possible!
RM,1,The Service Idicator can only be reset manually on this vehicle.
RM,2,To Reset the Service Idicator follow these steps:
RM,3,Press/hold the Button right next to the Speedometer while the Ignition is switched OFF.
RM,4,Now switch the Ignition ONS and keep holding the Button for an additional 10 Seconds.
RM,5,Service should now be Reset. Verify if the Service Message disappeared by Cycling the Ignition.
;
