;
; VCDS Label File
;
; Copyright © 2010-2011 Ross-Tech, LLC
;
; Audi A4 (8D)
;
; Component: J220 - Engine (#01) - AFC (2.8l 12V)
;
; P/N: 8D0-906-266-?
;
; See special notes on this Ecu:
;
; http://www.ross-tech.com/vag-com/audi_issues.html#HitachiOBD2
;
; Readiness Status via Generic OBD-2 (Binary Data in MVB 029)
;
; created on 01/Dec/2010 by Dana Smetanick (Dana@Ross-Tech.com)
; updated on 28/Jan/2011 by Dana Smetanick (Dana@Ross-Tech.com) / added Coding
; updated on 31/Jan/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; requires VCDS 10.6.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Note: Only run one group at a time on this ECU
001,1,Engine Coolant, temperature, ECT (G62)
001,2,MAF sensor, output voltage 
001,3,Altitude, only w/SAI
001,4,ECM voltage
;
002,0,Throttle position sensor
002,1,TPS (G69) Coarse, Idle to WOT range, Specification: 0.250...4.750 V 
002,2,TPS (G69) Fine, Idle && Lower, Partial throttle range: 0.250...1.275 V
002,3,TPS (G69),Learning value, Specification: 0.250...0.500 V
002,4,Closed Throttle, switch (F60), Specification: Open = 0 Closed = 1
;
003,0,Note: Only run one group at a time on this ECU
003,1,Engine speed, (RPM)
003,2,Engine load
003,3,Throttle angle
003,4,Vehicle speed
;
004,0,IAC && ASC Learning
004,1,Idle Air Control, valve (IAC)
004,2,Idle Speed, Control learning
004,3,Idle Speed, Control learning
;
005,0,Oxygen Sensor Learning Bank 1
005,1,O2s Learning,at Idle
005,2,O2s Learning,Part Throttle I
005,3,O2s Learning,Part Throttle II
005,4,O2s Learning,Part Throttle III
;
006,0,Oxygen Sensor Learning  Bank 2
006,1,O2s Learning,at Idle
006,2,O2s Learning,Part Throttle I
006,3,O2s Learning,Part Throttle II
006,4,O2s Learning,Part Throttle III
;
007,0,Oxygen Sensor Control Bank 1
007,1,O2s Control,, Specification: 0.0 +/- 6.0 %
007,2,O2s Learning, Range
007,3,O2s Learning, Diagnosis
007,4,O2s Learning, Display
;
008,0,Oxygen Sensor Control Bank 2
008,1,O2s Control,, Specification: 0.0 +/- 6.0 %,
008,2,O2s Learning, Range
008,3,O2s Learning, Diagnosis
008,4,O2s Learning, Display
;
009,0,Note: Only run one group at a time on this ECU
009,1,O2s Control, Bank 1
009,2,O2s Control, Bank 2
009,3,Evap Sol.(N80), Duty Cycle
009,4,Throttle angle
;
010,0,Oxygen Sensor
010,1,O2s Control, Bank 1, and momentary O2s learning value
010,2,O2s Control, Bank 2, and momentary O2s learning value
010,3,Heated O2s, Bank 1, control Voltage
010,4,Heated O2s, Bank 2, control Voltage
;
011,1,Ignition Timing,, w/o knock or idle speed control
011,2,Ignition Timing,, with knock and idle speed control
011,3,Ignition Timing, Access to ISC, Idle Speed Control
011,4,Closed Throttle, Position switch 
;
012,0,Note: Only run one group at a time on this ECU
012,1,Engine Speed
012,2,Engine Load
012,3,Ignition Timing,Map switching
012,4,Ignition Timing,,Retarded by knock control
;
013,0,Ignition Timing
013,1,Ignition Timing,Map switching
013,2,Ignition Timing,Cylinder 1, retarded by knock control
013,3,Ignition Timing,Cylinder 2, retarded by knock control
013,4,Ignition Timing,Cylinder 3, retarded by knock control
;
014,0,Ignition Timing
014,1,Ignition Timing,Map switching
014,2,Ignition Timing,Cylinder 4, retarded by knock control
014,3,Ignition Timing,Cylinder 5, retarded by knock control
014,4,Ignition Timing,Cylinder 6, retarded by knock control
;
015,1,Engine Speed 
015,2,Knock Sensor,Cylinder 1
015,3,Knock Sensor,Cylinder 2
015,4,Knock Sensor,Cylinder 3
;
016,1,Engine Speed
016,2,Knock Sensor,Cylinder 4
016,3,Knock Sensor,Cylinder 5
016,4,Knock Sensor,Cylinder 6
;
017,0,Note: Only run one group at a time on this ECU
017,1,Timer 1
017,2,Timer 2
017,3,Engine load
017,4,EGR temperature 
;
018,0,Idle Air Control
018,1,Specified IAC, Duty Cycle
018,2,Current Draw, IAC valve (N71)
018,3,Power Control, IAC valve (N71)
018,4,ECM Voltage, supply
;
019,0,Note: Only run one group at a time on this ECU
019,1,Engine Power
019,2,Intake Air, volume
019,3,Vehicle Speed
019,4,Fuel Injection, time
;
020,0,Secondary Air Injection (If Applicable)
;
021,0,Secondary Air Injection (If Applicable)
;
022,0,Traction control (If Applicable)
;
023,0,Note: Only run one group at a time on this ECU
;
027,0,Fuel level display
;
028,0,Note: Only run one group at a time on this ECU
;
029,0,Readiness Diagnostic Status *Note: Use generic OBD-2
029,1,Readiness code,,000x00x0 is passed \ "x" = N/A
029,2,Trip status, display
;
030,0,Evap System with Pressure Sensor (G172)
;
031,0,Misfire Recognition operating conditions
;
032,0,Bank 1 O2s
;
033,0,Bank 2 O2s
;
034,0,O2s
;
035,0,Three way catalytic convertor diagnosis, Bank 1
;
036,0,Three way catalytic convertor diagnosis, Bank 2
;
037,0,Sensor wheel learning
;
038,0,Misfire Recognition current
;
039,0,Misfire Recognition statistical
;
040,0,HO2s current front and rear
;
041,0,HO2s voltage front and rear
;
042,0,Diagnostic conditions for front O2s response time
;
043,0,Current conditions for front O2S response time
;
044,0,Diagnostic conditions for catalytic convertor
;
045,0,EVAP system tank diagnosis
;
046,0,Next Valid Group is 99
;
099,0,Note: Only run one group at a time on this ECU
099,1,Engine speed
099,2,Engine load
099,3,ECT Coolant,Temperature 
099,4,O2s Control,On/Off
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine Electronics (J220) Coding
C01,??xxx: Country/Emission
C02,01 = Exhaust Gas Recirculation and Evaporative Emissions Sensor (G172)
C03,10 = Exhaust Gas Recirculation / Evaporative Emissions Sensor (G172) and Secondary Air Injection (SAI)
C04,xx?xx: Drive/Additional Functions
C05,0 = Front-Wheel-Drive w/o Traction Control (ASR)
C06,1 = Front-Wheel-Drive with Traction Control (ASR)
C07,2 = All-Wheel-Drive w/o Traction Control (ASR)
C08,xxx?x: Transmission
C09,0 = 5-Speed Manual Transmission
C10,3 = 4 Speed Automatic Transmission (01N)
C11,4 = 4 Speed Automatic Transmission (01F/01K - HP-18)
C12,5 = 5 Speed Automatic Transmission (01V)
C13,xxxx?: Vehicle Type
C14,1 = B-Class (e.g. Audi A4)
C15,2 = C-Class (e.g. Audi A6)
C16,4 = Special (e.g. Audi Cabriolet)
;
