;
; VCDS Label File
;
; Copyright © 2008 Ross-Tech, LLC
;
; VW Touareg (7L6)
;
; Component: J502 - Tire Pressure Monitoring (#65)
;
; P/N: 7L6-907-273-???
;
; includes measuring blocks and long coding
;
; created on 14/Feb/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 26/Jul/2008
;
; requires VCDS 805.0 / LCode 807.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Front Left Wheel Status I
001,1,Wheel Sensor,Position
001,2,Wheel,Temperature,Range: -50.0...+125.0 °C
001,3,Wheel Pressure,(actual),Range: 0.0...5.5 bar
001,4,Wheel Pressure,(specified),Range: 1.3...5.5 bar
;
002,0,Front Left Wheel Status II
002,1,Wheel Sensor,Position / Identification / Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
;
003,0,Front Right Wheel Status I
003,1,Wheel Sensor,Position
003,2,Wheel,Temperature,Range: -50.0...+125.0 °C
003,3,Wheel Pressure,(actual),Range: 0.0...5.5 bar
003,4,Wheel Pressure,(specified),Range: 1.3...5.5 bar
;
004,0,Front Right Wheel Status II
004,1,Wheel Sensor,Position / Identification / Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
;
005,0,Rear Left Wheel Status I
005,1,Wheel Sensor,Position
005,2,Wheel,Temperature,Range: -50.0...+125.0 °C
005,3,Wheel Pressure,(actual),Range: 0.0...5.5 bar
005,4,Wheel Pressure,(specified),Range: 1.3...5.5 bar
;
006,0,Rear Left Wheel Status II
006,1,Wheel Sensor,Position / Identification / Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
;
007,0,Rear Right Wheel Status I
007,1,Wheel Sensor,Position
007,2,Wheel,Temperature,Range: -50.0...+125.0 °C
007,3,Wheel Pressure,(actual),Range: 0.0...5.5 bar
007,4,Wheel Pressure,(specified),Range: 1.3...5.5 bar
;
008,0,Rear Right Wheel Status II
008,1,Wheel Sensor,Position / Identification / Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
;
016,0,Wheel Sensor Status (from last Received Wheel ID) I
016,1,Wheel Sensor,Identification / Status / Pressure
;
017,1,Ambient,Temperature
;
019,0,Monitored Pressure
019,1,Monitored Pressure,Front / Partial Load
019,2,Monitored Pressure,Front / Full Load
019,3,Monitored Pressure,Rear / Partial Load
019,4,Monitored Pressure,Rear / Full Load
;
020,0,Specified Pressure 1
020,1,Spec. Pressure 1,Front / Partial Load
020,2,Spec. Pressure 1,Front / Full Load
020,3,Spec. Pressure 1,Rear / Partial Load
020,4,Spec. Pressure 1,Rear / Full Load
;
021,0,Specified Pressure 2
021,1,Spec. Pressure 2,Front / Partial Load
021,2,Spec. Pressure 2,Front / Full Load
021,3,Spec. Pressure 2,Rear / Partial Load
021,4,Spec. Pressure 2,Rear / Full Load
;
022,0,Specified Pressure 3
022,1,Spec. Pressure 3,Front / Partial Load
022,2,Spec. Pressure 3,Front / Full Load
022,3,Spec. Pressure 3,Rear / Partial Load
022,4,Spec. Pressure 3,Rear / Full Load
;
023,0,Specified Pressure 4
023,1,Spec. Pressure 4,Front / Partial Load
023,2,Spec. Pressure 4,Front / Full Load
023,3,Spec. Pressure 4,Rear / Partial Load
023,4,Spec. Pressure 4,Rear / Full Load
;
024,0,Specified Pressure 5
024,1,Spec. Pressure 5,Front / Partial Load
024,2,Spec. Pressure 5,Front / Full Load
024,3,Spec. Pressure 5,Rear / Partial Load
024,4,Spec. Pressure 5,Rear / Full Load
;
025,0,Specified Pressure 6
025,1,Spec. Pressure 6,Front / Partial Load
025,2,Spec. Pressure 6,Front / Full Load
025,3,Spec. Pressure 6,Rear / Partial Load
025,4,Spec. Pressure 6,Rear / Full Load
;
030,0,CAN-Databus Communication
030,1,Status,Terminal 15,Range: Term 15 On/Term 15 Off
030,2,Engine Speed
030,3,Vehicle Speed
030,4,Ambient,Temperature
;
031,0,CAN-Databus Communication
031,1,Voltage,(Terminal 30)
031,2,CAN-Gateway,(J533),Range: Gateway 1/Gateway 0
031,4,Access/Start,Authorization,Specification: El.Ign.Lock 1\nRange: El.Ign.Lock 1/El.Ign.Lock 0
;
032,0,Transport Mode
032,1,Transport Mode,,Range: Yes/No
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,0,Automatic Activation active/coded
LC,00,1,Automatic Deactivation active/coded
LC,00,2,De-/Activation via Menu active/coded
LC,00,3,Message after Wheel Change active/coded
LC,00,4,Soft Warning Output immediate
LC,00,5,Soft Warning active/coded
LC,00,6,Minimum Pressure 1.4 bar rel.
LC,00,7,Carrier Frequency 315 MHz
LC,01,0~0,00,Malfunction Lamp Type "Blinking Light"
LC,01,0~0,01,Malfunction Lamp Type "Continuous Light"
; Byte 01 Bit 1 unused
; Byte 01 Bit 2 unused
LC,01,3,Full/Partial Load via Menu switchable
LC,01,4,Specified Pressure Temperature Evaluation active
LC,01,5,Specified Pressures coded
LC,01,6,Actual Pressures coded
LC,01,7,Actual Temperatures coded
;
; {Byte 02 unused}
;
; {Specified Pressure 1 Rear Axle Partial Load}
LC,03,0~3,00,Specified Pressure 1 Rear Axle Partial Load 0.0 bar
LC,03,0~3,01,Specified Pressure 1 Rear Axle Partial Load 2.0 bar
LC,03,0~3,02,Specified Pressure 1 Rear Axle Partial Load 2.1 bar
LC,03,0~3,03,Specified Pressure 1 Rear Axle Partial Load 2.2 bar
LC,03,0~3,04,Specified Pressure 1 Rear Axle Partial Load 2.3 bar
LC,03,0~3,05,Specified Pressure 1 Rear Axle Partial Load 2.4 bar
LC,03,0~3,06,Specified Pressure 1 Rear Axle Partial Load 2.5 bar
LC,03,0~3,07,Specified Pressure 1 Rear Axle Partial Load 2.6 bar
LC,03,0~3,08,Specified Pressure 1 Rear Axle Partial Load 2.7 bar
LC,03,0~3,09,Specified Pressure 1 Rear Axle Partial Load 2.8 bar
LC,03,0~3,0A,Specified Pressure 1 Rear Axle Partial Load 2.9 bar
LC,03,0~3,0B,Specified Pressure 1 Rear Axle Partial Load 3.0 bar
LC,03,0~3,0C,Specified Pressure 1 Rear Axle Partial Load 3.1 bar
LC,03,0~3,0D,Specified Pressure 1 Rear Axle Partial Load 3.2 bar
LC,03,0~3,0E,Specified Pressure 1 Rear Axle Partial Load 3.3 bar
LC,03,0~3,0F,Specified Pressure 1 Rear Axle Partial Load 3.4 bar
; {Specified Pressure 1 Front Axle Partial Load}
LC,03,4~7,00,Specified Pressure 1 Front Axle Partial Load 0.0 bar
LC,03,4~7,10,Specified Pressure 1 Front Axle Partial Load 2.0 bar
LC,03,4~7,20,Specified Pressure 1 Front Axle Partial Load 2.1 bar
LC,03,4~7,30,Specified Pressure 1 Front Axle Partial Load 2.2 bar
LC,03,4~7,40,Specified Pressure 1 Front Axle Partial Load 2.3 bar
LC,03,4~7,50,Specified Pressure 1 Front Axle Partial Load 2.4 bar
LC,03,4~7,60,Specified Pressure 1 Front Axle Partial Load 2.5 bar
LC,03,4~7,70,Specified Pressure 1 Front Axle Partial Load 2.6 bar
LC,03,4~7,80,Specified Pressure 1 Front Axle Partial Load 2.7 bar
LC,03,4~7,90,Specified Pressure 1 Front Axle Partial Load 2.8 bar
LC,03,4~7,A0,Specified Pressure 1 Front Axle Partial Load 2.9 bar
LC,03,4~7,B0,Specified Pressure 1 Front Axle Partial Load 3.0 bar
LC,03,4~7,C0,Specified Pressure 1 Front Axle Partial Load 3.1 bar
LC,03,4~7,D0,Specified Pressure 1 Front Axle Partial Load 3.2 bar
LC,03,4~7,E0,Specified Pressure 1 Front Axle Partial Load 3.3 bar
LC,03,4~7,F0,Specified Pressure 1 Front Axle Partial Load 3.4 bar
;
; {Specified Pressure 1 Rear Axle Full Load}
LC,04,0~3,00,Specified Pressure 1 Rear Axle Full Load 0.0 bar
LC,04,0~3,01,Specified Pressure 1 Rear Axle Full Load 2.0 bar
LC,04,0~3,02,Specified Pressure 1 Rear Axle Full Load 2.1 bar
LC,04,0~3,03,Specified Pressure 1 Rear Axle Full Load 2.2 bar
LC,04,0~3,04,Specified Pressure 1 Rear Axle Full Load 2.3 bar
LC,04,0~3,05,Specified Pressure 1 Rear Axle Full Load 2.4 bar
LC,04,0~3,06,Specified Pressure 1 Rear Axle Full Load 2.5 bar
LC,04,0~3,07,Specified Pressure 1 Rear Axle Full Load 2.6 bar
LC,04,0~3,08,Specified Pressure 1 Rear Axle Full Load 2.7 bar
LC,04,0~3,09,Specified Pressure 1 Rear Axle Full Load 2.8 bar
LC,04,0~3,0A,Specified Pressure 1 Rear Axle Full Load 2.9 bar
LC,04,0~3,0B,Specified Pressure 1 Rear Axle Full Load 3.0 bar
LC,04,0~3,0C,Specified Pressure 1 Rear Axle Full Load 3.1 bar
LC,04,0~3,0D,Specified Pressure 1 Rear Axle Full Load 3.2 bar
LC,04,0~3,0E,Specified Pressure 1 Rear Axle Full Load 3.3 bar
LC,04,0~3,0F,Specified Pressure 1 Rear Axle Full Load 3.4 bar
; {Specified Pressure 1 Front Axle Full Load}
LC,04,4~7,00,Specified Pressure 1 Front Axle Full Load 0.0 bar
LC,04,4~7,10,Specified Pressure 1 Front Axle Full Load 2.0 bar
LC,04,4~7,20,Specified Pressure 1 Front Axle Full Load 2.1 bar
LC,04,4~7,30,Specified Pressure 1 Front Axle Full Load 2.2 bar
LC,04,4~7,40,Specified Pressure 1 Front Axle Full Load 2.3 bar
LC,04,4~7,50,Specified Pressure 1 Front Axle Full Load 2.4 bar
LC,04,4~7,60,Specified Pressure 1 Front Axle Full Load 2.5 bar
LC,04,4~7,70,Specified Pressure 1 Front Axle Full Load 2.6 bar
LC,04,4~7,80,Specified Pressure 1 Front Axle Full Load 2.7 bar
LC,04,4~7,90,Specified Pressure 1 Front Axle Full Load 2.8 bar
LC,04,4~7,A0,Specified Pressure 1 Front Axle Full Load 2.9 bar
LC,04,4~7,B0,Specified Pressure 1 Front Axle Full Load 3.0 bar
LC,04,4~7,C0,Specified Pressure 1 Front Axle Full Load 3.1 bar
LC,04,4~7,D0,Specified Pressure 1 Front Axle Full Load 3.2 bar
LC,04,4~7,E0,Specified Pressure 1 Front Axle Full Load 3.3 bar
LC,04,4~7,F0,Specified Pressure 1 Front Axle Full Load 3.4 bar
;
; {Specified Pressure 2 Rear Axle Partial Load}
LC,05,0~3,00,Specified Pressure 2 Rear Axle Partial Load 0.0 bar
LC,05,0~3,01,Specified Pressure 2 Rear Axle Partial Load 2.0 bar
LC,05,0~3,02,Specified Pressure 2 Rear Axle Partial Load 2.1 bar
LC,05,0~3,03,Specified Pressure 2 Rear Axle Partial Load 2.2 bar
LC,05,0~3,04,Specified Pressure 2 Rear Axle Partial Load 2.3 bar
LC,05,0~3,05,Specified Pressure 2 Rear Axle Partial Load 2.4 bar
LC,05,0~3,06,Specified Pressure 2 Rear Axle Partial Load 2.5 bar
LC,05,0~3,07,Specified Pressure 2 Rear Axle Partial Load 2.6 bar
LC,05,0~3,08,Specified Pressure 2 Rear Axle Partial Load 2.7 bar
LC,05,0~3,09,Specified Pressure 2 Rear Axle Partial Load 2.8 bar
LC,05,0~3,0A,Specified Pressure 2 Rear Axle Partial Load 2.9 bar
LC,05,0~3,0B,Specified Pressure 2 Rear Axle Partial Load 3.0 bar
LC,05,0~3,0C,Specified Pressure 2 Rear Axle Partial Load 3.1 bar
LC,05,0~3,0D,Specified Pressure 2 Rear Axle Partial Load 3.2 bar
LC,05,0~3,0E,Specified Pressure 2 Rear Axle Partial Load 3.3 bar
LC,05,0~3,0F,Specified Pressure 2 Rear Axle Partial Load 3.4 bar
; {Specified Pressure 2 Front Axle Partial Load}
LC,05,4~7,00,Specified Pressure 2 Front Axle Partial Load 0.0 bar
LC,05,4~7,10,Specified Pressure 2 Front Axle Partial Load 2.0 bar
LC,05,4~7,20,Specified Pressure 2 Front Axle Partial Load 2.1 bar
LC,05,4~7,30,Specified Pressure 2 Front Axle Partial Load 2.2 bar
LC,05,4~7,40,Specified Pressure 2 Front Axle Partial Load 2.3 bar
LC,05,4~7,50,Specified Pressure 2 Front Axle Partial Load 2.4 bar
LC,05,4~7,60,Specified Pressure 2 Front Axle Partial Load 2.5 bar
LC,05,4~7,70,Specified Pressure 2 Front Axle Partial Load 2.6 bar
LC,05,4~7,80,Specified Pressure 2 Front Axle Partial Load 2.7 bar
LC,05,4~7,90,Specified Pressure 2 Front Axle Partial Load 2.8 bar
LC,05,4~7,A0,Specified Pressure 2 Front Axle Partial Load 2.9 bar
LC,05,4~7,B0,Specified Pressure 2 Front Axle Partial Load 3.0 bar
LC,05,4~7,C0,Specified Pressure 2 Front Axle Partial Load 3.1 bar
LC,05,4~7,D0,Specified Pressure 2 Front Axle Partial Load 3.2 bar
LC,05,4~7,E0,Specified Pressure 2 Front Axle Partial Load 3.3 bar
LC,05,4~7,F0,Specified Pressure 2 Front Axle Partial Load 3.4 bar
;
; {Specified Pressure 2 Rear Axle Full Load}
LC,06,0~3,00,Specified Pressure 2 Rear Axle Full Load 0.0 bar
LC,06,0~3,01,Specified Pressure 2 Rear Axle Full Load 2.0 bar
LC,06,0~3,02,Specified Pressure 2 Rear Axle Full Load 2.1 bar
LC,06,0~3,03,Specified Pressure 2 Rear Axle Full Load 2.2 bar
LC,06,0~3,04,Specified Pressure 2 Rear Axle Full Load 2.3 bar
LC,06,0~3,05,Specified Pressure 2 Rear Axle Full Load 2.4 bar
LC,06,0~3,06,Specified Pressure 2 Rear Axle Full Load 2.5 bar
LC,06,0~3,07,Specified Pressure 2 Rear Axle Full Load 2.6 bar
LC,06,0~3,08,Specified Pressure 2 Rear Axle Full Load 2.7 bar
LC,06,0~3,09,Specified Pressure 2 Rear Axle Full Load 2.8 bar
LC,06,0~3,0A,Specified Pressure 2 Rear Axle Full Load 2.9 bar
LC,06,0~3,0B,Specified Pressure 2 Rear Axle Full Load 3.0 bar
LC,06,0~3,0C,Specified Pressure 2 Rear Axle Full Load 3.1 bar
LC,06,0~3,0D,Specified Pressure 2 Rear Axle Full Load 3.2 bar
LC,06,0~3,0E,Specified Pressure 2 Rear Axle Full Load 3.3 bar
LC,06,0~3,0F,Specified Pressure 2 Rear Axle Full Load 3.4 bar
; {Specified Pressure 2 Front Axle Full Load}
LC,06,4~7,00,Specified Pressure 2 Front Axle Full Load 0.0 bar
LC,06,4~7,10,Specified Pressure 2 Front Axle Full Load 2.0 bar
LC,06,4~7,20,Specified Pressure 2 Front Axle Full Load 2.1 bar
LC,06,4~7,30,Specified Pressure 2 Front Axle Full Load 2.2 bar
LC,06,4~7,40,Specified Pressure 2 Front Axle Full Load 2.3 bar
LC,06,4~7,50,Specified Pressure 2 Front Axle Full Load 2.4 bar
LC,06,4~7,60,Specified Pressure 2 Front Axle Full Load 2.5 bar
LC,06,4~7,70,Specified Pressure 2 Front Axle Full Load 2.6 bar
LC,06,4~7,80,Specified Pressure 2 Front Axle Full Load 2.7 bar
LC,06,4~7,90,Specified Pressure 2 Front Axle Full Load 2.8 bar
LC,06,4~7,A0,Specified Pressure 2 Front Axle Full Load 2.9 bar
LC,06,4~7,B0,Specified Pressure 2 Front Axle Full Load 3.0 bar
LC,06,4~7,C0,Specified Pressure 2 Front Axle Full Load 3.1 bar
LC,06,4~7,D0,Specified Pressure 2 Front Axle Full Load 3.2 bar
LC,06,4~7,E0,Specified Pressure 2 Front Axle Full Load 3.3 bar
LC,06,4~7,F0,Specified Pressure 2 Front Axle Full Load 3.4 bar
;
; {Specified Pressure 3 Rear Axle Partial Load}
LC,07,0~3,00,Specified Pressure 3 Rear Axle Partial Load 0.0 bar
LC,07,0~3,01,Specified Pressure 3 Rear Axle Partial Load 2.0 bar
LC,07,0~3,02,Specified Pressure 3 Rear Axle Partial Load 2.1 bar
LC,07,0~3,03,Specified Pressure 3 Rear Axle Partial Load 2.2 bar
LC,07,0~3,04,Specified Pressure 3 Rear Axle Partial Load 2.3 bar
LC,07,0~3,05,Specified Pressure 3 Rear Axle Partial Load 2.4 bar
LC,07,0~3,06,Specified Pressure 3 Rear Axle Partial Load 2.5 bar
LC,07,0~3,07,Specified Pressure 3 Rear Axle Partial Load 2.6 bar
LC,07,0~3,08,Specified Pressure 3 Rear Axle Partial Load 2.7 bar
LC,07,0~3,09,Specified Pressure 3 Rear Axle Partial Load 2.8 bar
LC,07,0~3,0A,Specified Pressure 3 Rear Axle Partial Load 2.9 bar
LC,07,0~3,0B,Specified Pressure 3 Rear Axle Partial Load 3.0 bar
LC,07,0~3,0C,Specified Pressure 3 Rear Axle Partial Load 3.1 bar
LC,07,0~3,0D,Specified Pressure 3 Rear Axle Partial Load 3.2 bar
LC,07,0~3,0E,Specified Pressure 3 Rear Axle Partial Load 3.3 bar
LC,07,0~3,0F,Specified Pressure 3 Rear Axle Partial Load 3.4 bar
; {Specified Pressure 3 Front Axle Partial Load}
LC,07,4~7,00,Specified Pressure 3 Front Axle Partial Load 0.0 bar
LC,07,4~7,10,Specified Pressure 3 Front Axle Partial Load 2.0 bar
LC,07,4~7,20,Specified Pressure 3 Front Axle Partial Load 2.1 bar
LC,07,4~7,30,Specified Pressure 3 Front Axle Partial Load 2.2 bar
LC,07,4~7,40,Specified Pressure 3 Front Axle Partial Load 2.3 bar
LC,07,4~7,50,Specified Pressure 3 Front Axle Partial Load 2.4 bar
LC,07,4~7,60,Specified Pressure 3 Front Axle Partial Load 2.5 bar
LC,07,4~7,70,Specified Pressure 3 Front Axle Partial Load 2.6 bar
LC,07,4~7,80,Specified Pressure 3 Front Axle Partial Load 2.7 bar
LC,07,4~7,90,Specified Pressure 3 Front Axle Partial Load 2.8 bar
LC,07,4~7,A0,Specified Pressure 3 Front Axle Partial Load 2.9 bar
LC,07,4~7,B0,Specified Pressure 3 Front Axle Partial Load 3.0 bar
LC,07,4~7,C0,Specified Pressure 3 Front Axle Partial Load 3.1 bar
LC,07,4~7,D0,Specified Pressure 3 Front Axle Partial Load 3.2 bar
LC,07,4~7,E0,Specified Pressure 3 Front Axle Partial Load 3.3 bar
LC,07,4~7,F0,Specified Pressure 3 Front Axle Partial Load 3.4 bar
;
; {Specified Pressure 3 Rear Axle Full Load}
LC,08,0~3,00,Specified Pressure 3 Rear Axle Full Load 0.0 bar
LC,08,0~3,01,Specified Pressure 3 Rear Axle Full Load 2.0 bar
LC,08,0~3,02,Specified Pressure 3 Rear Axle Full Load 2.1 bar
LC,08,0~3,03,Specified Pressure 3 Rear Axle Full Load 2.2 bar
LC,08,0~3,04,Specified Pressure 3 Rear Axle Full Load 2.3 bar
LC,08,0~3,05,Specified Pressure 3 Rear Axle Full Load 2.4 bar
LC,08,0~3,06,Specified Pressure 3 Rear Axle Full Load 2.5 bar
LC,08,0~3,07,Specified Pressure 3 Rear Axle Full Load 2.6 bar
LC,08,0~3,08,Specified Pressure 3 Rear Axle Full Load 2.7 bar
LC,08,0~3,09,Specified Pressure 3 Rear Axle Full Load 2.8 bar
LC,08,0~3,0A,Specified Pressure 3 Rear Axle Full Load 2.9 bar
LC,08,0~3,0B,Specified Pressure 3 Rear Axle Full Load 3.0 bar
LC,08,0~3,0C,Specified Pressure 3 Rear Axle Full Load 3.1 bar
LC,08,0~3,0D,Specified Pressure 3 Rear Axle Full Load 3.2 bar
LC,08,0~3,0E,Specified Pressure 3 Rear Axle Full Load 3.3 bar
LC,08,0~3,0F,Specified Pressure 3 Rear Axle Full Load 3.4 bar
; {Specified Pressure 3 Front Axle Full Load}
LC,08,4~7,00,Specified Pressure 3 Front Axle Full Load 0.0 bar
LC,08,4~7,10,Specified Pressure 3 Front Axle Full Load 2.0 bar
LC,08,4~7,20,Specified Pressure 3 Front Axle Full Load 2.1 bar
LC,08,4~7,30,Specified Pressure 3 Front Axle Full Load 2.2 bar
LC,08,4~7,40,Specified Pressure 3 Front Axle Full Load 2.3 bar
LC,08,4~7,50,Specified Pressure 3 Front Axle Full Load 2.4 bar
LC,08,4~7,60,Specified Pressure 3 Front Axle Full Load 2.5 bar
LC,08,4~7,70,Specified Pressure 3 Front Axle Full Load 2.6 bar
LC,08,4~7,80,Specified Pressure 3 Front Axle Full Load 2.7 bar
LC,08,4~7,90,Specified Pressure 3 Front Axle Full Load 2.8 bar
LC,08,4~7,A0,Specified Pressure 3 Front Axle Full Load 2.9 bar
LC,08,4~7,B0,Specified Pressure 3 Front Axle Full Load 3.0 bar
LC,08,4~7,C0,Specified Pressure 3 Front Axle Full Load 3.1 bar
LC,08,4~7,D0,Specified Pressure 3 Front Axle Full Load 3.2 bar
LC,08,4~7,E0,Specified Pressure 3 Front Axle Full Load 3.3 bar
LC,08,4~7,F0,Specified Pressure 3 Front Axle Full Load 3.4 bar
;
; {Specified Pressure 4 Rear Axle Partial Load}
LC,09,0~3,00,Specified Pressure 4 Rear Axle Partial Load 0.0 bar
LC,09,0~3,01,Specified Pressure 4 Rear Axle Partial Load 2.0 bar
LC,09,0~3,02,Specified Pressure 4 Rear Axle Partial Load 2.1 bar
LC,09,0~3,03,Specified Pressure 4 Rear Axle Partial Load 2.2 bar
LC,09,0~3,04,Specified Pressure 4 Rear Axle Partial Load 2.3 bar
LC,09,0~3,05,Specified Pressure 4 Rear Axle Partial Load 2.4 bar
LC,09,0~3,06,Specified Pressure 4 Rear Axle Partial Load 2.5 bar
LC,09,0~3,07,Specified Pressure 4 Rear Axle Partial Load 2.6 bar
LC,09,0~3,08,Specified Pressure 4 Rear Axle Partial Load 2.7 bar
LC,09,0~3,09,Specified Pressure 4 Rear Axle Partial Load 2.8 bar
LC,09,0~3,0A,Specified Pressure 4 Rear Axle Partial Load 2.9 bar
LC,09,0~3,0B,Specified Pressure 4 Rear Axle Partial Load 3.0 bar
LC,09,0~3,0C,Specified Pressure 4 Rear Axle Partial Load 3.1 bar
LC,09,0~3,0D,Specified Pressure 4 Rear Axle Partial Load 3.2 bar
LC,09,0~3,0E,Specified Pressure 4 Rear Axle Partial Load 3.3 bar
LC,09,0~3,0F,Specified Pressure 4 Rear Axle Partial Load 3.4 bar
; {Specified Pressure 4 Front Axle Partial Load}
LC,09,4~7,00,Specified Pressure 4 Front Axle Partial Load 0.0 bar
LC,09,4~7,10,Specified Pressure 4 Front Axle Partial Load 2.0 bar
LC,09,4~7,20,Specified Pressure 4 Front Axle Partial Load 2.1 bar
LC,09,4~7,30,Specified Pressure 4 Front Axle Partial Load 2.2 bar
LC,09,4~7,40,Specified Pressure 4 Front Axle Partial Load 2.3 bar
LC,09,4~7,50,Specified Pressure 4 Front Axle Partial Load 2.4 bar
LC,09,4~7,60,Specified Pressure 4 Front Axle Partial Load 2.5 bar
LC,09,4~7,70,Specified Pressure 4 Front Axle Partial Load 2.6 bar
LC,09,4~7,80,Specified Pressure 4 Front Axle Partial Load 2.7 bar
LC,09,4~7,90,Specified Pressure 4 Front Axle Partial Load 2.8 bar
LC,09,4~7,A0,Specified Pressure 4 Front Axle Partial Load 2.9 bar
LC,09,4~7,B0,Specified Pressure 4 Front Axle Partial Load 3.0 bar
LC,09,4~7,C0,Specified Pressure 4 Front Axle Partial Load 3.1 bar
LC,09,4~7,D0,Specified Pressure 4 Front Axle Partial Load 3.2 bar
LC,09,4~7,E0,Specified Pressure 4 Front Axle Partial Load 3.3 bar
LC,09,4~7,F0,Specified Pressure 4 Front Axle Partial Load 3.4 bar
;
; {Specified Pressure 4 Rear Axle Full Load}
LC,10,0~3,00,Specified Pressure 4 Rear Axle Full Load 0.0 bar
LC,10,0~3,01,Specified Pressure 4 Rear Axle Full Load 2.0 bar
LC,10,0~3,02,Specified Pressure 4 Rear Axle Full Load 2.1 bar
LC,10,0~3,03,Specified Pressure 4 Rear Axle Full Load 2.2 bar
LC,10,0~3,04,Specified Pressure 4 Rear Axle Full Load 2.3 bar
LC,10,0~3,05,Specified Pressure 4 Rear Axle Full Load 2.4 bar
LC,10,0~3,06,Specified Pressure 4 Rear Axle Full Load 2.5 bar
LC,10,0~3,07,Specified Pressure 4 Rear Axle Full Load 2.6 bar
LC,10,0~3,08,Specified Pressure 4 Rear Axle Full Load 2.7 bar
LC,10,0~3,09,Specified Pressure 4 Rear Axle Full Load 2.8 bar
LC,10,0~3,0A,Specified Pressure 4 Rear Axle Full Load 2.9 bar
LC,10,0~3,0B,Specified Pressure 4 Rear Axle Full Load 3.0 bar
LC,10,0~3,0C,Specified Pressure 4 Rear Axle Full Load 3.1 bar
LC,10,0~3,0D,Specified Pressure 4 Rear Axle Full Load 3.2 bar
LC,10,0~3,0E,Specified Pressure 4 Rear Axle Full Load 3.3 bar
LC,10,0~3,0F,Specified Pressure 4 Rear Axle Full Load 3.4 bar
; {Specified Pressure 4 Front Axle Full Load}
LC,10,4~7,00,Specified Pressure 4 Front Axle Full Load 0.0 bar
LC,10,4~7,10,Specified Pressure 4 Front Axle Full Load 2.0 bar
LC,10,4~7,20,Specified Pressure 4 Front Axle Full Load 2.1 bar
LC,10,4~7,30,Specified Pressure 4 Front Axle Full Load 2.2 bar
LC,10,4~7,40,Specified Pressure 4 Front Axle Full Load 2.3 bar
LC,10,4~7,50,Specified Pressure 4 Front Axle Full Load 2.4 bar
LC,10,4~7,60,Specified Pressure 4 Front Axle Full Load 2.5 bar
LC,10,4~7,70,Specified Pressure 4 Front Axle Full Load 2.6 bar
LC,10,4~7,80,Specified Pressure 4 Front Axle Full Load 2.7 bar
LC,10,4~7,90,Specified Pressure 4 Front Axle Full Load 2.8 bar
LC,10,4~7,A0,Specified Pressure 4 Front Axle Full Load 2.9 bar
LC,10,4~7,B0,Specified Pressure 4 Front Axle Full Load 3.0 bar
LC,10,4~7,C0,Specified Pressure 4 Front Axle Full Load 3.1 bar
LC,10,4~7,D0,Specified Pressure 4 Front Axle Full Load 3.2 bar
LC,10,4~7,E0,Specified Pressure 4 Front Axle Full Load 3.3 bar
LC,10,4~7,F0,Specified Pressure 4 Front Axle Full Load 3.4 bar
;
; {Specified Pressure 5 Rear Axle Partial Load}
LC,11,0~3,00,Specified Pressure 5 Rear Axle Partial Load 0.0 bar
LC,11,0~3,01,Specified Pressure 5 Rear Axle Partial Load 2.0 bar
LC,11,0~3,02,Specified Pressure 5 Rear Axle Partial Load 2.1 bar
LC,11,0~3,03,Specified Pressure 5 Rear Axle Partial Load 2.2 bar
LC,11,0~3,04,Specified Pressure 5 Rear Axle Partial Load 2.3 bar
LC,11,0~3,05,Specified Pressure 5 Rear Axle Partial Load 2.4 bar
LC,11,0~3,06,Specified Pressure 5 Rear Axle Partial Load 2.5 bar
LC,11,0~3,07,Specified Pressure 5 Rear Axle Partial Load 2.6 bar
LC,11,0~3,08,Specified Pressure 5 Rear Axle Partial Load 2.7 bar
LC,11,0~3,09,Specified Pressure 5 Rear Axle Partial Load 2.8 bar
LC,11,0~3,0A,Specified Pressure 5 Rear Axle Partial Load 2.9 bar
LC,11,0~3,0B,Specified Pressure 5 Rear Axle Partial Load 3.0 bar
LC,11,0~3,0C,Specified Pressure 5 Rear Axle Partial Load 3.1 bar
LC,11,0~3,0D,Specified Pressure 5 Rear Axle Partial Load 3.2 bar
LC,11,0~3,0E,Specified Pressure 5 Rear Axle Partial Load 3.3 bar
LC,11,0~3,0F,Specified Pressure 5 Rear Axle Partial Load 3.4 bar
; {Specified Pressure 5 Front Axle Partial Load}
LC,11,4~7,00,Specified Pressure 5 Front Axle Partial Load 0.0 bar
LC,11,4~7,10,Specified Pressure 5 Front Axle Partial Load 2.0 bar
LC,11,4~7,20,Specified Pressure 5 Front Axle Partial Load 2.1 bar
LC,11,4~7,30,Specified Pressure 5 Front Axle Partial Load 2.2 bar
LC,11,4~7,40,Specified Pressure 5 Front Axle Partial Load 2.3 bar
LC,11,4~7,50,Specified Pressure 5 Front Axle Partial Load 2.4 bar
LC,11,4~7,60,Specified Pressure 5 Front Axle Partial Load 2.5 bar
LC,11,4~7,70,Specified Pressure 5 Front Axle Partial Load 2.6 bar
LC,11,4~7,80,Specified Pressure 5 Front Axle Partial Load 2.7 bar
LC,11,4~7,90,Specified Pressure 5 Front Axle Partial Load 2.8 bar
LC,11,4~7,A0,Specified Pressure 5 Front Axle Partial Load 2.9 bar
LC,11,4~7,B0,Specified Pressure 5 Front Axle Partial Load 3.0 bar
LC,11,4~7,C0,Specified Pressure 5 Front Axle Partial Load 3.1 bar
LC,11,4~7,D0,Specified Pressure 5 Front Axle Partial Load 3.2 bar
LC,11,4~7,E0,Specified Pressure 5 Front Axle Partial Load 3.3 bar
LC,11,4~7,F0,Specified Pressure 5 Front Axle Partial Load 3.4 bar
;
; {Specified Pressure 5 Rear Axle Full Load}
LC,12,0~3,00,Specified Pressure 5 Rear Axle Full Load 0.0 bar
LC,12,0~3,01,Specified Pressure 5 Rear Axle Full Load 2.0 bar
LC,12,0~3,02,Specified Pressure 5 Rear Axle Full Load 2.1 bar
LC,12,0~3,03,Specified Pressure 5 Rear Axle Full Load 2.2 bar
LC,12,0~3,04,Specified Pressure 5 Rear Axle Full Load 2.3 bar
LC,12,0~3,05,Specified Pressure 5 Rear Axle Full Load 2.4 bar
LC,12,0~3,06,Specified Pressure 5 Rear Axle Full Load 2.5 bar
LC,12,0~3,07,Specified Pressure 5 Rear Axle Full Load 2.6 bar
LC,12,0~3,08,Specified Pressure 5 Rear Axle Full Load 2.7 bar
LC,12,0~3,09,Specified Pressure 5 Rear Axle Full Load 2.8 bar
LC,12,0~3,0A,Specified Pressure 5 Rear Axle Full Load 2.9 bar
LC,12,0~3,0B,Specified Pressure 5 Rear Axle Full Load 3.0 bar
LC,12,0~3,0C,Specified Pressure 5 Rear Axle Full Load 3.1 bar
LC,12,0~3,0D,Specified Pressure 5 Rear Axle Full Load 3.2 bar
LC,12,0~3,0E,Specified Pressure 5 Rear Axle Full Load 3.3 bar
LC,12,0~3,0F,Specified Pressure 5 Rear Axle Full Load 3.4 bar
; {Specified Pressure 5 Front Axle Full Load}
LC,12,4~7,00,Specified Pressure 5 Front Axle Full Load 0.0 bar
LC,12,4~7,10,Specified Pressure 5 Front Axle Full Load 2.0 bar
LC,12,4~7,20,Specified Pressure 5 Front Axle Full Load 2.1 bar
LC,12,4~7,30,Specified Pressure 5 Front Axle Full Load 2.2 bar
LC,12,4~7,40,Specified Pressure 5 Front Axle Full Load 2.3 bar
LC,12,4~7,50,Specified Pressure 5 Front Axle Full Load 2.4 bar
LC,12,4~7,60,Specified Pressure 5 Front Axle Full Load 2.5 bar
LC,12,4~7,70,Specified Pressure 5 Front Axle Full Load 2.6 bar
LC,12,4~7,80,Specified Pressure 5 Front Axle Full Load 2.7 bar
LC,12,4~7,90,Specified Pressure 5 Front Axle Full Load 2.8 bar
LC,12,4~7,A0,Specified Pressure 5 Front Axle Full Load 2.9 bar
LC,12,4~7,B0,Specified Pressure 5 Front Axle Full Load 3.0 bar
LC,12,4~7,C0,Specified Pressure 5 Front Axle Full Load 3.1 bar
LC,12,4~7,D0,Specified Pressure 5 Front Axle Full Load 3.2 bar
LC,12,4~7,E0,Specified Pressure 5 Front Axle Full Load 3.3 bar
LC,12,4~7,F0,Specified Pressure 5 Front Axle Full Load 3.4 bar
;
