;
; VCDS Redirect File
;
; Copyright © 2006-2012 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J523 - Control Head Front (#07)
;
; P/N: 4E0-910-7??-???
;
; includes measuring blocks, coding and adaptation
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4E-07.LBL
; 4E0-910-7xx-07.LBL
;
; created on 09/Feb/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 29/Mar/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Voltage Status,,Range: 0 = inactive / 1 = active\n\nx000xxx? = Term. S\nx000xx?x = Term. 15\nx000x?xx = Term. X\nx000?xxx = Term. 50\n?000xxxx = Status invalid
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
002,4,Send Diode,Temperature,Specification: -40.0...+85.0 °C
;
003,0,Diagnostic Wire
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
017,0,MMI-Terminal I
017,1,Function,Buttons,Range: 0 = Not Operated / 1 = Operated\n\nxxxxxxx? = RADIO\nxxxxxx?x = CD/TV\nxxxxx?xx = NAME\nxxxx?xxx = TEL\nxxx?xxxx = NAV\nxx?xxxxx = INFO\nx?xxxxxx = CAR\n?xxxxxxx = SETUP
017,2,Control/Arrow,Buttons,Range: 0 = Not Operated / 1 = Operated\n\n0xxxxxx? = Left Upper Control Button\n0xxxxx?x = Left Lower Control Button\n0xxxx?xx = Right Upper Control Button\n0xxx?xxx = Right Lower Control Button\n0xx?xxxx = Return Button\n0x?xxxxx = Left Arrow Button\n0?xxxxxx = Right Arrow Button
;
018,0,MMI-Terminal II
018,1,Operating Knobs,,Range: 0 = Not Operated / 1 = Operated\n\n000000x? = Control Button\n000000?x = ON/OFF Knob
018,2,Control Knob,Rotation,Range: -127.0...+127.0
018,3,ON/OFF Knob,Rotation,Range: -127.0...+127.0
;
020,0,MMI-Terminal (External)
020,1,MMI-Display,Button,Range: 0 = Not Operated / 1 = Operated
;
033,0,MMI-Display
033,1,MMI-Display,Temperature,Specification: -40.0...+85.0 °C
033,2,MMI-Display,Brightness,Unit: cd/m˛
;
049,0,Input Signals (via MOST-Bus)
049,1,Dimming,(Terminal 58d),Range: 0.0...100.0 %
049,2,Dimming,(Terminal 58s),Range: 0.0...100.0 %
049,3,Vehicle Speed
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Control Head Front (J523) Coding
C01,00?0xxx: Start Screen
C02,0 = Audi A8 (4E) / 1 = Audi S8 (4E)
C03,00x0?xx: Mute
C04,0 = Mute-Wire inactive
C05,1 = Mute-Wire active
C06,2 = Soft-Mute active (for Special Purpose Vehicles with Radio)
C07,3 = Soft-Mute and Line-In active (for Telephone Retrofitting)
C08,00x0x??: Language
C09,01 = German / 02 = English (GB) / 03 = English (US)
C10,04 = Spanish / 05 = Italian / 06 = French
C11,07 = Potuguese / 08 = Japanese / 09 = Chinese
C12,10 = Dutch / 11 = Greek / 12 = Russian
C13,13 = Polski / 14 = Hungarian / 15 = Croation
C14,16 = Turkish / 17 = Slovenian / 18 = Slovakian
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Installation List I (MMI Functionality)
A001,5,Installation List I (MMI Functionality)
A001,6,+00001 = Adaptive Cruise Control installed (PR-8T4)
A001,7,+00002 = Ambient Lighting installed (PR-QQ1)
A001,8,+00004 = Acoustic Parking System Front installed (PR-7X2)
A001,9,+00008 = Acoustic Parking System Rear installed (PR-7X1/7X2)
A001,10,+00016 = Tire Pressure Monitoring System installed (PR-7K3/7K4/7K5)
A001,11,+00032 = Sunroof installed (PR-3FE/3FR)
A001,12,+00064 = Adaptive Air Suspension installed (PR-1BK)
A001,13,+00128 = 802.11p Module installed
A001,14,+00256 = Rain Sensor installed (PR-8N3)
A001,14,+00512 = One Touch Memory (Fingerprint) installed
A001,16,+01024 = Seat Adjustment Front installed (PR-3PN)
A001,17,+02048 = Seat Adjustment Rear installed (PR-5Z1)
A001,18,+04096 = Multi-Function Steering Wheel installed (PR-1XW)
A001,19,+08192 = Lane Change Assistant installed
A001,20,+16384 = Lane Holding Assistant installed
A001,21,+32768 = Back-Up Camera installed
;
A002,0,Installation List II (MMI Functionality)
A002,5,Installation List II (MMI Functionality)
A002,6,+00001 = Left-Hand-Steering (LHD) [Standard]
A002,7,+00002 = Vehicle Identification Number (VIN) available
A002,8,+00008 = Oil Level Display available
A002,9,+00016 = Digital Radio (DAB) Video Transmission
A002,10,+00032 = Battery Status Display active
;
A003,0,Auto-Return Value
A003,5,Auto-Return Value
A003,6,Time period for automatic closing MMI note menus.
;
A004,0,Speed Threshold
A004,5,Speed Threshold
A004,6,Speed above which "CAR Menu" function is disabled.
;
A005,0,Speed Delta
A005,5,Speed Delta
;
A006,0,MMI After-Run Time
A006,1,Current Value
A006,5,MMI After-Run Time
A006,6,Time between shut-off and automatic shut-down of the MMI.
A006,7, 
A006,8,0 = Telematics / No Telephone installed
A006,9,16 = Mobile Phone Base Plate installed
;
A008,0,Service Menu
A008,5,Service Menu
A008,6,0 = Service Menu active
A008,7,1 = Service Menu active
A008,8, 
A008,9,The Service Menu gives you access to certain advanced functions.
A008,10,Use this at your own risk and only if you really understand
A008,11,what it is meant for. You can reach the menu by pressing
A008,12,and holding the buttons [SETUP]+[CAR] simultaneously.
;
A011,0,Additional MMI Options
A011,5,Additional MMI Options
A011,6,+00001 = Owners Manual available
A011,7,+00002 = One Touch Memory (Fingerprint NEW - from 4E*-905-128-B)
A011,8,+00004 = Frequency/Source Change via Function Button active
A011,9,+00016 = Driver Information System (DIS) installed
A011,10,+00032 = Climate Control Comfort available
A011,11,+00064 = Auxiliary Heating available
A011,12,+00256 = AUX-IN installed
;
A012,0,Telephone Type
A012,5,Telephone Type
A012,6,0 = No Telephone
A012,7,1 = Permanently installed
A012,8,2 = Mobile Phone Base Plate installed
A012,9,4 = Telematics installed
;
A014,0,MMI Remote Control learning (Part 1)
;
A015,0,MMI Remote Control learning (Part 2)
;
A016,0,Start/Boot Screen Time (OFF/Cold Boot)
A016,5,Start/Boot Screen Time (OFF/Cold Boot)
A016,6,Time for which the Start/Boot Screen will be
A016,7,shown when starting/booting the MMI.
A016,8, 
A016,9,Standard: 4 Seconds
;
A017,0,Start/Boot Screen Time (Standby)
A017,5,Start/Boot Screen Time (Standby)
A017,6,Time for which the Start/Boot Screen will be
A017,7,shown when starting/booting the MMI´from Standby.
A017,8, 
A017,9,Standard: 3 Seconds
;
A020,0,Optical Parking Aid Display (Duration)
A020,5,Optical Parking Aid Display (Duration)
A020,6,Time for which the Optical Parking Aid will be
A020,7,displayed in the Rear View/Backup Camera Display.
A020,8, 
A020,9,Standard: 3 Seconds
;
A021,0,Optical Parking Aid Display (Distance)
A021,5,Optical Parking Aid Display (Distance)
A021,6,Setting the Distance (Segments) as of which the Optical Parking Aid
A021,7,will be displayed in the Rear View Camera once an Obstacle is recognized.
A021,8, 
A021,9,Standard: 11 Segments
A021,10,Range: 0...12 Segments (0 = OFF / 12 = Always ON)
;
A063,0,Vehicle Speed Threshold (TV-Function)
;A063,5,Vehicle Speed Threshold (TV-Function)
;A063,6,Anpassung der Geschwindigkeit ab der
;A063,7,kein TV-Bild mehr angezeigt wird.
;
A064,0,Search Illumination Brightness
A064,5,Search Illumination Brightness
A064,6,Changes the Brightness of the Operating Control Search Illumination.
A064,7, 
A064,8,Note: This Change is for Testing only and will not be saved!
;
A065,0,Function Illumination Brightness
A065,5,Function Illumination Brightness
A065,6,Changes the Brightness of the Operating Control Functional Illumination.
A065,7, 
A065,8,Note: This Change is for Testing only and will not be saved!
;
A066,0,Display Test: Display ON/OFF
;
A067,0,Display Test: Brightness
A067,5,Display Test: Brightness
A067,6,Anpassung der Helligkeit der Bedienteil Displaybeleuchtung.
A067,7, 
A067,8,Note: This Change is for Testing only and will not be saved!
;
A068,0,Display Test: Test Pattern/Image
A068,5,Display Test: Test Pattern/Image
A068,6,To display a Test Pattern/Image on the
A068,7,MMI Screen enter the following Values:
A068,8, 
A068,9,1 = Red
A068,10,2 = Green
A068,11,3 = Blue
A068,12,4 = White
A068,13,5 = Black
A068,14,6 = Checkerboard
A068,15,7 = Checkerboard (inverted)
A068,16,8 = 64 Gray Scale (vertical Bars)
;
A070,0,One Touch Memory (Fingerprint) PIN
A070,5,One Touch Memory (Fingerprint) PIN
A070,6,Reset the Fingerprint PIN to "0000"
A070,7,for the selected User/Driver.
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
A111,0,MMI System Restart
A111,5,MMI System Restart
A111,6,An MMI system restart may be necessary to activate recoded or adapted values.
A111,7,To initiate the restart save '1' as new value.
;
