;
; VAG-COM Label File
;
; Audi A4 (8E)
;
; Component: J364 - Auxiliary Heater (#18)
;
; P/N: 8E0-265-105-X
;
; includes measuring blocks, coding and adaptation
;
; created on 28/Jan/2012 by Jochen Bender (a4quattro@gmx.net)
;
; last modification: 02/Feb/2012
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,1,Battery voltage,,Display range: 11...14 Volt
001,2,Voltage at ECU,,Display range: 11...14 Volt
001,3,Undervoltage limit,,Display range: Volt
001,4,Type of under-, voltage turn-off,,Display range: Automatic/Fixed
;
002,1,Actual heater, temperature,,Display range: °C
002,2,N279 valve trigger,,Display range: %
002,3,Lowest temp., since start,,Display range: °C
002,4,Actual speed of, comb. air blower,,Display range: 1/min
;
003,1,Power factor, comb. air blower,,Display range: %
003,2,Power factor, circul. pump,,Display range: %
003,3,Power factor, glow plug,,Display range: %
003,4,Power factor, dosage pump,,Display range: %
;
004,1,Signal from, flame detector,,Display range: recogneized/ not recogneized
004,2,Signal to air cond., fan control,,Display range: %
004,3,Power factor, actual heat load,,Display range: %
004,4,Fuel consumption, since start in ml,,Display range: ml
;
005,1,Time until, turn-off,, Display range: s
005,2,Actual working time, since start,,Display range: s
005,3,Signals from CAN-, bus status 1,,Display range: bits
005,4,Signals from CAN-, bus status 2,,Display range: bits
;
006,1,Actual status, auxiliary heater,,Display range: Start/Stop
006,2,Actual or last, duty type,,Display range: Pump on/?
006,3,Actual start/stop, condition from CAN,,Display range: ?
006,4,N/A
;
007,1,Signal status, rem. control R64,,
007,2,Status of analog, control port,,(not used for factory heaters)
007,3,Counter f. stops, due to overtemp.,,
007,4,Counter f. errors, in heater mode,,
;
008,1,Total burn time., (with flame) in h,,
008,2,Total operation, time in h,,
008,3,Total glow cycles, (start cyles),,
008,4,Total fuel cons., in Liter,,
;
009,1,Lowest temp., since start,,Display range: °C
009,2,Outside temp., comm. from -J285-,,Display range: °C
009,3,Coolant temp., comm. from -J285-,,Display range: °C
009,4,Outside temp., comm. from -J255-,,Display range: °C
;
010,1,Lowest temp., since start,,Display range: °C
010,2,Engine speed comm., from -J285- in 1/min,,
010,3,Time until, turn-off,, Display range: s
010,4,N/A
;
011,1,Last turn-off, issued by ..,,(special look-up table necessary)
011,2,2nd last turn-o., issued by ..,,(special look-up table necessary)
011,3,3rd last turn-o., issued by ..,,(special look-up table necessary)
011,4,4th last turn-o., issued by ..,,(special look-up table necessary)
;
012,1,Boundary condition, of last turn-o.,,
012,2,Boundary condition, of last turn-o.,,
012,3,Boundary condition, of last turn-o.,,
012,4,Boundary condition, of last turn-o.,,
;
013,1,Boundary condition, 2nd last turn-o.,,
013,2,Boundary condition, 2nd last turn-o.,,
013,3,Boundary condition, 2nd last turn-o.,,
013,4,Boundary condition, 2nd last turn-o.,,
;
014,1,Boundary condition, 3rd last turn-o.,,
014,2,Boundary condition, 3rd last turn-o.,,
014,3,Boundary condition, 3rd last turn-o.,,
014,4,Boundary condition, 3rd last turn-o.,,
;
015,1,Unburnt fuel, quantity,,
015,2,Unburnt fuel, quantity,,
015,3,Unburnt fuel, quantity,,
015,4,Unburnt fuel, quantity,,
;
080,1,Manufacturer, mark of -J364-,,
080,2,Day of manuf.,of ECU -J364-,,
080,3,Revision level, of -J364-,,
080,4,Teststand ID where, -J364- was checked,,
080,5,Manufacturer ID, of ECU -J364-,,
;
082,1,ID of updater, (flash tool ID),,
082,2,Date of last, SW update,,
082,3,HW rev. level, of ECU -J364-,,
082,4,SW rev. level, of ECU -J364-,,
;
090,1,Heater tested, during manuf.,, Display Range: ARDIC TEST: Y/ARDIC TEST: N
090,3,Heater tested, during manuf.,, Display Range: BERIFORS TEST: Y/BERIFORS TEST: N
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Auxiliary Heater (-J364-) Coding
C01,00?xx: Shutoff valve -N279-
C02,0 = Shutoff valve -N279- not installed
C03,1 = Shutoff valve -N279- installed (coding not recommended if valve is available in 4 cyl. Diesel;
C04,requires adaption value "0001x" in channel 18 of instrument cluster -J285- to activate "Incl. Motor")
C05,
C06,00x?x: Circulation pump -V55-
C07,0 = Circulation pump not installed (variant not planned)
C08,1 = Circulation pump installed
C09,
C10,00xx?: Type of undervoltage turn-off
C11,1 = Temperature dependent voltage correction value (factory default)
C12,2 = Fixed voltage value (on customer request; refer to settings in adaption channel 1)
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A001,0,Undervoltage heater turn-off setting
A001,5,Undervoltage heater turn-off setting
A001,6,Turn-off temperature dependent (if factory default Coding 00xx1)
A001,7,Factory setting is 12.17V which equates to encryption value "9138"
A001,8,Recommended setting range is 9.98V - 12.65V encrytion look up table below:
A001,9,
A001,10,Encrytion value   Voltage value   Encrytion value   Voltage value
A001,11,      9106     =     9.98V               9130     =    11.60V
A001,12,      9110     =    10.25V               9138     =    12.17V
A001,13,      9120     =    10.90V               9145     =    12.65V
A001,14,
A001,15,Turn-off at fixed value (if coding 00xx2 on customer request AND/OR if heater is in
A001,16,automatic heating mode at Coding 00xx1) factory setting is 9.5V which equates to "9097"
A001,17,Recommended setting range 8.00V - 12.99V encrytion look up table below:
A001,18,
A001,19,Encrytion value   Voltage value   Encrytion value   Voltage value
A001,20,      9077     =     8.00V               9120     =    10.90V
A001,21,      9090     =     9.00V               9130     =    11.60V
A001,22,      9097     =     9.50V               9140     =    12.30V
A001,23,      9100     =     9.60V               9150     =    12.99V
A001,24,      9110     =    10.25V
;
A002,0,Dosage pump -V54- control to adjust CO2 volume in exhaust
A002,5,Dosage pump -V54- control to adjust CO2 volume in exhaust
A002,6,The adjustment is done by changing the pulse frequency
A002,7,
A002,8,Gasoline version: Factory default is 147ms (147/1000 sec) equates to 6.8Hz (pulses per second)
A002,9,Diesel version: Factory default is 176ms (176/1000 sec) equates to 5.7Hz (pulses per second)
A002,10,
A002,11,Remark: The correct setpoint for CO2 volume is 9.5% +/-0.04% (for both Gasoline and Diesel engines)
A002,12,The CO2 volume changes by 0.07% per 1ms. Example: The measured CO2 value is 8.8% and the setting
A002,13,is 176ms -> changing it to 166ms results in a CO2 setpoint value of 9.5%.
;
A003,0,Aux. heater turn-off condition after engine stop
A003,5,Aux. heater turn-off condition after engine stop
A003,6,Setting "1" = Heater keeps running until the remaining set time is elapsed (factory default)
A003,7,Setting "2" = Heater turns off with engine stop (on customer request)
;
A004,0,Learn remote control unit
A004,5,Learn remote control unit
A004,6,
A004,7,Start the learn process by entering "1" =>> "LERNEN" appears.
A004,8,Press the "Turn ON" button of the remote control unit within 30sec =>> "ERKANNT" appears.
A004,9,
A004,10,Up to 4 remote control units can be learned. Learning a 5th remote control unit automatically
A004,11,deletes the 1st remote control unit!
:
A005,0,Matching the ECU -J364- to fuel type (Gasoline or Diesel)
A005,5,Matching the ECU -J364- to fuel type (Gasoline or Diesel)
A005,6,Setting "1" = The ECU -J364- is set to Diesel
A005,7,Setting "2" = The ECU -J364- is set to Gasoline
A005,8,Remark: With this adjustment it is possible to use one and the same ECU -J364- in either Gasoline or
A005,9,Diesel cars but never swap the entire aux. heater because of the different heater hardware!!
;
A006,0,Set ECU -J364- to operate in automatic heating mode (at outside temp. < 5°C and "ECON" off)
A006,5,Set ECU -J364- to operate in automatic heating mode
A006,6,Setting "0" = Automatic heating ON (factory default)
A006,7,Setting "1" = Automatic heating OFF (on customer request; works only for Gasoline engines)
;
A081,0,Learn Vehicle Identification Number (VIN)
A081,5,Learned Values (Vehicle Data)
A081,6,To start the process for vehicle data (VIN)
A081,7,learning just enter and save "26467" as new value.
; 
A087,0,Setting for lowest speed of combustion air blower -V6- >>> Enter "22222" in LOGIN first <<<
A087,5,Setting for lowest speed of combustion air blower -V6-
A087,6,The following procedure is to correct smoking heaters while switching from full throttle to
A087,7,part throttle mode (only necessary for cars up to model year 2004!).
A087,8,
A087,9,Factory default for ECUs until index B is "00048" (= 4800/min). Change this value to "00065"
A087,10,(= 6500/min) and save it. The lowest allowed speed is now set to 6500/min. Please start heater
A087,11,until the heater switches from full to part throttle and see whether the smoking phenomenon is mitigated.
A087,12,
A087,13,Remark: You need to login in ECU (function "11") with login code "22222" at first!
;