;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; Seat Altea/Toledo (5P) / Seat Leon (1P) / Skoda Octavia II (1Z)
; VW Caddy (2K) / VW Eos (1F) / VW Golf/Jetta (1K) / VW Touran (1T)
;
; Component: J255 - A/C Heating Electronics (#08) - Climatronic
;
; P/N: 1K0-907-044-???
;
; includes measuring blocks, basic setting and adaptation
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1P-08.LBL
; 1Q-08.LBL
; 1T-08.LBL
; 1Z-08.LBL
; 5P-08.LBL
; 1K0-907-044.LBL
;
; created on 23/Mar/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 18/Jun/2010
;
; requires VCDS 11.9.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,General
001,1,Compressor,Shut-Off Code,Specification: 0 = Compressos ON\n\nSee Label File
001,2,Engine Speed
001,3,Vehicle Speed
001,4,Standing Time
;
B001,0,Potentiometer && Flap Alignment
B001,1, , , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
B001,11,The Basic Setting (Duration max. 30 Seconds) must be performed when:
B001,12,- Climatronic Control Module (J255) or Display/Operating Unit Rear (E265) replaced
B001,13,- Flap Motor or Fan Control replaced
;
002,0,Compressor
002,1,Compressor,Current (actual)
002,2,Compressor,Current (specified)
002,3,Compressor,Rotations
002,4,Compressor Load
;
003,1,Coolant,Pressure
003,2,Radiator Fan,Activation (actual)
003,3,Radiator Fan,Activation (spec.)
003,4,Engine Speed,(increase)
;
004,0,Temperatures
004,1,Outside Temp.,Unfiltered,Display Range: -50...+63 °C
004,2,Outside Temp.,Regulation,Display Range: -50...+77 °C
004,3,Fresh Air Intake,Temperature,Display Range: -40...+60 °C
004,4,Coolant,Temperature,Display Range: -48...+126 °C
;
005,0,Outlet/Footwell Blower Temperature
005,1,Left Outlet Blower,Temperature,Display Range: 0...84 °C
005,2,Right Outlet Blower,Temperature,Display Range: 0...84 °C
005,3,Left Footwell,Blower Temp.,Display Range: 0...84 °C
005,4,Right Footwell,Blower Temp.,Display Range: 0...84 °C
;
006,1,Evaporator,Temperature
006,2,Interior,Temperature
006,3,Left Sunlight,Intensity (G107),W/m²
006,4,Right Sunlight,Intensity (G134),W/m²
;
007,1,Turbine Voltage,(actual),Display Range: 0.0...13.0 V
007,2,Turbine Voltage,(specified),Display Range: 0.0...13.0 V
007,3,Turbine Load,,Display Range: 0.0...100.0 %
007,4,Voltage,(Terminal 30)
;
008,1,Voltage,(Terminal 15)
008,3,Dimming,(Terminal 58d),Display Range: 0.0...100.0 %
008,4,Country,,0 = Rest of World (RoW)\n2 = North America (NAR)\n5 = Japan
;
009,0,Rear Window Heater (Z2) && Aux. Heater
009,1,Rear Window,Heater (Z2 / Actual)
009,2,Rear Window,Heater (Z2 / Spec.)
009,3,Aux. Heater,Status,Display Range: ON/OFF
009,4,Aux. Heater,Current
;
010,1,Aux. Heater,Request,Display Range: ON/OFF
010,2,Heater OFF,,Display Range: ON/OFF
010,3,Back-Up Lights,,Display Range: ON/OFF
010,4,Front Wiper,,Display Range: ON/OFF
;
011,0,Air Recirculation Flap Control Motor (V113) / Potentiometer (G143)
011,1,Current Value
011,2,Specified Value
011,3,Minimum Position,(Lower Stop/Close)
011,4,Maximum Position,(Upper Stop/Open)
;
012,0,Left Temperature Flap Control Motor (V158) / Potentiometer (G220)
012,1,Current Value
012,2,Specified Value
012,3,Minimum Position,(Lower Stop/Close)
012,4,Maximum Position,(Upper Stop/Open)
;
013,0,Right Temperature Flap Control Motor (V159) / Potentiometer (G221)
013,1,Current Value
013,2,Specified Value
013,3,Minimum Position,(Lower Stop/Close)
013,4,Maximum Position,(Upper Stop/Open)
;
014,0,Center Flap Control Motor (V70) / Potentiometer (G112)
014,1,Current Value
014,2,Specified Value
014,3,Minimum Position,(Lower Stop/Close)
014,4,Maximum Position,(Upper Stop/Open)
;
015,0,Defroster Flap Control Motor (V107) / Potentiometer (G135)
015,1,Current Value
015,2,Specified Value
015,3,Minimum Position,(Lower Stop/Close)
015,4,Maximum Position,(Upper Stop/Open)
;
016,0,Air Flow Flap Control Motor (V71) / Potentiometer (G113)
016,1,Current Value
016,2,Specified Value
016,3,Minimum Position,(Lower Stop/Close)
016,4,Maximum Position,(Upper Stop/Open)
;
017,2,Roof Status,,0 = Closed\n1 = Moving: Opening\n2 = Open\n3 = Moving: Closing
;
080,0,Advanced Control Module Identification I
;
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Air Flow Flap Control Motor (V71)
A001,5,Air Flow Flap Control Motor (V71)
A001,6,0 = Vehicles with separate Air Flow Flap Control Motor (through ca. MY 2007)
A001,7,1 = Vehicles w/o separate Air Flow Flap Control Motor (from ca. MY 2008)
A001,8, 
A001,9,Only effects the following Control Modules:
A001,10,1K0-907-044-* (from SW 1111)
A001,11,1Q0-907-044-* (from SW 0303)
A001,12,1Z0-907-044-* (from SW 0600)
A001,13,3C0-907-044-* (from SW 0707)
A001,14, 
A001,15,Note: See TPI 2016077 (VW) or TPI 2020543 (Skoda)
;
A002,0,Air Recirculation Flap Control Motor (V113)
A002,5,Air Recirculation Flap Control Motor (V113)
A002,6,0 = Vehicles with separate Air Recirculation Flap Control Motor (from ca. MY 2007)
A002,7,1 = Vehicles w/o separate Air Recirculation Flap Control Motor (from ca. MY 2008)
A002,8, 
A002,9,Only effects the following Control Modules:
A002,10,1Z0-907-044-* (from SW 0600)
A002,11, 
A002,12,Note: See TPI 2016077 (VW) or TPI 2020543 (Skoda)
;
