;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Audi A6 (4F) / Audi Q7 (4L)
;
; Component: J520 - Central Electronics II (#4F)
;
; P/N: 4F0-910-280-???
;
; includes measuring blocks, adaptation, coding, security access and selective output tests
;
; created on 11/Jul/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 24/Jan/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring block
;
;---------------------------------------------------
;
;
001,1,Voltage Supply,(Terminal 30)
001,2,Outside,Temperature
;
002,0,Vehicle Data
002,1,Engine Speed
002,2,Vehicle Speed
002,3,Steering Angle,Sensor
;
003,0,Servotronic
003,2,Servotronic Valve,Adjusted Current
003,3,Servotronic Valve
;
004,0,Sunroof Comfort Function
004,1,Sunroof Comfort,Opening (CAN)
004,2,Sunroof Comfort,Closing (CAN)
004,3,Sunroof Comfort,Opening
004,4,Sunroof Comfort,Closing
;
005,0,Eneryg,
005,1,Terminal 15,Status
005,2,Terminal X,Status
005,3,Energy Manager,Dynamic Shut-Off
005,4,Energy Manager,Static Shut-Off
;
006,0,Inclination Sensor
006,1,X-Value,(absolute)
006,2,X-Value,(difference)
006,3,Y-Value,(absolute)
006,4,Y-Value,(difference)
;
007,0,Sunroof
007,1,Speed Signal,(Sunroof)
007,2,Enabling Sunroof
007,3,Enabling,Comfort Functions
;
008,0,Glove Compartment && Central Locking
008,1,Button for,Glove Compartm.
008,2,Central Locking,Open
008,3,Links of,Pre-Conditions
008,4,Glove Compartm.,Motor
;
020,0,Component Protection
020,1,Component,Protection
020,2,CAN Lock Counter
020,3,SA Lock Counter
;
140,0,CAN-Databus Communication (Comfort)
140,1,Battery Manager,,Specification: Batt.Mgmt 1
140,2,CAN-Gateway,,Specification: Gateway 1
140,3,Electrical,Ignition Lock,Specification: El.Ign.Lock 1
;
141,0,CAN-Databus Communication (Comfort)
141,1,Climate Control,,Specification: A/C 1
141,2,Databus,Status,Display Range: 1-Wire/2-Wire/No Communication 
141,3,Central,Electronics,Specification: Central 1
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T2264,Servotronic Steering: Full Assistance
T2265,Servotronic Steering: No Assistance
T2661,Speed Signal (Sunroof)
T2662,Comfort Opening of Sunroof
T2663,Comfort Closing of Sunroof
T2752,Glovebox Unlocking Motor (V327)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S0,Central Electronics II (J520) Security Access
S1,12151 - General Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Inclination Sensor Threshold
A001,5,Inclination Sensor Threshold
A001,6,Alarm threshold in X and Y direction.
;
A002,0,Glove Compartment Activation Time
A002,5,Glove Compartment Activation Time
A002,6,Time for which the glove compartment opening is
A002,7,permitted after the ignition is switched off.
;
A003,0,Anti-Play Protection Decrease Time
A003,5,Anti-Play Protection Decrease Time
A003,6,Time after the anti-play protection counter is decreased by 1.
;
A004,0,Anti-Play Protection Threshold
A004,5,Anti-Play Protection Threshold
A004,6,Threshold for anti-play protection counter from which an activation is prevented.
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electronics II (J520) Coding
C01,00?xxxx: Engine Type I
C02,0 = All Engine Types / Audi Q7 (4L)
C03,0 = Other Engine Types / Audi A6 (4F)
C04,1 = 8/10-Cylinder Gasoline Engine / Audi A6 (4F)
C05,00x?xxx: Country
C06,+1 = Rest of World (RoW)
C07,+2 = North American Region (NAR)
C08,00xx?xx: Options I
C09,+1 = Inclination Sensor installed
C10,00xxx?x: Options II
C11,0 = Sunroof NOT installed (PR-3FA/3FL) OR Open-Sky-System (OSS) installed (PR-3FU)
C12,1 = Sunroof installed (PR-3FE/3FR) / ONLY Audi A6 (4F)
C13,00xxxx?: Engin Type II
C14,1 = All Engine Types / ONLY Audi Q7 (4L)
C15,3 = 6-Cylinder Diesel Engine / ONLY Audi A6 (4F)
C16,4 = Other Engine Types / ONLY Audi A6 (4F)
;
