;
; VCDS Label File
;
; Copyright © 2005-2009 Ross-Tech, LLC
;
; Audi A3 (8P) / Audi TT (8N) / Seat Altea (5P) / Seat Toledo (5P)
; Skoda Octavia (1Z) / VW Golf IV (1J) / VW Golf V (1K) / VW Touran (1T)
;
; Component: Automatic Transmission (#02) - 02E
;
; P/N: 02E-300-0??-??
;
; includes measuring blocks
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 02-02.LBL
; 02E-300-0xx.LBL
;
; created on 04/Apr/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 02/Jul/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;---------------------------------------------------
;
;
001,1,Brake Light,Switch (F),Display Range: operated/not operated
001,2,Brake Test,Switch,Display Range: operated/not operated
001,3,Shift Lock,Status,Display Range: PN active/PN inactive
001,4,Vehicle Speed,,Display Range: 0...255 km/h
;
002,1,Selector Lever,Position,Display Range: P/R/N/D/S/TT/PL/MI/ZS/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; PL - Plus (upshift in tiptronic Mode)
; MI - Minus (downshift in tiptronic Mode)
; ZS - intermediate position (selector lever between 2 gears or driving modes)
; ER - ERROR
002,2,Selector Lever,Position,Display Range: P/R/N/D/S/TT/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; ER - ERROR
002,3,Error Byte from,Selector Lever,Display Range: 0 = not active/ 1 = active
002,4,Selected gear,or driving mode,Display Range (driving modes): P/R/N/D | Display Range (Tiptronic) 1/2/3/4/5/6
;
003,1,Selector Lever,Position,Display Range: P/R/N/D/S/TT/PL/MI/ZS/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; PL - Plus (upshift in tiptronic Mode)
; MI - Minus (downshift in tiptronic Mode)
; ZS - intermediate position (selector lever between 2 gears or driving modes)
; ER - ERROR
003,2,Selector Lever,Position,Display Range: P/R/N/D/S/TT/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; ER - ERROR
003,3,Tiptronic,upshift,Display Range: operated/not operated
003,4,Tiptronic,downshift,Display Range: operated/not operated
;
004,1,Selector Lever,Position,Display Range: P/R/N/D/S/TT/PL/MI/ZS/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; PL - Plus (upshift in tiptronic Mode)
; MI - Minus (downshift in tiptronic Mode)
; ZS - intermediate position (selector lever between 2 gears or driving modes)
; ER - ERROR
004,2,Driving,direction,Display Range: forward/backward/not recognized
004,3,Transmission,Output Speed 1,G195 (Display Range: 0...4080 RPM)
004,4,Transmission,Output Speed 2,G196 (Display Range: 0...4080 RPM)
;
005,1,Selector Lever,Position,Display Range: P/R/N/D/S/TT/PL/MI/ZS/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; PL - Plus (upshift in tiptronic Mode)
; MI - Minus (downshift in tiptronic Mode)
; ZS - intermediate position (selector lever between 2 gears or driving modes)
; ER - ERROR
005,2,Starting,enabled,Display Range: operated/not operated
005,3,Voltage Supply 1,,Display Range: 0.0...25.5 V
005,4,Voltage Supply 2,,Display Range: 0.0...25.5 V
;
006,1,Selector Lever,Position,Display Range: P/R/N/D/S/TT/PL/MI/ZS/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; PL - Plus (upshift in tiptronic Mode)
; MI - Minus (downshift in tiptronic Mode)
; ZS - intermediate position (selector lever between 2 gears or driving modes)
; ER - ERROR
006,2,Valve current,clutch valve 1,N215 (Display Range: 0...1.530 A)
006,3,Safety valve 1,(N233),Display Range: 0...100 %
006,4,Main pressure,valve current,N217 (Display Range: 0...1.530 A)
;
007,1,Selector Lever,Position,Display Range: P/R/N/D/S/TT/PL/MI/ZS/ER
;  P - Parking
;  R - Reverse Gear
;  N - Neutral
;  D - Drive (Normal)
;  S - Drive (Sport)
; TT - tiptronic Mode
; PL - Plus (upshift in tiptronic Mode)
; MI - Minus (downshift in tiptronic Mode)
; ZS - intermediate position (selector lever between 2 gears or driving modes)
; ER - ERROR
007,2,Valve current,clutch valve 2,N216 (Display Range: 0...1.530 A)
007,3,Safety valve,(N371),Display Range: 0...100 %
007,4,Main pressure,valve current,Display Range: 0...1.530 A
;
008,1,Transmission,Input Speed (G182),Display Range: 0...8160 RPM
008,2,Driveshaft 1,Speed (G501),Display Range: 0...8160 RPM
008,3,Driveshaft 2,Speed (G502),Display Range: 0...8160 RPM
008,4,Transmission,Output Speed,Display Range: 0...4080 RPM
;
009,1,Engine Speed (G28),,Display Range: 0...8160 RPM
009,2,Transmission,Input Speed (G182),Display Range: 0...8160 RPM
009,3,Transmission,Output Speed,Display Range: 0...4080 RPM
009,4,Transmission,Output Speed,via CAN (Display Range: 0...4080 RPM)
;
010,1,Accelerator,pedal angle,Display Range: 0...100 %
010,2,Kick-Down switch,,Display Range: operated/not operated
010,3,Engine torque,,Display Range: -100...+410 Nm
010,4,Engine torque,(loss),Display Range: -50...+205 Nm
;
011,1,Driveshaft 1,Speed (G501),Display Range: 0...8160 RPM
011,2,Specified clutch,torque K1,Display Range: -600...600 Nm
011,3,Valve current,clutch valve 1,Display Range: 0...1.530 A
011,4,Actual pressure,clutch 1 (G193),Display Range: -327.68...327.67 bar
;
012,1,Driveshaft 2,Speed (G502),Display Range: 0...8160 RPM
012,2,Specified clutch,torque K2,Display Range: -600...600 Nm
012,3,Valve current,clutch valve 2,Display Range: 0...1.530 A
012,4,Actual pressure,clutch 2 (G194),Display Range: -327.68...327.67 bar
;
013,1,Solenoid current,clutch valve 1,Display Range: 0...1.530 A
013,2,Safety Valve 1,,Display Range: 0...100 %
013,3,Solenoid Valve 1,(N88),Display Range: 0...100 %
013,4,Solenoid Valve 2,(N89),Display Range: 0...100 %
;
014,1,Solenoid current,clutch valve 2,Display Range: 0...1.530 A
014,2,Safety Valve 2,,Display Range: 0...100 %
014,3,Solenoid Valve 3,(N90),Display Range: 0...100 %
014,4,Solenoid Valve 4,(N91),Display Range: 0...100 %
;
015,0,Gear Selector
015,1,Gear Selector 1-3,,Display Range: 0...1023
015,2,Gear Selector 2-4,,Display Range: 0...1023
015,3,Gear Selector 5-N,,Display Range: 0...1023
015,4,Gear Selector 6-R,,Display Range: 0...1023
;
016,0,Travel Distance
016,1,Travel Distance,Gear Selector 1-3,Specification: -12.7...+12.8 mm
016,2,Travel Distance,Gear Selector 2-4,Specification: -12.7...+12.8 mm
016,3,Travel Distance,Gear Selector 5-N,Specification: -12.7...+12.8 mm
016,4,Travel Distance,Gear Selector 6-R,Specification: -12.7...+12.8 mm
;
017,0,Synchronous travel path
017,1,Synchronous travel,path 3rd gear,Display Range: -12.7...+12.8 mm
017,2,Synchronous travel,path 2nd gear,Display Range: -12.7...+12.8 mm
017,3,Synchronous travel,path N gear,Display Range: -12.7...+12.8 mm
017,4,Synchronous travel,path R gear,Display Range: -12.7...+12.8 mm
;
018,0,Synchronous travel path
018,1,Synchronous travel,path 1st gear,Display Range: -12.7...+12.8 mm
018,2,Synchronous travel,path 4th gear,Display Range: -12.7...+12.8 mm
018,3,Synchronous travel,path 5th gear,Display Range: -12.7...+12.8 mm
018,4,Synchronous travel,path 6th gear,Display Range: -12.7...+12.8 mm
;
019,1,Temperature,Transmission Fluid,G93 (Display Range: -250.0...250.0 °C)
019,2,Temperature,Control Module,G510 (Display Range: -250.0...250.0 °C)
019,3,Temperature,Clutch Oil (G509),Display Range: -250.0...250.0 °C
019,4,Idle Status,,Display Range: 0 = not idle / 1 = idle
;
030,0,Adapted clutch adjustment (clutch 1)
030,1,Lower adjustment,,from IKp0 adaptation (Display Range: 0...1.275 A)
030,2,Lower adjustment,,from Micro-Slip-Adaptation (Display Range: 0...1.275 A)
030,3,Upper adjustment,,from Micro-Slip-Adaptation (Display Range: 0...1.275 A)
030,4,Upper adjustment,,from Macro-Slip-Adaptation (Display Range: 0...1.275 A)
;
031,0,Adapted clutch adjustment (clutch 2)
031,1,Lower adjustment,,from IKp0 adaptation (Display Range: 0...1.275 A)
031,2,Lower adjustment,,from Micro-Slip-Adaptation (Display Range: 0...1.275 A)
031,3,Upper adjustment,,from Micro-Slip-Adaptation (Display Range: 0...1.275 A)
031,4,Upper adjustment,,from Macro-Slip-Adaptation (Display Range: 0...1.275 A)
;
040,1,Flash,Check-Sum
;
041,1,Parameter,identifier
;
042,0,Mantissa
042,1,Software,parameter 1
042,2,Software,parameter 2
042,3,Software,parameter 3
042,4,Software,parameter 4
;
043,0,Mantissa
043,1,Software,parameter 5
043,2,Software,parameter 6
043,3,Software,parameter 7
043,4,Software,parameter 8
;
044,0,Mantissa
044,1,Software,parameter 9
044,2,Software,parameter 10
;
045,0,Exponent
045,1,Software,parameter 1
045,2,Software,parameter 2
045,3,Software,parameter 3
045,4,Software,parameter 4
;
046,0,Exponent
046,1,Software,parameter 5
046,2,Software,parameter 6
046,3,Software,parameter 7
046,4,Software,parameter 8
;
047,0,Exponent
047,1,Software,parameter 9
047,2,Software,parameter 10
;
048,1,Software,identifier,DQ250
;
050,1,Selector Lever,Part Number (E313)
; character  1...12 - part number
; character 16      - programmable (0 or 1)
; character 18...19 - program version
; character 21...22 - data version
;
051,0,Internal Mulfunction-ID's
051,1,internal,Malfunction-ID #0,Display Range: 0...65536
051,2,internal,Malfunction-ID #1,Display Range: 0...65536
051,3,internal,Malfunction-ID #2,Display Range: 0...65536
051,4,internal,Malfunction-ID #3,Display Range: 0...65536
;
052,0,Internal Mulfunction-ID's
052,1,internal,Malfunction-ID #4,Display Range: 0...65536
052,2,internal,Malfunction-ID #5,Display Range: 0...65536
052,3,internal,Malfunction-ID #6,Display Range: 0...65536
052,4,internal,Malfunction-ID #7,Display Range: 0...65536
;
052,0,Internal Mulfunction-ID's
053,1,internal,Malfunction-ID #8,Display Range: 0...65536
053,2,internal,Malfunction-ID #9,Display Range: 0...65536
053,3,internal,Malfunction-ID #10,Display Range: 0...65536
053,4,internal,Malfunction-ID #11,Display Range: 0...65536
;
054,1,SV-Parameter
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test number
;
082,0,Flash-Tool-Code (FTC)
; Flash-Date (in dd.mm.yy)
; Hardware subassembly
; Software subassambly
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine
125,2,Brake Electronics
125,3,Instrument Cluster
125,4,Selector Lever
;
126,0,CAN-Databus Communication (Powertrain)
126,1,CAN-Gateway
126,2,Steering Column,Control Module
;
225,0,CAN-Databus Timeouts (Powertrain)
225,1,Engine
225,2,Brake Electronics
225,3,Instrument Cluster
225,4,Selector Lever
;
226,0,CAN-Databus Timeouts (Powertrain)
226,1,CAN-Gateway
226,2,Steering Column,Control Module
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,6-Speed Direct-Selection-Gearbox (02E) Coding
C01,0000020 = Standard
;
