;
; VCDS Label File
;
; Copyright © 2007-2011 Ross-Tech, LLC
;
; Audi A3 (8L) / VW Golf IV (1J) / VW New Beetle (1C/9C/1Y)
;
; Component: J104 - Brake Electronics (#03) - MK20 ESP FWD
;
; P/N: 1J0-907-37?-???
;
; includes measuring blocks, basic setting, login and misc
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1J-03.LBL
; 1J0-907-37x-ABS.LBL   (MK20 ABS)
; 1J0-907-37x-ESP-A.LBL (MK20 ESP AWD)
; 1J0-907-37x-ESP-F.LBL (MK20 ESP FWD)
;
; created on 04/Mar/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 14/Sep/2011
;
; requires VCDS 11.2.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Range: 0.0...255.0 km/h
;
B001,0,Brake Pump Bleeding
B001,1,Status &,Instructions, 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Starting Wheel Speed
002,1,Speed Sensor,Front Left (G47),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,2,Speed Sensor,Front Right (G45),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,3,Speed Sensor,Rear Left (G46),Range: 0.0...254.0 km/h (255.0 km/h = standing)
002,4,Speed Sensor,Rear Right (G44),Range: 0.0...254.0 km/h (255.0 km/h = standing)
;
003,0,Switches
003,1,Brake Light,Switch (F),Range: not oper./operated
003,2,Brake Recognition,Switch (F83),Range: not oper./operated
;
004,0,Steering Angle / Lateral Acceleration / Rotation Rate
004,1,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
004,2,Lateral Acc.,Sensor (G200),Specification: ± 0.5 m/s²
004,3,Rotation Rate,,Specification: ± 2.5 °/s
;
005,0,Brake Pressure
005,1,Brake Pressure,Sensor,Specification: ±7 bar
005,2,Brake Pressure,Sensor,Specification: ±7 bar
;
B060,0,Adjustment of Steering Angle Sensor (G85)
B060,1,Adjustment, , 
B060,2,Adjustment,Status, 
B060,3,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±4.5 °
;
B063,0,Adjustment of Lateral Acceleration Sensor (G200)
B063,1,Adjustment, , 
B063,2,Adjustment,Status, 
B063,3,Lateral Acc.,Sensor (G200),Specification: ± 2.5 m/s²
;
B066,0,Adjustment of Brake Pressure Sensor (G201)
B066,1,Adjustment, , 
B066,2,Adjustment,Status, 
B066,3,Brake Pressure,Sensor (G201),Specification: ± 7.0 bar
;
B093,0,Activate ESP System/Function Test
B093,1,System/Function,Test
B093,2,System/Function,Test Status
B093,3, , , 
B093,4, , , 
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Range: Engine 1/Engine 0\nSpecification: Engine 1
125,2,Steering Angle,Sensor (G85),Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Engine,,Range: Engine 1/Engine 0\nSpecification: Engine 1
225,2,Steering Angle,Sensor (G85),Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104/MK20 ESP FWD) Coding
C01,18952 = Ford Galaxy (7M)/Seat Alhambra (7M)/VW Sharan (7M)
C02, 
C03,Note: For all other Models please contact your local VCDS
C04,Distributor or send an Email to Support@Ross-Tech.com
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Brake Electronics (J104) Login
L01,40168 = Basic Setting Enabling
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
SN,MK20 ESP FWD
;
