;
; VCDS Label File
;
; Copyright © 2012 Ross-Tech, LLC
;
; VW Phaeton (3D)
;
; Component: J400 - Wiper Electronics (#68)
;
; T/N: 3D1-955-119-???
;
; includes measuring blocks
;
; created on 01/Jan/2012 by Jason Young (jyoung8607@gmail.com)
; updated on 26/Jan/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 26/Jan/2012
;
; requires VCDS 11.11.2 / LCode 1.0.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
;
001,0,Wiper Control Status
001,1,Wiper Switch,Status,0000000 = Wiper Switch not operated\nxxxxxxx1 = Wiper Switch - Single Wipe\nxxxxxx1x = Wiper Switch - Interval 0/Rain Sensor\nxxxxx1xx = Wiper Switch - Interval Level 1 (Slow)\n; xxxx1xxx = Wiper Switch - Interval Level 2 (Fast)xxx1xxxx = Wiper Switch - Washer Request\nxx1xxxxx = Washer Pump active\nx1xxxxxx = Wiper Switch - Intermittent Speed +1 (Stalk @ 1 / Dial @ 1)\n1xxxxxxx = Wiper Switch - Intermittent Speed +2 (Stalk @ 1 / Dial @ 2)
; 00000000 = Wiper Switch not operated
; xxxxxxx1 = Wiper Switch - Single Wipe
; xxxxxx1x = Wiper Switch - Interval 0/Rain Sensor
; xxxxx1xx = Wiper Switch - Interval Level 1 (Slow)
; xxxx1xxx = Wiper Switch - Interval Level 2 (Fast)
; xxx1xxxx = Wiper Switch - Washer Request
; xx1xxxxx = Washer Pump active
; x1xxxxxx = Wiper Switch - Intermittent Speed +1 (Stalk @ 1 / Dial @ 1)
; 1xxxxxxx = Wiper Switch - Intermittent Speed +2 (Stalk @ 1 / Dial @ 2)
001,2,Status Bits 2,,x1xx = Wipe required due Rain Sensor Input
; x1xx = Wipe required due Rain Sensor Input
;
001,3,Ignition Status,(Terminal 15),Range: Terminal 15 ON/ Terminal 15 OFF
001,4,Vehicle Speed,,Range: 0.0...300.0 km/h
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification I
;
128,0,Wiper Control Status
128,1,Status Bits 3,,x1 = Wiper Service Position Request from Infotainment\n1x = Wiper Normal Operation
; x1 = Wiper Service Position Request from Infotainment
; 1x = Wiper Normal Operation
;
128,3,Starter Status,(Terminal X),Range: Terminal X ON/ Terminal X OFF
;
