;
; VCDS Label File
;
; Copyright © 2009-2010 Ross-Tech, LLC
;
; Audi A3 (8P) / Seat Altea/Toledo (5P) / Seat Leon (1P)
; Skoda Octavia II (1Z) / VW Caddy (2K) / VW Golf/Jetta (1K)
; VW Touran (1T)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 1K0-953-549-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1K-16.LBL
; 1K0-953-549-MY8.LBL (< SW 0101)
; 1K0-953-549-MY9.LBL (SW 0110 >)
;
; includes measuring blocks, coding and selective output test
;
; created on 22/Mar/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 11/Nov/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic settings
;
;---------------------------------------------------
;
;
001,1,Blinker,,Display Range: n. operated/left/right
001,2,Headlamp Flasher,,Display Range: n. operated/operated
001,3,High Beam,,Display Range: n. operated/operated
001,4,Front Wiper,,Display Range: n. operated/level/Stage Int./Stage 1/Stage 2
;
002,1,Interval Stages,,Display Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Display Range: n. operated/operated
002,3,Wiping Rear,,Display Range: n. operated/operated/not installed
002,4,Washing Rear,,Display Range: n. operated/operated/not installed
;
003,1,Terminal Status,,?xxxx - P-Contact\nx?xxx - S-Contact\nxx?xx - Terminal 75\nxxx?x - Terminal 15\nxxxx? - Terminal 50
003,2,Horn,,Display Range: n. operated/operated
003,3,Multi-Function,Display,Display Range: n. installed/n. operated/Reset/Up/Down
;
004,0,Cruise-Cntrol-System
004,1,Main Switch,,Display Range: n. installed/off/on
004,2,CCS-Set,,Display Range: n. operated/decelerate/accelerate/Reset
;
005,1,Park Position in,Selector Lever,Display Range: n. installed/n.Ok/on/recognized
005,2,Selector Lever,Information (Pos. P),Display Range: n. defined/recognized/on
005,3,Key,Removal Lock,Display Range: n. installed/on/off
005,4,Status Key,Removal Lock,Display Range: n. installed/Ok/n.Ok
;
006,0,Multi-Function Steering Wheel
006,1,Communication,,Display Range: n. intalled/Ok/n.Ok
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Display Range: yes/no
;
007,0,Multifunction Steering Wheel II
007,1,Vehicle Type
; 0 = Volkswagen
; 1 = Audi
; 2 = Seat
; 3 = Skoda
; 4 = Volkswagen Nutzfahrzeuge
; 5 = Bugatti
; 6 = Lamborghini
; 7 = Bentley
; 8 = Rolls Royse
; 14 = Ford
; 15 = Porsche
007,2,Vehicle Version
;
008,0,Multifunction Steering Wheel III
008,3,Tiptronic,(Down),Display Range: Not Installed/Not Oper./Operated
008,4,Tiptronic,(Up),Display Range: Not Installed/Not Oper./Operated
;
010,0,Heated Steering Wheel && Heated Seats
010,1,Steering Wheel,Heater,Display Range: Not Installed/OFF/ON\nSignal Type: Output
010,2,Temperature,,Display Range: Not Installed/Temperature\nSignal Type: Input
010,3,Steering Wheel,Heater Output,Signal Type: Output
010,4,Heated Seats,,Display Range: OFF/Stage\nSignal Type: Input
;
011,0,Dimming
011,1,Dimming,,Display Range: 0.0...100.0 %\nSignal Type: Input
011,2,Dimming,(Discrete),Display Range: 0.0...100.0 %\nSignal Type: Input
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,0?xxxxx: Driver-Assistance-Systems
C02,0 = Driver-Assistance-Systems not installed
;0 = Message for Driver-Assistance-Systems active w/o Button
;1 = Message for Driver-Assistance-Systems inactive w/o Button
;2 = Message for Driver-Assistance-Systems active with Button
;3 = Message for Driver-Assistance-Systems inactive with Button
C03,0x?xxxx: Vehicle Type
C04,0 = Normal
C05,1 = Special Purpose with Multi-Function Control Module (Steer. Column. Contr. Mod. as Master)
C06,2 = Special Purpose with Multi-Function Control Module (Multi-Function Contr. Mod. as Master)
C07,0xx?xxx: Transmission
C08,0 = Manual Transmission / 1 = Automatic Transmission
C09,0xxx?xx: Multi-Function Steering Wheel (1-4 = LIN 1.3 / 5-8 = LIN 2.0)
C10,0 = Multi-Function Steering Wheel not installed
C11,1 OR 5 = Multi-Function Steering Wheel w/o Tiptronic and w/o Push-To-Talk (PTT) installed
C12,2 OR 6 = Multi-Function Steering Wheel with Tiptronic and no Push-To-Talk (PTT) installed
C13,3 OR 7 = Multi-Function Steering Wheel w/o Tiptronic and with Push-To-Talk (PTT) installed
C14,4 OR 8 = Multi-Function Steering Wheel with Tiptronic and with Push-To-Talk (PTT) installed
C15,0xxxx?x: Cruise Control System (CCS) and Adaptive Cruise Control (ACC)
C16,0 = Cruise Control System (CCS) not installed
C17,1 = Cruise Control System (CCS) with 6 Positions via separate Stalk installed
;2 = Adaptive Cruise Control (ACC) with 6 Positions installed
C18,3 = Cruise Control System (CCS) with 4 Positions via Blinker Stallk installed
;4 = Cruise Control System (CCS) via Multi-Function Steering Wheel installed
;5 = Adaptive Cruise Control (ACC) via Multi-Function Steering Wheel installed
C19,0xxxxx?: Rear Wiper and Board Computer
C20,1 = Rear Wiper not installed / Board Computer via Wiper Stalk not installed
C21,2 = Rear Wiper installed / Board Computer via Wiper Stalk not installed
C22,3 = Rear Wiper not installed / Board Computer via Wiper Stalk verbaut
C23,4 = Rear Wiper installed / Board Computer via Wiper Stalk installed
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T194,Ignition Key Removal Lock
;
