;
; VAG-COM Label File
;
; Audi A6 (4F)
;
; component: J393 - Central Convenience (#46)
;
; p/n: 4F0-910-289-???
;
; includes measuring blocks, adaptation and coding and selective output tests
;
; created on 27/Jun/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 30/May/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
;
001,0,Status - Driver's Door
001,1,Door Contact,Switch,Display Range: Door Open/Door Closed/no communication
001,2,Central Locking,Interior Button,Display Range: locking/unlocking/not operated/no communication
001,3,Lock Feedback,,Display Range: locked/unlocked/no communication
001,4,Safe Feedback,,Display Range: safe/not safe/no communication
;
002,0,Status - Passenger Door
002,1,Door Contact,Switch,Display Range: Door Open/Door Closed/no communication
002,2,Central Locking,Interior Button,Display Range: locking/unlocking/not operated/no communication
002,3,Lock Feedback,,Display Range: locked/unlocked/no communication
002,4,Safe Feedback,,Display Range: safe/not safe/no communication
;
003,0,Status - Rear Left Door
003,1,Door Contact,Switch,Display Range: Door Open/Door Closed/no communication
003,2,Central Locking,Interior Button,Display Range: locking/unlocking/not operated/no communication
003,3,Lock Feedback,,Display Range: locked/unlocked/no communication
003,4,Safe Feedback,,Display Range: safe/not safe/no communication
;
004,0,Status - Rear Right Door
004,1,Door Contact,Switch,Display Range: Door Open/Door Closed/no communication
004,2,Central Locking,Interior Button,Display Range: locking/unlocking/not operated/no communication
004,3,Lock Feedback,,Display Range: locked/unlocked/no communication
004,4,Safe Feedback,,Display Range: safe/not safe/no communication
;
005,0,Window Regulators && Shut-Off Buttons
005,1,Window Regulator,standardized,1 = standardized\n0 = not standardized\n\n?xxx - Driver's Door\nx?xx - Passenger Door\nxx?x - Rear Left Door\nxxx? - Rear Right Door
005,2,Window Regulator,Thermal Protection,1 = active\n0 = not active\n\n?xxx - Driver's Door\nx?xx - Passenger Door\nxx?x - Rear Left Door\nxxx? - Rear Right Door
005,3,Interior Monitoring,Shut-Off Button,Display Range: operated/not operated/no communication
005,4,Inclination Sensor,Shut-Off Button,Display Range: operated/not operated/no communication
;
006,0,Rear Lid && Rear Window
006,1,Rear Lid Switch,(Driver's Door),Display Range: operated/not operated/no communication
006,2,Rear Lid,Contact Switch,Display Range: lid open/lid closed
006,3,Rear Lid,Soft Touch,Display Range: operated/not operated
006,4,Rear Window,Break,Anti-Theft-System\n\nDisplay Range: not recognized/recognized/not installed
;
007,1,Enabling,Sunroof,Display Range: ON/OFF
007,2,Luggage,Compartment Light,Display Range: ON/OFF
007,3,Interior Light,,Display Range: ON/OFF
007,4,Rear Lid,Key Switch,Display Range: open/closed/not operated
;
008,0,Basic Functions
008,1,Speed Signal
008,2,Engine Speed
008,3,Interior,Temperature
008,4,Fuel Filler,Flap Detection,Display Range: not recognized/recognized/not installed
;
009,0,Terminal Status
009,1,S-Terminal,,Display Range: on/off/no communication
009,2,Terminal 15,(hardware input),Display Range: Term. 15 On/Term. 15 Off
009,3,Terminal 15,(CAN),Display Range: Term. 15 On/Term. 15 Off/no communication
;
010,1,Terminal 30,(right),Specification: 8.5...15.5 V
010,2,Terminal 30,(left),Specification: 8.5...15.5 V
010,3,Rear Window,Heater,Display Range: heater on/heater off
010,4,Hood Contact,Switch,Display Range: lid open/lid closed/no communication
;
011,0,Light Status
011,1,Back-Up Light,,?x - left\nx? - right
011,2,Turn Signal,,?x - left\nx? - right
011,3,Fog Light,,?x - left\nx? - right
011,4,Tail Light,,?x - left\nx? - right
;
012,1,Terminal 54,,?xx - Hardware Terminal 54\nx?x - Terminal 54 CAN\nxx? - Brake Test Switch
012,2,Brake ESP,,?x - Hardware ECD Brake\nx? - CAN ECD Brake
012,3,Brake light,,?xx - left\nx?x - center\nxx? - right
012,4,Garage Door,Opener,Display Range: ON/OFF
;
013,1,Rear Window,Shaded,Display Range: ON/OFF/not installed
013,2,Luggage Compartment,Closing Aid,Display Range: locked/unlocked/not insalled
013,3,Crash,Recognized,Display Range: Yes/No
013,4,Energy Manager,Shut-Off Stage,Display Range: 0...6
;
014,0,Interior Monitoring Sensor
014,1,Interior Monitoring,Sensor Status,Display Range: not installed/no communication/activated/inactive
;
015,0,Alarm Horn
015,1,Alarm Horn,Status,Display Range: not installed/no communication/activated/inactive
;
016,0,Alarm Sources
016,1,Last,Alarm Source,0 = Door contact (driver's door)\n1 = Door contact (passenger door)\n2 = Door contact (rear left)\n3 = Door contact (rear right)
016,2,2nd last,Alarm Source,4 = Hood contact\n5 = Rear lid contact\n6 = Terminal 15\n7 = Interior monitoring\n8 = non-authorized key
016,3,3rd last,Alarm Source,9 = Intelligent siren\n10 = Inclination sensor\n11 = Driver door control module\n12 = Passenger door control module
016,4,4th last,Alarm Source,13 = Left rear door control module\n14 = Right rear door control module\n15 = Rear window breakage\n255 = no alarm source
;
018,0,Horn - Alarm Trigger
018,1,Last,Alarm Trigger,0 = no alarm trigger\n1 = alarm trigger by J393\n2 = communication break (ground/open circuit)\n3 = voltage supply (open circuit)
018,2,2nd last,Alarm Trigger,0 = no alarm trigger\n1 = alarm trigger by J393\n2 = communication break (ground/open circuit)\n3 = voltage supply (open circuit)
018,3,3rd last,Alarm Trigger,0 = no alarm trigger\n1 = alarm trigger by J393\n2 = communication break (ground/open circuit)\n3 = voltage supply (open circuit)
018,4,Alarm Trigger,Counter,Display Range: 0...15
;
019,0,Interior Monitoring - Alarm Trigger
019,1,1st Alarm Trigger,,0 = no alarm\n1 = alarm with vehicle closed\n2 = alarm at window open\n3 = alarm with fan operation
019,2,2nd Alarm Trigger,,0 = no alarm\n1 = alarm with vehicle closed\n2 = alarm at window open\n3 = alarm with fan operation
019,3,3rd Alarm Trigger,,0 = no alarm\n1 = alarm with vehicle closed\n2 = alarm at window open\n3 = alarm with fan operation
019,4,4th Alarm Trigger,,0 = no alarm\n1 = alarm with vehicle closed\n2 = alarm at window open\n3 = alarm with fan operation
;
020,1,FPI User ID
020,2,Key Number,(Keyless Entry)
020,3,Rear Lid,Position,Display Range: 0...100 % / not installed
;
;
;---------------------------------------------------
;
; Coding Informations
;
;---------------------------------------------------
;
;
C00,Comfort System (J393) Coding
C01,+0000001 = Reserved (always)
C02,+0000002 = 10 Tamper Alarms (PR-B09)
C03,+0000004 = Thatcham inactive (PR-7AA/A8U)
C04,+0000008 = Selective Central Locking (PR-4K2/4K7/4K8)
C05,+0000016 = Anti-Theft Warning System (PR-7AN/7AL)
C06,+0000032 = Inclination Sensor installed (PR-7AN/7AL)
C07,+0000064 = Interior Monitoring (PR-7AL)
C08,+0000128 = Comfort Function via Remote (NOT PR-B29/B30/B34/B35)
C09,+0000256 = Right Hand Steering (PR-L0R)
C10,+0000512 = Avant (PR-K8D)
C11,+0001024 = Electrical Rear Shades installed (PR-3Y2/3Y5)
C12,+0002048 = Confirmation Anti-Theft System via Horn (PR-A8U)
C13,+0004096 = SAE Rear Lights (PR-A8U)
C14,+0008192 = Light Package (PR-QQ1)
C15,+0016384 = SAFE-Function deactivated (PR-A8U)
C16,+0065536 = No Anti-Theft Delay (0 Seconds)
C17,+0131072 = Highline (LED Rear Lights)
C18,+0262144 = Sunroof (PR-3FE/3FR)
;   +0524288 = Multi Function Module (PR-F0X/F4E/F4F/F4G/F4J/F4Q/F4X/F4Z/F5F)
C19,+1048576 = Luggage Compartment Closing Assistance (PR-4E7/4E9)
C20,+2097152 = Rear Lid Control Module (PR-4E7/4E9)
;   +4194304 = Fuel Lid Unlock via Driver Door Button
;
;
;---------------------------------------------------
;
; Adaptation Informations
;
;---------------------------------------------------
;
;
A001,0,Personalization - Key 1
A001,5,Personalization - Key 1
A001,6,+00001 = Passenger Door
A001,7,+00002 = Rear Left Door
A001,8,+00004 = Rear Right Door
A001,9,+00008 = Luggage Compartment
A001,10,+00016 = Auto-Lock/Unlock
A001,11,+00032 = Comfort Opening of Front Window Regulators
A001,12,+00064 = Comfort Opening of Rear Window Regulators
A001,13,+00128 = Comfort Opening of Sunroof
A001,14,+00256 = Rear Shade automatic
A001,15,+00512 = Interior Light Dimming 1 %
A001,16,+01024 = Interior Light Dimming 2 %
A001,17,+02048 = Interior Light Dimming 4 %
A001,18,+04096 = Interior Light Dimming 8 %
A001,19,+08192 = Interior Light Dimming 16 %
A001,20,+16384 = Interior Light Dimming 32 %
A001,21,+32768 = Interior Light Dimming 64 %
;
A002,0,Personalization - Key 2
A002,5,Personalization - Key 2
A002,6,+00001 = Passenger Door
A002,7,+00002 = Rear Left Door
A002,8,+00004 = Rear Right Door
A002,9,+00008 = Luggage Compartment
A002,10,+00016 = Auto-Lock/Unlock
A002,11,+00032 = Comfort Opening of Front Window Regulators
A002,12,+00064 = Comfort Opening of Rear Window Regulators
A002,13,+00128 = Comfort Opening of Sunroof
A002,14,+00256 = Rear Shade automatic
A002,15,+00512 = Interior Light Dimming 1 %
A002,16,+01024 = Interior Light Dimming 2 %
A002,17,+02048 = Interior Light Dimming 4 %
A002,18,+04096 = Interior Light Dimming 8 %
A002,19,+08192 = Interior Light Dimming 16 %
A002,20,+16384 = Interior Light Dimming 32 %
A002,21,+32768 = Interior Light Dimming 64 %
;
A003,0,Personalization - Key 3
A003,5,Personalization - Key 3
A003,6,+00001 = Passenger Door
A003,7,+00002 = Rear Left Door
A003,8,+00004 = Rear Right Door
A003,9,+00008 = Luggage Compartment
A003,10,+00016 = Auto-Lock/Unlock
A003,11,+00032 = Comfort Opening of Front Window Regulators
A003,12,+00064 = Comfort Opening of Rear Window Regulators
A003,13,+00128 = Comfort Opening of Sunroof
A003,14,+00256 = Rear Shade automatic
A003,15,+00512 = Interior Light Dimming 1 %
A003,16,+01024 = Interior Light Dimming 2 %
A003,17,+02048 = Interior Light Dimming 4 %
A003,18,+04096 = Interior Light Dimming 8 %
A003,19,+08192 = Interior Light Dimming 16 %
A003,20,+16384 = Interior Light Dimming 32 %
A003,21,+32768 = Interior Light Dimming 64 %
;
A004,0,Personalization - Key 4
A004,5,Personalization - Key 4
A004,6,+00001 = Passenger Door
A004,7,+00002 = Rear Left Door
A004,8,+00004 = Rear Right Door
A004,9,+00008 = Luggage Compartment
A004,10,+00016 = Auto-Lock/Unlock
A004,11,+00032 = Comfort Opening of Front Window Regulators
A004,12,+00064 = Comfort Opening of Rear Window Regulators
A004,13,+00128 = Comfort Opening of Sunroof
A004,14,+00256 = Rear Shade automatic
A004,15,+00512 = Interior Light Dimming 1 %
A004,16,+01024 = Interior Light Dimming 2 %
A004,17,+02048 = Interior Light Dimming 4 %
A004,18,+04096 = Interior Light Dimming 8 %
A004,19,+08192 = Interior Light Dimming 16 %
A004,20,+16384 = Interior Light Dimming 32 %
A004,21,+32768 = Interior Light Dimming 64 %
;
A015,0,Interior Monitoring Sensitivity
A015,5,Interior Monitoring Sensitivity
A015,6,200 = 100 %
A015,7,180 = 90 %
A015,8,160 = 80 %
A015,9,140 = 70 %
A015,10,120 = 60 %
A015,11,100 = 50 %
;
A050,0,Adaptive Brake Light
A050,5,Adaptive Brake Light
A050,6,+1 = Emergency Brake Blinking
A050,7,+2 = Brake Light Surface Amplification (only Sedan)
;
A061,0,Comfort Functions
A061,5,Comfort Functions
A061,6,+001 = Comfort Closing: Window Regulators via Remote Control
A061,7,+002 = Comfort Opening: Window Regulators via Remote Control
A061,8,+004 = Comfort Closing: Sunroof via Remote Control
A061,9,+008 = Comfort Opening: Sunroof via Remote Control
A061,10,+016 = Comfort Closing: Window Regulator via Switch Drivers Door
A061,11,+032 = Comfort Opening: Window Regulator via Switch Drivers Door
A061,12,+064 = Comfort Closing: Sunroof via Switch Drivers Door
A061,13,+128 = Comfort Opening: Sunroof via Switch Drivers Door
A061,14,+256 = Comfort Closing: Window Regulators via Lock Cylinder
A061,15,+512 = Comfort Closing: Sunroof via Lock Cylinder
;
A062,0,Central Locking Functions
A062,5,Central Locking Functions
A062,6,+1 = Central Locking Closing Confirmation (Blink)
A062,7,+2 = Central Locking Opening Confirmation (Blink)
A062,8,+4 = Terminal 87 USA Logic
;
;
;---------------------------------------------------
;
; Selective Output Test Informations
;
;---------------------------------------------------
;
;
T0959,Warning light for central locking (SAFE) -K133- max. 30 seconds
T1551,Lock central locking signal (once)
T1148,Activation of safe-locks of doors (once)
T1223,Signal open central locking
T2615,Locking fuel filler flap
T2616,Unlocking fuel filler flap
T0987,Left Brake Light -M9- (max. 30 seconds)
T0988,Right Brake Light -M10- (max. 30 seconds)
T1503,High-mount Brake Light -M9- (max. 30 seconds)
T1828,Left Tail Light -M4- (max. 30 seconds)
T0042,Left Parking Light Lamp -M43- (max. 30 seconds)
T1829,Right Tail Light -M2- (max. 30 seconds)
T0043,Right Parking Light Lamp -M44- (max. 30 seconds)
T1518,Left Back-Up Light -M16- (max. 30 seconds)
T1519,Right Back-Up Light -M17- (max. 30 seconds)
T1501,Rear Left Turn Signal Light -M6- (max. 30 seconds)
T1505,Rear Right Turn Signal Light -M8- (max. 30 seconds)
T1502,Rear Left Fog Light -L46- (max. 30 seconds)
T1506,Rear Right Fog Light -L47- (max. 30 seconds)
T1504,License Plate Light -X- (max. 30 seconds)
T1565,Luggage compartment Light -W3- (max. 30 seconds)
T1696,Rear Left Footwell Light -W45- (max. 30 seconds)
T1697,Rear Right Footwell Light -W46- (max. 30 seconds)
T1483,Actuation of rear lid release (rotary latch opens/power latch rises)
T2106,Rear Window Shades
T0834,Signal for actuation of heated rear window (max. 30 seconds)
T2570,Interior lighting (interior light switch must be in AUTO position) (max. 30 seconds)
T2899,Sunroof comfort opening (can only be activated as of software version 0120) 
T2900,Sunroof comfort closing (can only be activated as of software version 0120) 
;
