;
; VAG-COM label file
;
; VW Passat (3B)
;
; component: Engine (#01) - BHW
;
; p/n: 038-906-016-???
;
; includes measuring blocks, coding and readiness
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 03-01.LBL
; 038-906-016-BHW.LBL  (2.0l TDI  @ 136 HP - BHW)
;
; created on 24/Jun/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 24/Apr/2008
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; Measuring Block Information
;
;---------------------------------------------------
;
;
001,0,Basic Functions - Injection Quantity
001,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
001,2,Injection,Quantity,Specification (Idle): 3...9 mg/str
001,3,Supply Duration,,Specification (Idle): 3...9 °KW
001,4,Coolant,Temperature (G62),Specification: 80...110 °C
;
002,0,Basic Informations - Idle Speed
002,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
002,2,Throttle Position,Sensor,Specification: 0 %
002,3,Operating,Conditions
002,4,Coolant,Temperature (G62),Specification: 80...110 °C
;
003,0,Basic Functions - Exhaust Gas Recirculation (EGR)
003,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
003,2,Mass Air Flow,(specified),Specification: 200...280 mg/str
003,3,Mass Air Flow,(actual),Specification: 180...300 mg/str
003,4,EGR,Duty Cycle,Specification: 20...75 %
;
004,0,Basic Functions - Injection Timing
004,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
004,2,Injection Start,,Specification: +4.0...-2.0 °KW
004,3,Injection Duration,,Specification: 3...9 °KW
004,4,Torsion Value,,Specification: -3...+3 °KW
;
005,0,Basic Functions - Start Conditions
005,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
005,2,Injection Quantity,,Specification: 7...19 mg/str
005,3,Synchronization,,Specification: 000...128
005,4,Coolant,Temperature (G62),Specification: 80...110 °C
;
006,0,Basic Functions - Switch Positions
006,1,Vehicle Speed,,Specification: 0...300 km/h
006,2,Switch Positions
; xxxxxxx1 = Brake Light Switch operated
; xxxxxx1x = Brake Pedal Switch operated
; xxxxx1xx = Clutch Pedal Switch operated
; xxxx1xxx = CCS enabled
; xxx1xxxx = ACC enabled
; xx1xxxxx = Main Button
; 00xxxxxx = ACC/CCS Mode inactive
; 10xxxxxx = Status surpassed
; 01xxxxxx = ACC/CCS in Range
; 11xxxxxx = ACC not enabled
006,3,Throttle Position,Sensor,Specification: 0 %
006,4,Cruise Control,Status
; xxxxxxx1 = Stuck ON
; xxxxxx1x = Pressed OFF
; xxxxx1xx = Decelerate (-)
; xxxx1xxx = Accelerate (+)
; xxx1xxxx = Set (SET)
; xx1xxxxx = Resume (RESET)
; 1xxxxxxx = Stuck ON (Hardware)
;
007,0,Basic Functions - Temperatures
007,1,Fuel Temperature,(G81),Specification: 20...95 °C (~ Ambient Temperature)
007,2,Fuel Cooling,Status,100 % = ON\n0 % = OFF
007,3,Intake Air,Temperature (G72),Specification: 5...80 °C
007,4,Coolant,Temperature (G62),Specification: 80...110 °C
;
008,0,Basic Functions - Injection Quantity Limitation
008,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
008,2,Driver Intention,Torque,Specification: -5...0 Nm
008,3,Torque Limitation,,Specification: 140...240 Nm
008,4,Smoke Limitation,,Specification: 100...200 Nm
;
009,0,Basic Functions - Injection Quantity Limitation
009,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
009,2,Desired Torque,Cruise Control
009,3,Transmission,Intervention Torque,Specification: 380...480 Nm
009,4,Torque Restriction,,Specification: 100...200 Nm
;
010,0,Air System
010,1,Mass Air Flow,(actual),Specification: 180...300 mg/str
010,2,Atmospheric,Pressure,Specification: 900...1100 mbar
010,3,Intake Manifold,Pressure (actual),Specification: 900...1150 mbar
010,4,Throttle Position,Sensor,Specification: 0 %
;
011,0,Charge Pressure Control
011,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
011,2,Intake Manifold,Pressure (spec.),Specification: 900...1150 mbar
011,3,Intake Manifold,Pressure (actual),Specification: 900...1150 mbar
011,4,Charge Pressure,Valve (N75),Specification: 40...90 %
;
012,0,Glow Plugs
012,1,Glow Status,,See Label File
; 11111111 = Glowing OFF
; 00010000 = Pre-Glow
; 01110000 = Glow Start
; 11110000 = Interim Glow
; 10110000 = Post-Glow
; 00110000 = Readiness Glowing
012,2,Pre-Glow Period,,Specification: 0...2 s
012,3,Battery Voltage,,Specification: 13.0...15.0 V
012,4,Coolant,Temperature (G62),Specification: 80...110 °C
;
013,0,Idle Stabilization
013,1,Injection Quantity,Cylinder 1,Specification: -2.8...+2.8 mg/str
013,2,Injection Quantity,Cylinder 2,Specification: -2.8...+2.8 mg/str
013,3,Injection Quantity,Cylinder 3,Specification: -2.8...+2.8 mg/str
013,4,Injection Quantity,Cylinder 4,Specification: -2.8...+2.8 mg/str
;
015,0,Fuel Consumption
015,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
015,2,Engine Torque,,Specification: 20...60 Nm
015,3,Fuel Consumption,,Specification: 1.0...2.0
015,4,Driver Intention,Torque,Specification: -5...0 Nm
;
016,0,Additional Heater
016,1,Generator Load,,Specification: 5...95 %
016,2,Auxiliary,Heating
; xxxxxxx1 - Coolant Temperatur ABOVE 70...80 °C OR Intake Air Temperature ABOVE 5 °C
; xxxxxx1x - Generator FAULTY
; xxxxx1xx - Battery Voltage BELOW 9 V
; xxxx1xxx - Engine Speed BELOW 800 RPM
; xxx1xxxx - Engine Start within last 10 Seconds
; xx1xxxxx - Coolant Temp. Sensor (G62) OR Intake Air Temp. Sensor (G72) FAULTY
016,3,Heating Element,Activation,1x - High Heating Output\nx1 - Low Heating Output
016,4,Battery Voltage,,Specification: 13.0...15.0 V
;
018,0,PD Injector Valve Status
018,1,Cylinder 1,Valve Status,Specification: 0
018,2,Cylinder 2,Valve Status,Specification: 0
018,3,Cylinder 3,Valve Status,Specification: 0
018,4,Cylinder 4,Valve Status,Specification: 0
;
020,0,Injection Quantity Limitation by ABS
020,1,Engine Speed,(G28),Specification (Idle): 820...900 RPM
020,2,Engine Torque,,Specification: 20...60 Nm
020,3,Limitation by ASR
020,4,Limitation by MSR
;
023,0,Switching Period
023,1,Solenoid Valve,Cylinder 1,Specification: -100...+100
023,2,Solenoid Valve,Cylinder 2,Specification: -100...+100
023,3,Solenoid Valve,Cylinder 3,Specification: -100...+100
023,4,Solenoid Valve,Cylinder 4,Specification: -100...+100
;
062,1,Coolant Temperat.,Engine Output,Specification: min. 75 °C
062,2,Coolant Temperat.,Radiator Output,Specification: max. 75 °C
062,3,Ambient,Temperature,Specification: -20.0...+50.0 °C
;
063,1,Refrigerant,Pressure (A/C ON),Specification: 5...30 bar
063,2,Load Torque,(A/C ON),Specification: 2...10 Nm
063,4,Shut-Off Status,of A/C System
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission,,Specification: Transm. 1
125,2,Brake Electronics,,Specification: ABS 1
125,3,Instrument Cluster,,Specification: Instruments 1
125,4,Airbag,,Specification: Airbag 1
;
;
;---------------------------------------------------
;
; Coding Information
;
;---------------------------------------------------
;
;
C0,Engine Control Unit (J248) Coding
C1,0050074 - Automatic Climate Control (Climatronic)
C2,0150034 - Manual Climate Control
;
;
;---------------------------------------------------
;
; readiness
;
;---------------------------------------------------
;
;
O,038-906-016-BHW
;
