;
; VCDS Label File
;
; Copyright © 2006-2009 Ross-Tech, LLC
;
; Skoda Fabia (6Y) / Skoda Fabia/Roomster (5J)
; Seat Ibiza/Toledo (6L) / VW Polo (9N)
;
; Component: J104 - Brake Electronics (#03) - Bosch 8.0 ABS/EDS/ASR/ESP
;
; P/N: 6Q0-907-37?-???
;
; includes measuring blocks, basic setting and login
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6Q-03.LBL
; 6R-03.LBL
; 6Q0-907-37x-ABS.LBL (ABS/EDS 5.7)
; 6Q0-907-37x-ASR.LBL (ABS/EDS/ASR 5.7)
; 6Q0-907-37x-ESP.LBL (ABS/EDS/ASR/ESP 5.7)
; 6R0-907-37x-ABS.LBL (ABS/EDS 8.0)
; 6R0-907-37x-ASR.LBL (ABS/EDS/ASR 8.0)
; 6R0-907-37x-ESP.LBL (ABS/EDS/ASR/ESP 8.0)
;
; created on 09/Aug/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 30/Aug/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right (G44),Range: 0.0...255.0 km/h
;
B001,0,Steering Angel Sensor (G85) Alignment
B001,1,Steering Angel,Sensor (G85), 
B001,2,Alignment, , 
B001,3,Alignment,Status,Specification: OK
B001,4, , , 
;
002,0,Button && Switch Status
002,1,Brake Test Switch,,0 = not operated\n1= operated
002,2,Brake Light Switch,,0 = not operated\n1= operated
002,3,Parking Brake,,0 = not operated\n1= operated
002,4,ESP-Button,,0 = not operated\n1= operated
;
B002,0,Brake System Bleeding
B002,1,Status, , 
B002,2, , , 
B002,3, , , 
B002,4, , , 
;
003,0,Engine Data
003,1,Engine Speed
003,2,Engine Torque
003,3,Engine Torque,(loss)
003,4,Throttle Valve Angle
;
004,1,Standing Time
004,2,EDL-T Flag,,Range: ON/OFF\nSpecification: OFF
;
005,1,Steering Angle,,Range: -720.0...+720.0 °
005,2,Rotation Rate,,Range: -69.0...+69.0 °/s
005,3,Brake Pressure,,Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
005,4,Transverse,Acceleration,Range: -25.0...+25.0 m/s²
;
006,1,Supply Voltage,(Terminal 30),Specification: 9.8...17.4 V
006,2,Valve Relay,,Display Range: ON = OK / OFF = not OK
006,3,Return Flow Pump,,Display Range: ON/OFF
006,4,Work Shop Code
;
009,1,Brake Test Switch,,0 = not operated\n1= operated
009,2,Brake Light Switch,,0 = not operated\n1= operated
009,3,Brake Pressure,,Display Range: -41.0...+292.0 bar\n40.0 bar = Short to Ground\n290.0 bar = Short to Plus
;
022,0,Steering Angle Sensor Data
;
023,0,Data Variant Coding
023,1,Data Variant,Coding
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Steering Angle,Sensor,Specification: Steer. ang. 1
125,2,Engine,,Specification: Engine 1
125,3,Transmission,,Specification: Transm. 1
125,4,Instrument Cluster,,Specification: Instruments 1
;
126,0,CAN-Databus Communication (Powertrain)
126,4,ESP Sensors,,Specification: ESP Sens. 1
;
127,0,CAN-Databus Communication (Powertrain)
127,2,Airbag,,Specification: Airbag 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Steering Angle,Sensor
225,2,Engine
225,3,Transmission
225,4,Instrument Cluster
;
226,0,CAN-Databus Time-Out (Powertrain)
226,4,ESP Sensors
;
227,0,CAN-Databus Time-Out (Powertrain)
227,2,Airbag
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Brake Electronics (J104) Login
L01,40168 = Basic Setting Enabling
;
