;
; VCDS Label File
;
; Copyright © 2011 Ross-Tech, LLC
;
; VW Transporter (7H/7J)
;
; Component: J446 - Parking Aid (#76) - 8-Channel
;
; P/N: 7E0-919-283-???
;
; includes measuring blocks, adaptation and coding
;
; created on 17/Mar/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 17/Mar/2011
;
; requires VCDS 10.6.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Distance (Front)
001,1,Front Left (G255),Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
001,2,Front Left (G254),Center Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
001,3,Front Right (G253),Center Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
001,4,Front Right (G252),Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
;
002,0,Distance (Rear)
002,1,Rear Left (G203),Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
002,2,Rear Left (G204),Center Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
002,3,Rear Right (G205),Center Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
002,4,Rear Right (G206),Sensor,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
;
003,1,Resulting,Distance Front,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
003,2,Resulting,Distance Rear,Range: 0...255 cm\n\n255 cm = No Obstacle recognized
003,3,Vehicle Speed,,Range: 0.0...255.0 km/h
003,4,Supply Voltage,(Terminal 30),Range: 0.0...20.0 V\nSpecification: 8.7...16.7 V
;
004,1,Confirm. Sound,(Reverse Gear),Range: Sound ON/Sound OFF
004,2,Reverese Gear,engaged,Range: Reverse: Yes/Reverse: No
004,3,Trailer hitched,,Range: YES/NO/Not Installed
004,4,Rear Lid,Status,Range: Tailg.close/Tailg.open
;
005,1,Parking Aid (K136),Indicator Lamp,Range: LED ON/LED OFF
005,2,Parking Aid,Button (E266),Display Range: ON/OFF/Not Oper./Not Installed
;
006,0,Oscillation Time (Front)
006,1,Front Left (G255),Sensor
006,2,Front Left (G254),Center Sensor
006,3,Front Right (G253),Center Sensor
006,4,Front Right (G252),Sensor
;
007,0,Oscillation Time (Rear)
007,1,Rear Left (G203),Sensor
007,2,Rear Left (G204),Center Sensor
007,3,Rear Right (G205),Center Sensor
007,4,Rear Right (G206),Sensor
;
080,0,Advanced Control Module Identification I
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,?xxxx: Trailer Hitch
C02,0 = Trailer Hitch not installed
C03,1 = Trailer Hitch installed
C04,x?xxx: Transmission
C05,0 = Manual Transmission
C06,1 = Automatic Transmission
C07,xx?xx: Confirmation Sound (for Reverse Gear)
C08,0 = Confirmation Sound inactive
C09,1 = Confirmation Sound active
C10,xxx?x: Chassis
C11,2 = Transporter/Multivan
C12,xxxx?: Model
C13,7 = VW Transporter/Multivan (7H)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A01,0,Rear Buzzer Volume
A01,5,Rear Buzzer Volume
A01,6,Adaptation of the Volume for the Rear Warning Buzzer.
A01,7,Changes can be checked with the Reverse Gear engaged.
A01,8, 
A01,9,Range: 1...7
;
A02,0,Rear Buzzer Frequency
A02,5,Rear Buzzer Frequency
A02,6,Adaptation of the Frequency for the Rear Warning Buzzer.
A02,7,Changes can be checked with the Reverse Gear engaged.
A02,8, 
A02,9,Range:
A02,10,0 = 500 Hz / 1 = 660 Hz / 2 = 800 Hz
A02,11,3 = 1000 Hz / 4 = 2000 Hz
;
A03,0,Front Buzzer Volume
A03,5,Front Buzzer Volume
A03,6,Adaptation of the Volume for the Front Warning Buzzer.
A03,7,Changes can be checked with the Reverse Gear engaged.
A03,8, 
A03,9,Range: 1...7
;
A04,0,Front Buzzer Frequency
A04,5,Front Buzzer Frequency
A04,6,Adaptation of the Frequency for the Front Warning Buzzer.
A04,7,Changes can be checked with the Reverse Gear engaged.
A04,8, 
A04,9,Range:
A04,10,0 = 500 Hz / 1 = 660 Hz / 2 = 800 Hz
A04,11,3 = 1000 Hz / 4 = 2000 Hz
;
