;
; VCDS Label File
;
; Copyright © 2008-2011 Ross-Tech, LLC
;
; Audi A6 (4F) / Audi A8 (4E) / Audi Q7 (4L)
;
; Component: R146 - Digital Radio (#0F) - SIRIUS
;
; P/N: 4E0-910-593-???
;
; includes measuring blocks and adaptation
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4E-0F.LBL
; 4E0-910-593-SIR.LBL
; 4E0-910-593-XM.LBL
;
; created on 29/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 26/Sep/2011
;
; requires VCDS 805.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
;
003,0,Diagnostic Wire
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
004,0,Electronic Serial Number (ESN)
004,1,Activation Code
;
005,0,Signal Status
005,1,Signal Quality,,1 = No Signal available \n2 = Too weak\n3 = OK\n4 = Optimal
005,2,Audio Signal,present,Display Range: Yes/No
;
006,0,Status
006,1,Status,(personalized),Display Range: Yes/No
006,2,Status,(subscribed),Display Range: Yes/No
006,3,Status,(activated),Display Range: Yes/No
;
008,0,Service Information
008,1,Provider,Information
; 0 = Normal Operation
; 1 = Antenna not connected
; 2 = Update enabling code
; 3 = No Signal
; 4 = Channel Change
; 5 = Channel not offered
; 6 = Channel no longer available
; 7 = Additional channel info not available
008,2,Satellite,Antenna Status,0/194 = OK\n1 = Short to Ground\n2 = Short to Plus
008,3,Terrestrial,Antenna Status,0/194 = OK\n1 = Short to Ground\n2 = Short to Plus
;
;053,1,
;0.0
;053,2,
;0.0
053,3,Regional Code,,0 = Full Program (US)\n1 = Family Program (US)\n2 = Full Program (Canada)\n3 = Family Program (Canada)\n255 = No Signal
;053,4,
;00,Bin. Bits
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
;A255,0,
;0
;
