;
; VAG-COM Label File
;
; Audi A4 (8D)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 8D?-919-???-???
;
; includes measuring blocks, adaptation, coding, login and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8D-17.LBL
; 8D0-919-0xx-17.LBL  (MY 1995-1997)
; 8D0-919-xxx-17.LBL  (MY 1998-1999)
; 8D0-920-xxx-17.LBL  (MY 2000+)
;
; created on 27/Feb/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 01/Jan/2008
;
; requires VAG-COM 610.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
;
003,0,General
003,1,Coolant,Temperature
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+01 = Brake Pad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,+16 = Navigation active 
C06,xx?xx: Country
C07,0 = Germany (D) / 1 = Europe (EU) / 2 = USA (US)
C08,3 = Canada (CDN) / 4 = Great Britain (GB)
C09,5 = Japan (JP) / 6 = Saudi Arabia (SA) / 7 = Australia (AUS) 
C10,xxx?x: Cylinder
C11,4 = 4-Cylinder
C12,6 = 6-Cylinder
C13,8 = 8-Cylinder
C14,xxxx?: Engine
C15,0 = TDI-Engine
C16,2 = 4-Cylinder and 6-Cylinder Gasoline-Engine
C17,3 = 8-Cylinder Gasoline-Engine
C18,4 = Turbo-Engine
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A02,0,Service Reminder
A02,5,Service Reminder
A02,6,Displayed Values:
A02,7,01 = Oil Service Due
A02,8,10 = Inspection Due
A02,9,11 = Oil Service and Inspection Due
A02,10, 
A02,11,New Values:
A02,12,00 = Reset Oil Service and Inspection
A02,13,01 = Reset Oil Service
A02,14,10 = Reset Inspection
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A005,0,Maximum Distance to Oil Service (OEL)
A005,5,Maximum Distance to Oil Service (OEL)
A005,6,15 = 15.000km (Standard)
A005,7, 
A005,8,Resolution: 1 = 1000 km
;
A006,0,Maximum Distance to Inspection (IN1)
A006,5,Maximum Distance to Inspection (IN1)
A006,6,30 = 30.000km (Standard)
A006,7, 
A006,8,Resolution: 1 = 1000 km
;
A007,0,Maximum Time to Inspection (IN2)
A007,5,Maximum Time to Inspection (IN2)
A007,6,37 = 370 Days (Standard)
A007,7, 
A007,8,Resolution: 1 = 10 Days
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km.
A009,11, 
A009,12,NOTE: Perform Login first.
;
A010,0,Distance to Oil Service (OEL)
A010,5,Distance to Oil Service (OEL)
A010,6,15 = 15.000km (Standard)
A010,7, 
A010,8,Resolution: 1 = 1000 km
;
A011,0,Distance to Inspection (IN1)
A011,5,Distance to Inspection (IN1)
A011,6,30 = 30.000km (Standard)
A011,7, 
A011,8,Resolution: 1 = 1000 km
;
A012,0,Time to Inspection (IN2)
A012,5,Time to Inspection (IN2)
A012,6,37 = 370 Days (Standard)
A012,7, 
A012,8,Resolution: 1 = 10 Days
;
A021,0,Immobilizer - Key Adaptation
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Maximum Distance to Oil Service (OEL),1000,km
RD,6,Maximum Distance to Inspection (IN1),1000,km
RD,7,Maximum Time to Inspection (IN2),10,Days
RD,10,Distance to Oil Service (OEL),1000,km
RD,11,Distance to Inspection (IN1),1000,km
RD,12,Time to Inspection (IN2),10,Days
;
RJ,0,0,Service Reset (OIL),,
RJ,0,1,2,10
;
RJ,1,0,Service Reset (INSP),,
RJ,1,1,2,1
;
RJ,2,0,Service Reset (OIL &  INSP),,
RJ,2,1,2,0
;
