;
; VCDS Label File
;
; Copyright © 2005-2009 Ross-Tech, LLC
;
; VW Passat (3C)
;
; Component: J519 - Central Electronics I (#09)
;
; P/N: 1K0-937-049-??? / 3C0-937-049-???
;
; includes measuring blocks, adaptation, selective output test and long coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-09.LBL
; 1T-09.LBL
; 3C-09.LBL
; 1K0-937-049-21-B.LBL
; 3C0-937-049-23-H.LBL
; 3C0-937-049-23-M.LBL
; 3C0-937-049-30-H.LBL
; 3C0-937-049-30-M.LBL
;
; created on 27/Apr/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 24/Jan/2009
;
; requires VCDS 805.0 / LCode 804.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Parking Lights
001,1,Left Front,Parking Light,Range: 0.0...100.0 %
001,2,Right Front,Parking Light,Range: 0.0...100.0 %
001,3,Left Rear,Parking Light,Range: 0.0...100.0 %
001,4,Right Rear,Parking Light,Range: 0.0...100.0 %
;
002,0,Fog Lights/Low Beams
002,1,Left Low Beam,Headlight,Range: 0.0...100.0 %
002,2,Right Low Beam,Headlight,Range: 0.0...100.0 %
002,3,Left Fog Light,,Range: 0.0...100.0 %
002,4,Right Fog Light,,Range: 0.0...100.0 %
;
003,0,Turn Signals
003,1,Left Front,Turn Signal,Range: 0.0...100.0 %
003,2,Right Front,Turn Signal,Range: 0.0...100.0 %
003,3,Left Rear,Turn Signal,Range: 0.0...100.0 %
003,4,Right Rear,Turn Signal,Range: 0.0...100.0 %
;
004,1,Left Side,Turn Signal,Range: 0.0...100.0 %
004,2,Right Side,Turn Signal,Range: 0.0...100.0 %
004,3,Left/Right,High Beam,Range: 0.0...100.0 %
004,4,Xenon-Shutter,,Range: ON/OFF
;
005,0,Brake Lights
005,1,Left,Brake Light,Range: 0.0...100.0 %
005,2,Right,Brake Light,Range: 0.0...100.0 %
005,3,Center,Brake Light,Range: 0.0...100.0 %
005,4,License Plate,Illumination,Range: 0.0...100.0 %
;
006,0,Back-Up Lights
006,1,Instrument,Illumination,Terminal 58d (Range: 0.0...100.0 %)
006,2,Left,Back-Up Light,Range: 0.0...100.0 %
006,3,Right,Back-Up Light,Range: 0.0...100.0 %
006,4,Left Rear,Fog Light,Range: 0.0...100.0 %
;
007,1,Activation Relay,Terminal 50,Range: ON/OFF
007,2,Activation Relay,Terminal 15,cockpit/engine (Range: ON/OFF)
007,3,Activation Relay,Terminal 75,Range: ON/OFF
007,4,Enabling SAD,,Range: active/inactive
;
008,1,Brightness,,Range: 0...7
008,2,Rain Quantity,,Range: 0...7
008,3,Right Rear,Fog Light,Range: 0.0...100.0 %
008,4,Footwell,Lighting,Range: 0.0...100.0 %
;
009,1,Terminal 30g,Relay,Range: ON/OFF
009,2,Dual Washer,Pump +,Range: ON/OFF
009,3,Dual Washer,Pump -,Range: ON/OFF
009,4,Heated Rear,Windshield,Range: ON/OFF
;
010,1,Horn,,Range: Operated/Not Oper.
010,2,Enabling of,Seat Heating,Range: Active/Inactive
010,3,Electric Fuel,Pump (FP) Relay,Range: ON/OFF
010,4,Headlight Washer,System Relay,Range: ON/OFF
;
011,1,LED Heated Rear,Windshield,Range: ON/OFF
011,2,LED Emergency,Flasher Button,Range: 0.0...100.0 %
011,3,LED Heated,Outside Mirror,Range: ON/OFF
011,4,Interior,Light Dimmed,Range: 0.0...100.0 %
;
012,1,Coming Home,LED,Range: ON/OFF
012,2,Heated Outside,Mirror,Range: ON/OFF
012,3,Rate Action 1,Relay Driver 1,Range: ON/OFF
012,4,Rate Action 2,Relay Driver 2,Range: ON/OFF
;
013,0,Terminals
013,1,Terminal 30,(left),Range: 0.00...17.75 V\nSpecification: 5.0...17.75 V
013,2,Terminal 30,(right),Range: 0.00...17.75 V\nSpecification: 5.0...17.75 V
013,3,Terminal 30,(ref.),Range: 0.00...17.75 V\nSpecification: 5.0...17.75 V
013,4,Terminal 31,(ref.),Range: 0.00...12.75 V\nSpecification: 0.0...1.00 V
;
014,1,Dimming,Potentiometer,Range: 0.0...100.0 %
014,2,Coming Home,Potentiometer,Range: 0.0...100.0 %
;
015,0,Terminals
015,1,Terminal 15,(Input),Range: ON/OFF
015,2,Terminal 50,(Input),Range: ON/OFF
015,3,Enabling P/N,,Range: ON/OFF
015,4,Terminal L,(Input),Range: ON/OFF
;
016,1,Light dark,,Range: dark = on/bright = off
016,2,Lights on (RLS),,Range: ON/OFF
016,3,Front Wiper,Status,Range: ON/OFF
016,4,Wiper turn-around,Position Signal,Range: Reached/Not Active
;
017,1,Light Switch,(Light off),Range: ON/OFF
017,2,Parking Light,Switch,Range: ON/OFF
017,3,Low Beam,Headlight Switch,Range: ON/OFF
017,4,AFL Light Switch,,Range: ON/OFF
;
018,1,Fog Light Switch,,Range: ON/OFF
018,2,Light Switch,Rear Fog Light,Range: ON/OFF
018,3,Brake Light Switch,,Range: ON/OFF
018,4,Back-Up,Light Switch,Range: ON/OFF
;
019,1,Emergency,Flasher Button,Range: Operated/Not Oper.
019,2,Engine Hood,,Range: Open/Closed
019,3,Heated Rear,Windshield Button,Range: Operated/Not Oper.
019,4,Heated Outside,Mirror,Range: Operated/Not Oper.
;
020,0,Backrest Recognition
020,3,Backrest,Left,Range: ON/OFF
020,4,Backrest,Right,Range: ON/OFF
;
021,0,Rotary Traps
021,1,Rotary Trap LF,,Range: ON/OFF
021,2,Rotary Trap RF,,Range: ON/OFF
021,3,Rotary Trap LR,,Range: ON/OFF
021,4,Rotary Trap RR,,Range: ON/OFF
;
022,1,Rear Lid,Main Catch,Range: ON/OFF
022,2,Heated Front,Windshield,Range: operated/n. oprated
022,3,Heated Front,Windshield Relay,Range: ON/OFF
022,4,Heated Front,Windshield LED,Range: ON/OFF
;
023,1,Rotary Light Switch,Position
023,2,Coming Home,Condition
023,3,Leaving Home,Condition
023,4,AFL Condition
;
024,1,Steering Column,Switch Information,via LIN-Databus
024,2,Terminal 15,(via LIN),Range: ON/OFF
024,3,Terminal 50,(via LIN),Range: ON/OFF
024,4,Wiper Cycle,Number (via LIN)
;
030,1,Load Management,,Range: Active/Inactive
030,2,Short-Distance,Operations
030,3,Critical,Time Fraction
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Reset Adaptation Channels
A000,5,Reset Adaptation Channels
A000,6,Reset all adaptation channels back
A000,7,to the original factory values.
;
A001,0,Coming-Home Time
A001,5,Coming-Home Time
A001,6,Time which the Coming-Home function will be active.
A001,7,Range: 10...60 Seconds
A001,8,Resolution: 10 Seconds
A001,9,Note: Only active if Byte 00 Bit 7 of Long Coding active.
;
A002,0,Leaving-Home Time
A002,5,Leaving-Home Time
A002,6,Time which the Leaving-Home function will be active.
A002,7,Range: 10...60 Seconds
A002,8,Resolution: 10 Seconds
A002,9,Note: Only active if Byte 00 Bit 5 of Long Coding active.
;
A003,0,Rear Window & Outside Mirror Heater Activation Time
A003,5,Rear Window & Outside Mirror Heater Activation Time
A003,6,Time which the Rear Window and Outside Mirror Heater will be active.
A003,7,Range: 1...254 Minutes
A003,8,Resolution: 1 Minute
;
A004,0,Headlight Washer Activation Time
A004,5,Headlight Washer Activation Time
A004,6,Range: 50...10000 ms
A004,7,Resolution: 50 ms (Adaptation Value * Resolution = Actual Value)
A004,8,Note: Only active if Byte 01 Bit 1 of Long Coding active.
;
A005,0,Footwell Lighting Dimming
A005,5,Footwell Lighting Dimming
A005,6,Range: 20...100 %
A005,7,Resolution: 1 %
A005,8,Note: Only active if Byte 00 Bit 1 of Long Coding active.
;
A006,0,Load Management
A006,5,Load Management
A006,6,Range: 0...3
A006,7,Note: Only active if Byte 02 Bit 3 of Long Coding active.
;
A007,0,Highbeam with Assistance Driving Light
A007,5,Highbeam with Assistance Driving Light
A007,6,0 = inactive
A007,7,1 = active
;
A008,0,Assistance Driving Light Activation/Deactivation Delay
A008,5,Assistance Driving Light Activation/Deactivation Delay
A008,6,Range: 0...10200 ms
A008,7,Resolution: 40 ms
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T906,Horn (H1)
T59,Interior Lighting
T61,Footwell Lights
T1504,License-Plate Light (X)
T1755,Parking Lights (E1)
T901,Back-Up Lamps
T1758,Brake Lamps
T967,Left Turn Signals
T968,Right Turn Signals
T975,Heated Rear Window (Z1)
T60,Fog Lights
T977,Low Beams (Left & Right)
T2486,High Beam
T1064,Interior Dimming (Terminal 58d)
T1259,Fuel Pump Relay (J17)
T1701,Dimmer for Interior Lighting
T2092,Enabling Heated Seat
T909,Windshield Wiper Motor (V)
T2377,Wiper: Upper Reverse Point
T156,Front Windshield Washer Pump
T2398,Rear Windshield Washer Pump
;
;
;---------------------------------------------------
;
; long coding
;
;---------------------------------------------------
;
;
LC,00,2,Footwell Lights installed
LC,00,3,Daytime Running Lights (Scandinavia) active
LC,00,4,Daytime Running Lights (North America)
LC,00,5,Assistance Driving Light & Leaving Home active
LC,00,6,Rain-/Light sensor installed
LC,00,7,Coming-Home active
LC,01,0,Rear Seat Recognition installed
LC,01,1,Headlight Washer installed
LC,01,2,Electronic Fuelpump Relay installed (Gasoline only)
LC,01,3,Rear Wiper installed
LC,01,7,Rear Wiper with Front Wiper continiously active
LC,02,0,Rear Wiper with Front Wiper intermittent active
LC,02,1,Comfort Turn Signals
LC,02,2,Cold Lamp Diagnosis active
LC,02,3,Load Management active
LC,02,4,Coming-Home Mode via (0 = Personalisation / 1 = Lightsensor)
LC,02,6,Side Turn Signal Lights installed
LC,02,7,Seat Heating installed
LC,03,0,Relay Terminal 15 installed
LC,03,1,Rear Fog Lights (0 = 2 Rear Fog Lights / 1 = 1 Rear Fog Light)
LC,03,2,Reverse Driving Lights (0 = 2 Reverse Driving Lights / 1 = 1 Reverse Driving Light)
LC,03,3,Reverse Driving Light off when Rear Lid open
LC,03,5,Teardrop Wiping for Rear Window active
LC,03,6,2nd Battery installed
LC,04,0,Auxiliary Heater installed
LC,04,4,Activation of both Rear Fog Lights
LC,04,6,Rear Fog Lights deactivated
LC,05,0-7,50,Headlight Washer Delay
LC,05,0-7,50,Decimal Value (Resolution 50 ms) (Example: 20 is 20 x 50 = 1000 ms)
LC,06,0-7,50,Headlight Washer Activation Time
LC,06,0-7,50,Decimal Value (Resolution 50 ms) (Example: 16 is 16 x 50 = 800 ms)
LC,07,0-7,1,Turn Signal Front left/right as Parking Light Front left/right (USA and Canada)
LC,07,0-7,1,Decimal Value (Resolution: 1%)
LC,08,0-7,1,Daytime Running Light Dimming
LC,08,0-7,1,Decimal Value (Resolution: 1%)
LC,09,0-7,1,Rear Brake Light as Parking Light
LC,09,0-7,1,Decimal Value (Resolution: 1%)
LC,10,0-7,1,Rear Fog Light as Parking Light
LC,10,0-7,1,Decimal Value (Resolution: 1%)
LC,11,0-7,1,Front Parking Light Dimming
LC,11,0-7,1,Decimal Value (Resolution: 1%)
LC,12,0-7,1,Rear Parking Light Dimming
LC,12,0-7,1,Decimal Value (Resolution: 1%)
LC,13,0-7,1,Backup Function: Rear Side Turn Signal as Parking/Brake Light
LC,13,0-7,1,Decimal Value (Resolution: 1%)
LC,14,0-7,1,Backup Function: Front Parking Light as Side Turn Signals
LC,14,0-7,1,Decimal Value (Resolution: 1%)
LC,15,0-7,1,Backup Function: Rear Parking Light as Side Turn Signals
LC,15,0-7,1,Decimal Value (Resolution: 1%)
LC,16,0-7,1,Backup Function: Front Fog Lights as Low Beam Headlight
LC,16,0-7,1,Decimal Value (Resolution: 1%)
LC,17,0,Emergency Brake Flash Light active
LC,17,2,Heated Front Window installed
LC,17,3,Diagnosis Terminal 50 active
LC,18,0,Cold Diagnosis License Plate Lights active
LC,18,1,Cold Diagnosis Brake Lights active
LC,18,3,Cold Diagnosis Rear Fog Lights active
LC,18,4,Cold Diagnosis High Beam active
LC,18,5,Cold Diagnosis Turn Signals active
LC,18,6,Cold Diagnosis Back-Up Light active
LC,18,7,Cold Diagnosis Side Turn Signals active
LC,19,0,Cold Diagnosis Low Beam active
LC,19,1,Cold Diagnosis Front Parking Lights active
LC,19,2,Cold Diagnosis Rear Parking Lights active
LC,19,3,Diagnosis Rear Parking Lights active
LC,19,6,Electric Parking Brake installed
;
