;
; VAG-COM Label File
;
; Skoda Octavia (1U)
;
; Component: A/C Heating Electronics (J255) (#01) - Climatronic
;
; P/N: 1U?-907-044-???
;
; includes measuring blocks, basic setting and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1U-08.LBL
; 1Ux-907-044.LBL
;
; created on 12/Jun/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 13/Jun/2007
;
; requires VAG-COM 603.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
B000,0,Flap Motor Basic Setting
B000,1,Temperature Regulator Flap Motor (V68),Specified Value: 0
B000,2,Central Air Flap Motor (V70),Specified Value: 0
B000,3,Footwell/Defroster Flap Motor (V85),Specified Value: 0
B000,4,Air Flow Flap Motor (V71),Specified Value: 0
;
001,0,General Values
001,1,Comprossor,Shut-Off,Specification: 0 = Compressor Running (See Label File for more Details)
;  0 = Compressor Running
;  1 = Compressor OFF by Pressure Switch (F129): Refrigerant Pressure too High
;  2 = Compressor OFF by Fresh Air Blower (V2) or Fresh Air Blower Control Module (J126) Malfunction
;  3 = Compressor OFF by Pressure Switch (F129): Refrigerant Pressure too Low
;  5 = Compressor OFF by Missing Engine Speed Signal
;  6 = Compressor OFF by ECON Button
;  7 = Compressor OFF by OFF Button (via Fresh Air Blower Speed Buttons)
;  8 = Compressor OFF by Ambient Temperature below 3 °C (37 °F)
; 10 = Compressor OFF by Voltage below 9.5 V
; 11 = Compressor OFF by Coolant Temperature too High
; 12 = Compressor OFF by Engine OR Transmission Control Module
; 13 = Compressor OFF by Voltage above 17 V
; 14 = Compressor OFF by Evaporator Temperature
; 15 = Compressor OFF by Control Module Coding incorrect
; 16 = Compressor OFF by Climate Control Module (J255) Malfunction
; 17 = Compressor OFF by Pressure Sensor Malfunction
001,2,Engine Speed,recognized,Display Range: 0 = no/1 = yes
001,3,Vehicle Speed,,Display Range: 0...255 km/h
001,4,Standing Time,,Specification: 0...240 Min | 250 = Battery disconnected | 255 = Transfer Malfunction
;
002,0,Temperature Regulator Flap Motor (V68)
002,1,Measured Value,,Display Range: 0...255
002,2,Specified Value,,Display Range: 0...255
002,3,Flap Position,(air supply cooled),Specification: 150...250
002,4,Flap Position,(air supply heated),Specification: 5...100
;
003,0,Central Air Flap Motor (V70)
003,1,Measured Value,,Display Range: 0...255
003,2,Specified Value,,Display Range: 0...255
003,3,Flap Position,(air flow to panel),Specification: 150...250
003,4,Flap Position,(air flow to footwell),Specification: 5...100
;
004,0,Footwell/Defroster Flap Motor (V85)
004,1,Measured Value,,Display Range: 0...255
004,2,Specified Value,,Display Range: 0...255
004,3,Flap Position,(air flow to footwell),Specification: 150...250
004,4,Flap Position,(air flow to defrost.),Specification: 5...100
;
005,0,Air Flow Flap Motor (V71)
005,1,Measured Value,,Display Range: 0...255
005,2,Specified Value,,Display Range: 0...255
005,3,Flap Position,(fresh air flow),Specification: 150...250
005,4,Flap Position,(recirculating),Specification: 5...100
;
006,0,Temperatures I && Photo Sensor
006,1,Calculated,Temperature,Calculated from temperature sensor (G89) and outside air temperature sensor (G17)
006,2,Fresh Air Duct,Temperature (G89)
006,3,Outside Air,Temperature (G17)
006,4,Sunlight Photo,Sensor (G107),Display Range: 0...120 %
; 
007,0,Temperatures II
007,1,Temperature at,Center Outl. (G191)
007,2,Temperature at,Floor Outlet (G192)
007,3,Temperature at,A/C Panel (G56)
;
008,0,Voltages
008,1,Fresh Air Blower,(V2 - specified),Display Range: 0 V = Blower Off / 3.6 V = Blower Speed 1 / 12 V = Blower Speed 7
008,2,Fresh Air Blower,(V2 - actual),Specification: ± 0.8 V to Specification (in Field 1)
008,3,Voltage,(Terminal 15)
008,4,Voltage,A/C Clutch (N25)
;
009,0,Map Cooling
009,1,Relay/Valve,Map Cooling
009,2,Map Cooling,(Engine)
009,3,Fresh Air Blower,(V2) Stage 1,Range: ON/OFF
009,4,Coolant Fan,Request
;
010,0,Fresh Air Blower (V2) && Aux. Heater
010,1,Aux. Heater,Request,Range: ON/OFF
010,2,Aux. Heater,,Range: ON/OFF
010,3,Wiper,,Range: ON/OFF
010,4,Coolant,Temperature,-99.0 °C = Unused/Ignore
;
011,1,Dimming,(Terminal 58d),Range: 0.0...100.0 %
011,2,Idle Speed,Increase,Range: ON/OFF
;
013,0,CAN-Databus Communication
013,1,Status,CAN-Datenbus
013,2,CAN-Gateway,(J533)
013,3,Instrument Cluster,(J285),Wertebereich: Kombi 0/1
;
080,0,Advanced Control Module Identification I
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Heating/Air Condition (J255) Coding
C01,?xxxx: Compressor Version
C02,0 = Internally regulated
C03,1 = Internally regulated with temp. sensor behind evaporator
C04,2 = Externally regulated
C05,x?xxx: Vehicle Type
C06,1 = Skoda Octavia (1U)
C07,xx?xx: Country
C08,0 = Rest of World / 1 = Japan / 2 = USA
C09,xxx?x: Engine Cooling
C10,0 = w/o characteristic map cooling
C11,1 = with characteristic map cooling
C12,xxxx?: Equipment
C13,0 = with outside temperature indication
C14,1 = w/o outside temperature indication
;
