;
; VCDS Label File
;
; Copyright © 2008-2012 Ross-Tech, LLC
;
; VW Touareg (7L)
;
; Component: J234 - Airbag (#15) - VW8T
;
; P/N: 7L0-959-655-???
;
; includes measuring blocks, basic setting, security access, adaptation and misc
;
; created on 15/Feb/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 02/Feb/2012
;
; requires VCDS 11.2.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
B001,0,Seat Occupied Recognition Control Module (J706) Basic Setting
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Belt Tensioner,Rear Center,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Pyrotechnic Igniter,Battery Separating,Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nRange: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniters III (Side Airbags)
005,1,Side Airbag,Front Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Side Airbag,Front Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Side Airbag,Rear Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Side Airbag,Rear Pass. Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
007,0,Igniters IV (Head Airbags)
007,1,Head-Level Airbag,Driver Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Head-Level Airbag,Passenger Side,Specification: Correct\nRange: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch
010,1,Passenger,Airbag Status,Range: ON/OFF
010,2,Key Switch,Logic Contact 1,Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Ingniters V (Front Airbags Stage 2)
011,1,Airbag (Stage 2),Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Airbag (Stage 2),Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
016,0,Seat Occupied Recognition Control Module (J706) I
016,1,Serial Number,(1/2)
016,2,Serial Number,(3/4)
016,3,Serial Number,(5)
016,4,Calibration Status
;
018,0,Seat Occupied Recognition Control Module (J706) II
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration,Sensor
;
019,0,Seat Occupied Recognition Control Module (J706) III
019,1,Workshop Code,(Last Coding)
019,2,Workshop Code,(Last 0-Balance)
;
021,0,Igniter Resistance I (Front Airbags Stage 1 && Front Belt Tensioners)
021,1,Airbag (Stage 1),Driver Side
021,2,Airbag (Stage 1),Passenger Side
021,3,Belt Tensioner,Driver Side
021,4,Belt Tensioner,Passenger Side
;
022,0,Igniter Resistance II (Rear Belt Tensioners)
022,1,Belt Tensioner,Rear Left
022,2,Belt Tensioner,Rear Right
022,3,Belt Tensioner,Rear Center
022,4,Pyrotechnic Igniter,Battery Separating,
;
023,1,Supply Voltage,(Terminal 30)
;
025,0,Igniter Resistance III (Side Airbags)
025,1,Side Airbag,Driver Side
025,2,Side Airbag,Passenger Side
025,3,Side Airbag,Rear Left
025,4,Side Airbag,Rear Right
;
027,0,Igniter Resistance IV (Head-Level Airbags)
027,1,Head-Level Airbag,Driver Side
027,2,Head-Level Airbag,Passenger Side
;
031,0,Igniter Resistance V (Front Airbags Stage 2)
031,1,Airbag (Stage 2),Driver Side
031,2,Airbag (Stage 2),Passenger Side
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Instrument Cluster,(J285),Specification: Instruments 1\Range: Instruments 1/Instruments 0
125,2,Brake Electronics,(J104),Specification: ABS 1\Range: ABS 1/ABS 0
125,4,CAN-Gateway,(J533),Range: Gateway 1/Gateway 0
;
225,0,CAN-Databus Powertrain (TimeOut)
225,1,Instrument Cluster
225,2,Brake Electronics,(J104)
225,4,CAN-Gateway,(J533)
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Airbag (J234) Security Access
S01,30475 = Seat Occupied Recognition Basic Setting/Zero Balancing
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Seat Occupied Recognition Reset
A000,5,Seat Occupied Recognition Reset
A000,6,If a repair on the Seat Occupied Recognition
A000,7,has been performed a reset has to be performed too.
A000,8, 
A000,9,Prerequisites:
A000,10,* Seat in normal position.
A000,11,* Seat must NOT be occupied during the whole procedure.
A000,12,* Seatbelt must NOT be plugged in.
A000,13,* No faults in the system.
A000,14,* Interior temperature must be between 0 °C and 37 °C (32 °F and 98 °F).
A000,15, 
A000,16,NOTE: Perform Security Access first.
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,5,Front Passenger Airbag Deactivation
A001,6,0 - Airbag Enabled
A001,7,1 - Airbag Disabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
A002,0,Front Driver Airbag Deactivation
A002,1,Front Driver,Airbag
A002,2,Current Status
A002,5,Front Driver Airbag Deactivation
A002,6,0 - Airbag Enabled
A002,7,1 - Airbag Disabled
A002,8, 
A002,9,Note: Refer to Service Manual!
;
A003,0,Front Passenger Side Airbag Deactivation
A003,1,Front Passenger,Side Airbag
A003,2,Current Status
A003,5,Front Passenger Side Airbag Deactivation
A003,6,0 - Airbag Enabled
A003,7,1 - Airbag Disabled
A003,8, 
A003,9,Note: Refer to Service Manual!
;
A004,0,Front Driver Side Airbag Deactivation
A004,1,Front Driver,Side Airbag
A004,2,Current Status
A004,5,Front Driver Side Airbag Deactivation
A004,6,0 - Airbag Enabled
A004,7,1 - Airbag Disabled
A004,8, 
A004,9,Note: Refer to Service Manual!
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
I,
;
