;
; VCDS Label File
;
; Copyright © 2012+ Ross-Tech, LLC
;
; Audi A6 (4B) / Audi A8 (4D)
;
; Component: J347 - Interior Monitoring (#45) with Head Airbags
;
; P/N: 4B0-951-178-??? / 4D0-951-177-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4D-45.LBL
; 4B0-951-178.LBL
;
; includes measuring blocks, adaptation and coding
;
; created on 16/Nov/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 21/Feb/2013
;
; requires VCDS 11.11.4 or newer
;
;
;---------------------------------------------------
;
; Measuring block informations
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Input Signals,,0000 = Communication Wire NOT OK\n0001 = Communication Wire OK
; 0000 = Communication Wire NOT OK
; 0001 = Communication Wire OK
001,2,Sensor,Sensitivity,Specification: 50.0...100.0 % (see Adaptation Channel 001)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Sensitivity
A001,5,Sensitivity
A001,6,Sensitivity of the Ultra-Sound Sensors can be lowered/raised.
A001,7, 
A001,8,Range: 50...100 %
A001,9,Standard: 100 (= 100 %)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Interior Monitoring (J247) Coding
C01,00?0x: Type
C02,0 = Audi A8 (4D)
C03,1 = Audi A6 (4B)
C04,00x0?: Chassis Type
C05,1 = Limousine/Sedan
C06,2 = Avant/Wagon
;
