;
; VAG-COM Label File
;
; Audi A6 (4F)
;
; Component: J525 - Sound System (#47) - Bose
;
; P/N: 4F5-910-223-???
;
; includes measuring blocks, coding, adaptation and selective output test
;
; created on 12/Oct/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 30/May/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Voltages
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Voltage Status,,0000xxx1 = Term. S active\n0000xx1x = Term. 15 active\n0000x1xx = Term. X active\n00001xxx = Term. 50 active
;
002,0,MOST-Databus
002,1,Dynamic Address,(MOST-Databus)
002,2,Message Identity
002,3,Optical Transm.,Power Reduction
002,4,Send Diode,Temperature
;
003,1,Electrical Coding
003,2,Diagnostic Wire,,0 = Loop Break Diagnosis active\n1 = Databus static
;
004,1,Temperature,Analog Circuit
004,2,Temperature,Digital Circuit
004,3,Fan Speed
004,4,Speed
;
005,0,Microphone Voltage
005,1,Voltage,Microphone 1
005,2,Voltage,Microphone 2
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Bose Sound System (J525) Coding
C01,0000xx?: Equipment
C02,1 = Right-Hand-Drive with Fabric Trim and Diesel Engine
C03,2 = Left-Hand-Drive with Leather Trim and Diesel Engine
C04,3 = Right-Hand-Drive with Leather Trim and Diesel Engine
C05,4 = Left-Hand-Drive with Fabric Trim and Petrol Engine
C06,5 = Right-Hand-Drive with Fabric Trim and Petrol Engine
C07,6 = Left-Hand-Drive with Leather Trim and Petrol Engine
C08,7 = Right-Hand-Drive with Leather Trim and Petrol Engine
C09,8 = Left-Hand-Drive with Fabric Trim and Diesel Engine (Standard)
C10, 
C11,0000x?x: Microphone
C12,1 = Microphone (Standard)
C13,2 = Microphone (Voice Control)
C14,4 = Microphone (Analog Input (AUX))
C15,5 = Microphone (Voice Control and Analog Input (AUX))
C16, 
C17,0000?xx: Variant
C18,0 = Saloon
C19,1 = Avant
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
; See Adaptation Channels 112, 113, 114, 115 & 116 for further Details.
;
T870,Bass Speaker Front Left (R21)
T871,Bass Speaker Front Right (R23)
T874,Treble Speaker Front Left (R20)
T875,Treble Speaker Front Right (R22)
T876,Treble Speaker Rear Left (R14)
T877,Treble Speaker Rear Right (R16)
T2246,Center Midrang/Treble Speaker (R158)
T2457,Hat Shelf Speaker (R150)
T2558,Rear Left Midrange/Woofer Loudspeaker (R159)
T2559,Rear Right Midtange/Woofer Loudspeaker (R160)
T419,Midrange Speaker Front Left (R103)
T420,Midrange Speaker Front Right (R104)
;
