;
; VCDS Label File
;
; Copyright © 2009 Ross-Tech, LLC
;
; Bentley Continental (3W)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 3W?-920-???-???
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3W-17.LBL
; 3Wx-920-xxx-17.LBL
;
; includes measuring blocks, adaptation, coding and service reset
;
; created on 13/May/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 13/May/2009
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A004,0,Language
A004,1,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
;
A030,0,Tank Characteristic
A030,5,Tank Characteristic
A030,6,Parallel shift of tank characteristic by ± 6 °
A030,7,Standard Value: 128
A030,8,Value Range: 115...140
A030,9,Increments: 1 = 0.5 °
A030,8, 
A030,9,Adaptation should be performed after emptying the tank
A030,10,and filling it with XX liters of fuel.
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km/mi
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km/mi
A043,7,00015 = fixed Service Intervals (15.000 km - w/o Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
;
;A060,0,
;48207
;
;A061,0,
;59839
;
;A062,0,
;754
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00??x03: Options
C02,+01 = Brake Pad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Low Washer Fluid Warning active
C05,+16 = Radio/Navigation System installed
C06,00xx?03: Country
C07,1 = Europe
C08,2 = USA
C09,3 = Canada
C10,4 = Great Britain
C11,5 = Japan
C12,6 = Arabian States
C13,7 = Australia
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,43,ST_MADTS,1000,DIST
RD,44,ST_MATTS,1,ST_D
;
RJ,0,0,General Service Reset,,
RJ,0,1,2,0
;
