;
; VAG-COM Label File
;
; Ford Galaxy (7M) / Seat Alhambra (7M) / VW Sharan (7M)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 7M?-919-???-???
;
; includes measuring blocks, adaptation, login, coding and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; Diese Datei gehört zu einem Redirect-Paket, stellen
; Sie sicher, das alle folgenden Dateien vorhanden sind.
;
; 7M-17.LBL
; 7Mx-919-xxx-17.LBL
; 7Mx-920-xxx-17.LBL
;
; created on 18/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 01/Jan/2008
;
; requires VAG-COM 610.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Distance Impulse
001,2,Vehicle Speed
001,3,Engine Speed
001,4,Fuel Consumption
;
002,0,General
002,1,Odometer
002,2,Coolant,Temperature
002,3,Oil Temperature
002,4,Ambient,Temperature
;
003,0,General
003,1,Fuel Level
;
004,1,Oil Pressure,Switch 1,at 0.3 bar
004,2,Oil Pressure,Switch 2,at 0.9/1.4/1.8 bar
004,3,Odometer Display,Switch
004,4,MFD 1/2,Switch
;
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,00?xx: Anti-Lock Braking System (ABS)
C02,0 = Anti-Lock Braking System (ABS) not installed
C03,1 = Anti-Lock Braking System (ABS) installed
C04,00x?x: Transmission (Distance Impulse Number)
C05,1 = Automatic Trabsmission (3440)
C06,2 = Manual Transmission (4815)
C07,00xx?: Cylinders
C08,4 = 4-Cylinders
C09,6 = 6-Cylinders
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Tank Characteristic (Fuel Level Sensor)
A001,5,Tank Characteristic (Fuel Level Sensor)
A001,6,Range: 0...254
A001,7, 
A001,8,Refer to Factory Repair Manual for further details.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km.
A009,11, 
A009,12,NOTE: Perform Login first.
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,5,Oil Service (Distance),1000,km
RD,6,Oil Service (Time),1,Tage
RD,7,Inspection 1 (Time),1,Tage
RD,8,Inspection 2 (Distance),1000,km
;
RJ,0,0,Service Reset (Oil Service),,
RJ,0,1,5,0
RJ,0,2,6,0
;
RJ,1,0,Service Reset (Inspection 1),,
RJ,1,1,5,0
RJ,1,2,6,0
RJ,1,3,7,0
;
RJ,2,0,Service Reset (Inspection 2),,
RJ,2,1,5,0
RJ,2,2,6,0
RJ,2,3,7,0
RJ,2,4,8,0
;
RJ,3,0,Service Reset (Delivery Inspection),,
RJ,3,1,5,0
RJ,3,2,6,0
RJ,3,3,7,0
RJ,3,4,8,0
;
