;
; VCDS Label File
;
; Copyright © 2005-2009 Ross-Tech, LLC
;
; Audi A3 (8P)
;
; Component: J285 - Instrument Cluster (#17) MY 2004-2007
;
; P/N: 8P0-920-???-???
;
; includes measuring blocks, adaptation, coding, security access,
;          selective output test and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8P-17.LBL
; 8P0-920-xxx-17-MY7.LBL (MY 2004-2007)
; 8P0-920-xxx-17-MY8.LBL (MY 2008+)
;
; created on 14/Jul/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 07/Nov/2009
;
; requires VCDS 800.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure
001,4,Time
;
002,1,Mileage
002,2,Remote Clock,(Test Mode)
002,3,Tank Content
002,4,Ambient,Temperature
;
003,1,Coolant,Temperature
003,2,Standing Time
003,3,Dimming Signal,(Terminal 58d)
003,4,Dimming Signal,(Terminal 58s)
;
004,0,Supply Voltage && Outside Temperature
004,1,Supply Voltage,(Terminal 30)
004,2,Outside Temp.,(Climate Control)
004,3,Outside Temp.,(Display)
004,4,Phototransistor
;
005,0,Service Reminder
005,1,Distance since,Service exceeded,Unit: 100 km
005,2,Time since,Service exceeded,Unit: 1 day(s)
005,3,Remaining Dist.,until Service,Unit: 100 km
005,4,Remaining Time,until Service,Unit: 1 day(s)
;
006,1,Min. (M2) Oil Level,in Service Interval
006,2,Max. (M2) Oil Level,in Service Interval
006,3,Long Time Average,Oil Level Dif.,
006,4,Engine Hood,Contact,Display Range: open/closed
;
008,1,Short Time Mean,Oil Level Dif.,
008,2,Current (M2) Value
;
010,0,Adaptation Channels 003 && 004
010,1,Adaptation,Channel
010,2,Consumption,Correction,See Adaptation Channel 003
010,3,Adaptation,Channel
010,4,Language,,See Adaptation Channel 004
;
011,0,Adaptation Channels 009 && 019
011,1,Adaptation,Channel
011,2,Mileage,,See Adaptation Channel 009
011,3,Adaptation,Channel
011,4,Remote Control,Clock Synchron.,See Adaptation Channel 019
;
012,0,Adaptation Channels 040 && 041
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 040
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 041
;
013,0,Adaptation Channels 042 && 043
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 042
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 043
;
014,0,Adaptation Channels 044 && 049
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 044
014,3,Adaptation,Channel
014,4,Minimum Time to Service,See Adaptation Channel 049
;
015,0,Adaptation Channel 045
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 045
;
016,0,Adaptation Channels 047 && 048
016,1,Adaptation,Channel
016,2,Soot Entry,,See Adaptation Channel 047
016,3,Adaptation,Channel
016,4,Thermal Load,,See Adaptation Channel 048
;
019,0,Adaptation Channel 030
019,3,Adaptation,Channel
019,4,Fuel Gauge,Sender 1,See Adaptation Channel 030
;
020,0,Adaptation Channels 035 && 037
020,1,Adaptation,Channel
020,2,Engine Speed,Threshold,See Adaptation Channel 035
020,3,Adaptation,Channel
020,4,Breake Wear,Indicator Install.,See Adaptation Channel 037
;
021,0,Adaptation Channels 038 && 039
021,1,Adaptation,Channel
021,2,Oil Minimum,Detection Sensor,See Adaptation Channel 038
021,3,Adaptation,Channel
021,4,TOG,Installation,See Adaptation Channel 039
;
022,0,Adaptation Channels 018 && 020
022,1,Adaptation,Channel
022,2,Auxiliary,Heating,See Adaptation Channel 018
022,3,Adaptation,Channel
022,4,Configuration,,See Adaptation Channel 020
;
023,0,Adaptation Channels 080 && 081
023,1,Adaptation,Channel
023,2,Day/Month,of Delivery,See Adaptation Channel 080
023,3,Adaptation,Channel
023,4,Year,of Delivery,See Adaptation Channel 081
;
024,0,Adaptation Channels 082 && 033
024,1,Adaptation,Channel
024,2,Comfort Menu,,See Adaptation Channel 082
024,3,Adaptation,Channel
024,4,Full Calibration,,See Adaptation Channel 033
;
026,0,Fuel Level Sender
026,1,Fuel Sender 1,(Resistance)
026,2,Fuel Sender 1,(Tank Content)
026,3,Fuel Sender 2,(Resistance)
026,4,Fuel Sender 2,(Tank Content)
;
050,1,Mileage
050,2,Engine Speed
050,3,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
120,0,Connector Status I
120,1,Brake Fluid,Connector
120,2,Washer Fluid,Connector
120,3,Coolant Level,Connector
120,4,Oil Level,Connector
;
121,0,Connector Status II
121,1,Brake Pad Waer,Indicator Connect.
121,2,Parking Brake
121,3,Learned Keys
121,4,S-Contact,Status
;
122,0,Seat Belt Inquiry
122,1,Seat Belt Inquiry,Driver,Display Range: Open/Closed
122,2,Seat Belt Inquiry,Passenger,Display Range: Open/Closed
;
125,0,CAN-Databus Communication (Powertrain)
125,1,CAN-Gateway,,Specification: Gateway 1
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Instrument Cluster (J285) Security Access
S01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English (also Japan and Arabic States)
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish (also Mexico)
A004,11,6 = Portuguese/Brazil 
A004,12,7 = Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once before
A009,10,the current value is not over 100 km/62 mi.
A009,11,After changing the value can be corrected
A009,12,within the next 5 km/3 mi.
;
A018,0,Auxiliary Heater
A018,5,Auxiliary Heater
A018,6,?x: Engine Pre-Heating
A018,7,0 = Engine Pre-Heating inactive
A018,8,1 = Engine Pre-Heating active
A018,9, 
A018,10,x?: Auxiliary Heating
A018,11,0 = Auxiliary Heating not installed
A018,12,1 = Auxiliary Heating installed
A018,13,2 = Auxiliary Heating installed but OFF with Engine OFF
A018,14,3 = Auxiliary Ventilation installed
A018,15,4 = Auxiliary Ventilation but OFF with Engine OFF
;
A019,0,Remote Clock
A019,5,Remote Clock
A019,6,Set the remote clock synchronization time.
A019,7, 
A019,8,0 = Remote Clock not installed
A019,9,1...50 = Synchronization Time (in minutes)
;
A020,0,Additional Functions
A020,5,Additional Functions
A020,6,xx?: Ambient Temperature
A020,7,0 = Display inactive and Sensor not installed
A020,8,1 = Display active and Sensor installed
A020,9,2 = Display inactive and Sensor installed (Climate Control Display only)
A020,10,x?x: Date Display (MY 2005+)
A020,11,0 = Date Display inactive
A020,12,1 = Date Display active
A020,13,?xx: Range Display (MY 2005+)
A020,14,0 = Range Display inactive 
A020,14,1 = Range Display active
;
A029,0,Tank Characteristic (Fuel Level Sensor 2)
A029,5,Tank Characteristic (Fuel Level Sensor 2)
A029,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A029,7, 
A029,8,Standard Value: 128
A029,9,Value Range: 96...160 (-8.0...+8.0 l)
A029,10,Increments: 1 = 1 Ohm = 1/4 l
;
A030,0,Tank Characteristic (Fuel Level Sensor 1)
A030,5,Tank Characteristic (Fuel Level Sensor 1)
A030,6,Parallel shift of tank characteristic by +/- 32 Ohm.
A030,7, 
A030,8,Standard Value: 128
A030,9,Value Range: 96...160 (-8.0...+8.0 l)
A030,10,Increments: 1 = 1 Ohm = 1/4 l
;
A033,0,Tank Characteristic (Full Calibration)
A033,5,Tank Characteristic (Full Calibration)
A033,6,Non-parallel shift of the tank characterictic above a readout of 1/2.
A033,7, 
A033,8,Standard Value: 128
A033,9,Value Range: 112...144 (-4.0...+4.0 l)
A033,10,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A038,0,Oil Minimum Detection
A038,5,Oil Minimum Detection
A038,6,With this function the oil-minimum-warning at
A038,7,low oil level can be deactivated or activated.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km
A040,7, 
A040,8,NOTE: Adaptation channels 40-49 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-49 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A42,0,Minimum Mileage to Service
A42,5,Minimum Mileage to Service
A42,6,Increments: 1 = 100 km
A42,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A42,8,00150 - flexible Service Intervals (15.000 km - with Longlife)
A42,9,or (if coded to miles)
A42,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A42,11,00090 - flexible Service Intervals (9.000 mi - with Longlife)
A42,12, 
A42,13,NOTE: Adaptation channels 40-49 must be
A42,14,entered and stored in the following order:
A42,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A43,0,Maximum Mileage to Service
A43,5,Maximum Mileage to Service
A43,6,Increments: 1 = 100 km
A43,7,00080 - fixed Service Intervals (8.000 km - w/o Longlife)
A43,8,00300 - flexible Service Intervals (30.000 km - with Longlife)
A43,9,or (if coded to miles)
A43,10,00050 - fixed Service Intervals (5.000 mi - w/o Longlife)
A43,11,00190 - flexible Service Intervals (19.000 mi - with Longlife)
A43,12, 
A43,13,NOTE: Adaptation channels 40-49 must be
A43,14,entered and stored in the following order:
A43,15,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-49 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
A045,8, 
A045,9,NOTE: Adaptation channels 40-49 must be
A045,10,entered and stored in the following order:
A045,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display
A046,8, 
A046,9,NOTE: Adaptation channels 40-49 must be
A046,10,entered and stored in the following order:
A046,11,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
A047,9, 
A047,10,NOTE: Adaptation channels 40-49 must be
A047,11,entered and stored in the following order:
A047,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: Adaptation channels 40-49 must be
A048,11,entered and stored in the following order:
A048,12,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 = fixed Service Intervals (w/o Longlife)
A049,8,00365 = flexible Service Intervals (gasoline engines with Longlife)
A049,9,00730 = flexible Service Intervals (diesel engines with Longlife)
A049,10, 
A049,11,NOTE: Adaptation channels 40-49 must be
A049,12,entered and stored in the following order:
A049,13,45 > 42 > 43 > 44 > 49 > 40 > 41 > 46 > 47 > 48
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Equipment
C02,+01 = 2nd Fuel Tank Characteristic (All-Wheel Drive)
C03,+02 = Highline without DIS (for Midline variant 9Q3 - Automatic without DIS)
C04,+04 = Manual Transmission (not midline variant 9Q3)
C05,+08 = 2nd tire circumference pair (e.g. winter tires)
C05,+32 = AFS (Advanced Front Lighting System (cornering lights)
C06,xx?xx: Country
C07,0 = Germany / 1 = Rest of World (RoW - Left Hand Steering) / 2 = USA / 3 = Canada
C08,4 = Great Britain (Right Hand Steering) / 5 = Japan (Left Hand Steering) / 6 = Arabien States
C09,7 = Australia / 8 = Rest of World (RoW - Right Hand Steering) / 9 = Japan (Right Hand Steering)
C10,xxx?x: Seat Belt Warning
C11,0 - No Seat Belt Warning
C12,1 = Europe-NCAP (permanent visual warning and acoustic warning active for 91 seconds)	
C13,2 = USA and Canada OLD (visual and acoustic warning for 6 seconds)	
C14,3 = USA and Canada NAR-NEW (permanent visual warning and acoustic warning active every 30 seconds)
C15,4 = Europe-NCAP (including passenger - permanent visual warning and acoustic warning active for 91 seconds)	
C16,5 = USA and Canada OLD (including passenger - visual and acoustic warning for 6 seconds)	
C17,6 = USA and Canada NAR-NEW (including passenger - permanent visual warning and acoustic warning active every 30 seconds)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T666,Chime/Buzzer/Gong
T694,Switch and Instrument Lighting
T798,Segment Test
T1150,Analog Indicators
T1298,Instrument Cluster Lamp Test
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,100,DIST
RD,43,Max Mileage to Service,100,DIST
RD,44,Max Time to Service,1,Days
RD,45,Oil Quality,1,
RD,47,Soot Quantity,100,DIST
RD,48,Thermal Load,100,DIST
RD,49,Min Time to Service,1,Days
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Change to Fixed Intervals (Kilometers),,ST_FIXED
RJ,1,1,45,1
RJ,1,2,42,80
RJ,1,3,43,80
RJ,1,4,44,365
RJ,1,5,49,365
;
; Change to flexible intervals (kilometers)
RJ,2,0,Change to Flexible Intervals (Kilometers),ST_DIESEL,ST_FLEXIBLE
RJ,2,1,45,2
RJ,2,2,42,150
RJ,2,3,43,300
RJ,2,4,44,730
RJ,2,5,49,730
;
; Change to flexible intervals (kilometers)
RJ,3,0,Change to Flexible Intervals (Kilometers),ST_GASOLINE,ST_FLEXIBLE
RJ,3,1,45,2
RJ,3,2,42,150
RJ,3,3,43,300
RJ,3,4,44,730
RJ,3,5,49,365
;
; Change to fixed intervals (miles)
RJ,4,0,Change to Fixed Intervals (Miles),,ST_FIXED
RJ,4,1,45,1
RJ,4,2,42,50
RJ,4,3,43,50
RJ,4,4,44,365
RJ,4,5,49,365
;
; Change to flexible intervals (miles)
RJ,5,0,Change to Flexible Intervals (Miles),ST_DIESEL,ST_FLEXIBLE
RJ,5,1,45,2
RJ,5,2,42,90
RJ,5,3,43,190
RJ,5,4,44,730
RJ,5,5,49,730
;
; Change to flexible intervals (miles)
RJ,6,0,Change to Flexible Intervals (Miles),ST_GASOLINE,ST_FLEXIBLE
RJ,6,1,45,2
RJ,6,2,42,90
RJ,6,3,43,190
RJ,6,4,44,730
RJ,6,5,49,365
;
