;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; Audi A2 (8Z) / Audi A3 (8P) / Audi A4 (8E) / Audi A6 (4B)
; Audi TT (8N) / Audi TT (8J) / Audi R8 (42) / Seat Exeo (3R)
;
; Component: Radio-/Navigation System (#37/#56) - RNS-E
;
; P/N: 3R0-035-192-??? / 420-035-19?-??? / 4B0-035-19?-???
;      8E0-035-19?-??? / 8P0-035-19?-??? / 8Z0-035-19?-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3R-37.LBL
; 3R-56.LBL
; 42-37.LBL
; 42-56.LBL
; 4B-37.LBL
; 4B-56.LBL
; 8E-37.LBL
; 8E-56.LBL
; 8J-37.LBL
; 8J-56.LBL
; 8P-37.LBL
; 8P-56.LBL
; 8Z-37.LBL
; 8Z-56.LBL
; 8E0-035-192-RNSE.LBL
;
; created on 15/Aug/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 11/Mar/2008 by Kiss Lorand (kisslorand666@yahoo.com)
; updated on 04/May/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 17/Dec/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Basic Information
001,1,Battery Voltage,(Terminal 30)
001,2,Status,Terminal 15,,Range: ON/OFF/Invalid
001,3,Status,S-Contact,,Range: ON/OFF/Invalid
001,4,Operating,Temperature
;
002,0,Sound System && Telephone Mute
002,1,Connection to,Sound System
002,2,Connection Status,Sound System,Range: OK/OFF/Short Circuit
002,3,Telephone Mute
002,4,Status,Telephone Mute,Range: ON/OFF
;
003,0,Status of Front Loudspeakers (software level <80 does not differ left/right)
003,1,Loudspeakers,Front Left
003,2,Status Loudspkr.,Front Left,Range: OK/Short Circuit/Open Circuit/not active
003,3,Loudspeakers,Front Right
003,4,Status Loudspkr.,Front Right,Range: OK/Short Circuit/Open Circuit/not active
;
004,0,Vehicle Speed && Driving Direction
004,1,Speed Signal
004,2,Vehicle Speed,,via CAN from ABS
004,3,Driving Direction,,Range: forward/reverse/invalid
;
005,0,Status active Antenna
005,1,active
005,2,Antenna
005,3,Status,active Antenna,Range: OK/Short Circuit/Open Circuit
;
006,0,Status IF-Output
006,1,IF-Output
006,2,Status,IF-Output,Range: OK/Short Circuit/Open Circuit
;
007,0,Satellite/GPS Status
007,1,Received,Satellites
007,2,Received/Utilized,Satellites
007,3,GPS-Antenna
007,4,Status GPS-Ant.,(Remote Feeding),Range: OK/Short Circuit/Open Circuit
;
008,1,Comunication,CD-Changer,Range: OK/not OK
008,2,Status,CD-Changer,0 = OK\n1 = Focus Malfunction\n2 = Mechanical Malfunction\n3 = Media Missing
;
009,0,GPS-Status
009,1,GPS-Status
009,2,GPS-Status,Information,  0 = GPS-Info not available (Cold Start necessary)\n  1 = GPS-Info not available (Almanac or Last Position/Time known)\n  2 = NO FIX: Satellites received / Position Sensing not possible\n  3 = 2D FIX: Satellites received / 2-Dimensional Position Sensing \n  4 = 3D FIX: Satellites received / 3-Dimensional Position Sensing \n255 = GPS Antenna not connected
;   0 = GPS-Info not available (Cold Start necessary)
;   1 = GPS-Info not available (Almanac or Last Position/Time known)
;   2 = NO FIX: Satellites received / Position Sensing not possible
;   3 = 2D FIX: Satellites received / 2-Dimensional Position Sensing 
;   4 = 3D FIX: Satellites received / 3-Dimensional Position Sensing 
; 255 = GPS Antenna not connected
;
010,0,DVD-Status
010,1,DVD-Status
010,2,DVD-Status,Information,0 = CD/DVD not inserted\n1 = CD/DVD incorrect / No Navigation-DVD inserted\n2 = Navigation-DVD inserted but Reading Error occured\n3 = Navigation-DVD inserted and OK\n4 = Load/Eject Error (End Switch not recognized)\n5 = DVD-Drive Malfunction (Drive cannot be initialized)\n6 = Unknown Malfunction
; 0 = CD/DVD not inserted
; 1 = CD/DVD incorrect / No Navigation-DVD inserted
; 2 = Navigation-DVD inserted but Reading Error occured
; 3 = Navigation-DVD inserted and OK
; 4 = Load/Eject Error (End Switch not recognized)
; 5 = DVD-Drive Malfunction (Drive cannot be initialized)
; 6 = Unknown Malfunction
;
011,0,Name/Label,of CD/DVD
011,1,Name/Label,of CD/DVD
;
020,0,Button Diagnosis I
020,1,Function Buttons,,xxxxxxx1 = RADIO (USA-Version: FM/AM)\nxxxxxx1x = CD/TV (USA-Version: CD/SD)\nxxxxx1xx = NAME\nxxxx1xxx = TEL\nxxx1xxxx = NAV \nxx1xxxxx = INFO\nx1xxxxxx = CAR \n1xxxxxxx = SETUP
; xxxxxxx1 = RADIO (USA-Version: FM/AM)
; xxxxxx1x = CD/TV (USA-Version: CD/SD)
; xxxxx1xx = NAME
; xxxx1xxx = TEL
; xxx1xxxx = NAV 
; xx1xxxxx = INFO
; x1xxxxxx = CAR 
; 1xxxxxxx = SETUP
020,2,Control and,Arrow Buttons,xxxxxxx1 = Top Left Control Button\nxxxxxx1x = Bottom Left Control Button\nxxxxx1xx = Top Right Control Button\nxxxx1xxx = Bottom Right Control Button\nxxx1xxxx = RETURN\nxx1xxxxx = Left Arrow Button\nx1xxxxxx = Right Arrow Button\n1xxxxxxx = OPEN
; xxxxxxx1 = Top Left Control Button
; xxxxxx1x = Bottom Left Control Button
; xxxxx1xx = Top Right Control Button
; xxxx1xxx = Bottom Right Control Button
; xxx1xxxx = RETURN
; xx1xxxxx = Left Arrow Button
; x1xxxxxx = Right Arrow Button
; 1xxxxxxx = OPEN
;
021,0,Button Diagnosis I
021,1,Operated Buttons,,xx1 = Rotation Button depressed\nx1x = Volume Button depressed\n1xx = EJECT Button depressed
; xx1 = Rotation Button depressed
; x1x = Volume Button depressed
; 1xx = EJECT Button depressed
021,2,Control Knob,(Rotation Pulse),per Time Unit (Range: -127...+127)
021,3,ON/OFF Knob,(Rotation Pulse),per Time Unit (Range: -127...+127)
;
025,0,Card Reader Status
025,1,Card Reader 1
025,2,Status,Card Reader 1,--xxxxx1 - Card Reader ready\n--xxxx1x - Card inserted and ready\n--xxx1xx - Card is beeing read\n--xx1xxx - Card is beeing written\n--x1xxxx - No Card inserted\n--1xxxxx - Malfunction occured
; --xxxxx1 - Card Reader ready
; --xxxx1x - Card inserted and ready
; --xxx1xx - Card is beeing read
; --xx1xxx - Card is beeing written
; --x1xxxx - No Card inserted
; --1xxxxx - Malfunction occured
025,3,Card Reader 2
025,4,Status,Card Reader 2,--xxxxx1 - Card Reader ready\n--xxxx1x - Card inserted and ready\n--xxx1xx - Card is beeing read\n--xx1xxx - Card is beeing written\n--x1xxxx - No Card inserted\n--1xxxxx - Malfunction occured
; --xxxxx1 - Card Reader ready
; --xxxx1x - Card inserted and ready
; --xxx1xx - Card is beeing read
; --xx1xxx - Card is beeing written
; --x1xxxx - No Card inserted
; --1xxxxx - Malfunction occured
;
030,1,Gyro Rough Value,,If navigation turns clockwise the values become greater counter clockwise smaller
030,2,Number of days,since last Almanac,Range: 0 = today / 1 = yesterday / 255 = no data received
;
031,0,Longitude (current Position)
031,1,Longitude
031,2,Degrees,,Range: -180...+180
031,3,Minutes,,Range: 0...59
031,4,Seconds,,Range: 0...59
;
032,0,Latitude (current Position)
032,1,Latitude
032,2,Degrees,,Range: -90...+90
032,3,Minutes,,Range: 0...59
032,4,Seconds,,Range: 0...59
;
033,0,Height/Direction (current Position)
033,1,Height
033,2,Height,,Range: -500...+8000 m
033,3,Direction
033,4,Angle,,000 = North\n090 = East\n180 = South\n270 = West
;
034,0,Longitude (last stored Position)
034,1,Longitude
034,2,Degrees,,Range: -180...+180
034,3,Minutes,,Range: 0...59
034,4,Seconds,,Range: 0...59
;
035,0,Latitude (last stored Position)
035,1,Latitude
035,2,Degrees,,Range: -90...+90
035,3,Minutes,,Range: 0...59
035,4,Seconds,,Range: 0...59
;
036,0,Height/Direction (last stored Position)
036,1,Height
036,2,Height,,Range: -500...+8000 m
036,3,Direction
036,4,Angle,,000 = North\n090 = East\n180 = South\n270 = West
;
037,0,GPS-Date (0.0.2000 = No Reception)
037,1,Date
037,2,Day,,Range: 0...31
037,3,Month,,Range: 0...12
037,4,Year,,Range: 2000...9999
;
038,0,GPS-Time (00:00:00 = No Reception)
038,1,Time
038,2,Hours,,Range: 0...23
038,3,Minutes,,Range: 0...59
038,4,Seconds,,Range: 0...59
;
039,0,Dilution of Precision (DOP | 0 = No Reception)
039,1,Quality of Satellite,Constallation,Note: the smaller the value the better the value
039,2,HDOP,horizontal Quality,2 Coordinates (Range: 1...25.4)
039,3,VDOP,vertical Quality,1 Coordinate (only Height / Range: 1...25.4)
039,4,PDOP,entire Quality,3 Coordinates (Range: 1...25.4)
;
048,1,Received,Wheel Pulses
;
049,1,Dimming,Terminal 58d,Range: 0.0...100.0 % (127.5 % = Signal invalid)
049,2,Dimming,Terminal 58s,Range: 0.0...100.0 % (127.5 % = Signal invalid)
049,3,Telephone,Software-Mute,Range: ON/OFF/invalid
;
070,1,Reception Level
070,2,RDS,Malfunction Rate
070,3,TMC-Data,avialiable,Range: 0 = NO / 1 = YES
070,4,Received,TMC-Data Packets,Range: 0...65535
;
071,0,Satellite Identification I
071,1,Satellite ID,best Reception
071,2,Signal Strength
071,3,Satellite ID,2nd best Reception
071,4,Signal Strength
;
072,0,Satellite Identification II
072,1,Satellite ID,3rd best Reception
072,2,Signal Strength
072,3,Satellite ID,4th best Reception
072,4,Signal Strength
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio/Navigation (J401/RNS-E) Coding
C01,0?xxxxx: Brand/Model
C02,1 = Lamborghini Gallardo / 2 = Audi A3 (8P) / 3 = Audi A4 (8E) OR Seat Exeo (3R)
C03,4 = Audi A4 Cabriolet (8H) / 5 = Audi A6 (4B) / 6 = Audi TT (8J) / 7 = Audi R8 (42)
C04,0x?xxxx: Treble Speaker Diagnosis / Optical Parking Aid
C05,+1 = Front Treble Speaker Diagnosis inactive
C06,+2 = Optical Parking Aid installed/active
C07,0xx?xxx: Sound Characteristic
C08,0 = Linear Sound Characteristic / 1 = Audi A4 (8E) OR Seat Exeo (3R) / 2 = Audi A6 (4B)
C09,3 = Audi A4 Cabriolet (8H) / 4 = Audi TT (8J) / 5 = Audi A3 (8P) / 9 = Sound System
C10,0xxx?xx: Telephone Preparation
C11,1 = Telephone Preparation NOT installed / 2 = Telephone Preparation without Comfort Functionality
C12,3 = Telephone Preparation (Aftermarket Retrofit) / 6 = Telephone Preparation for North American Region (NAR)
; 4 = Telephone Preparation Nokia (Remote Feed Voltage for Microphone inactive)
; 5 = Telematic Europe (Remote Feed Voltage for Microphone inactive)
C13,7 = Telephone Preparation with Comfort Functionality
C14,0xxxx?x: Equipment I (1 = Standard/Basic Value - Add to the Sum of Options below!)
C15,+1 = Audi Music Interface (AMI/PR-UF7) installed
C16,+2 = Satellite Radio (SIRIUS/XM) installed
C17,+4 = Analog Input (AUX/PR-UF0/UF1/UF2) installed
C18,0xxxxx?: Equipment II (1 = Standard/Basic Value - Add to the Sum of Options below!)
C19,+1 = TV-Tuner (PR-QV1/QV9) installed
C20,+2 = CD-Changer or iPod/USB-Interface (PR-7A2/7A5/UF1/UF2) installed
C21,+4 = Multi-Function-Steering Wheel (MFSW) installed
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T850,Control Output Active: Radio Amplifier
T852,Loudspeaker(s) Front
T870,Bass Speaker Front Left (R21)
T871,Bass Speaker Front Right (R23)
T872,Bass Speaker Rear Left (R15)
T873,Bass Speaker Rear Right (R17)
T874,Treble Speaker Front Left (R20)
T875,Treble Speaker Front Right (R22)
T876,Treble Speaker Rear Left (R14)
T877,Treble Speaker Rear Right (R16)
T2247,Subwoofer (R148/R157)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Tire Circumference
A001,5,Tire Circumference
A001,6,The tire circumference is beeing adapted in "mm".
A001,7,A tire circumference list can be found here:
A001,8, 
A001,9,http://de.openobd.org/audi/rns.htm#reifen
;
A002,0,Wheel Impulse
A002,5,Wheel Impulse
A002,6,The Distance Impulse describes the amount of ABS Pulses per Wheel Revolution.
A002,7, 
A002,8,43 = Audi A3 (8P)/ Audi TT (8J) / Audi R8 (42)
A002,9,45 = Audi A4 (8E) OR Seat Exeo (3R)
A002,10, 
A002,11,NOTE: If "0" is entered as new Value the System calibrates
A002,12,itself automatically after a short distance and inputs a proper Value.
;
A003,0,Language (Screen)
A003,5,Language (Screen)
A003,6,0 = German
A003,7,1 = English (UK only)
A003,8,2 = French
A003,9,3 = Italian
A003,10,5 = Spanish
A003,11,6 = Portuguese
A003,12,7 = English (USA only)
;
A004,0,Rear View Camera
A004,5,Rear View Camera
A004,6,0 = Rear View Camera not installed
A004,7,1 = Rear View Camera (Lamborghini) installed
A004,8,2 = Rear View Camera (DDP/RNS-E HIGH) installed
A004,9,3 = Rear View Camera (BAP/RNS-E PU) installed
;
A005,0,Speed Threshold (Video In Motion)
A005,5,Speed Threshold (Video In Motion)
A005,6,0 = max. 0 km/h (only while Standing)
A005,7,1 = max. 5 km/h (Standard for Europe)
; 250 = unlocked units only/otherwise value will not be stored
;
A007,0,Settings
A007,5,Settings
A007,6,+01 = Distance in Miles
A007,7,+02 = Speed in mph
A007,8,+04 = Time in am/pm
A007,9,+08 = Date in MM:TT:JJJJ
A007,10,+16 = Repeat Voice Commands
;
A008,0,Speed Dependant Volume Control (GALA)
A008,5,Speed Dependant Volume Control (GALA)
A008,6,000 = Speed Dependant Volume Control (GALA) OFF
A008,7,001 = Charakteristics 1
A008,8,002 = Charakteristics 2
A008,9,003 = Charakteristics 3
A008,10,004 = Charakteristics 4
A008,11,005 = Charakteristics 5
A008,12,255 = GALA via Microphone (Bose AudioPilot)
;
A010,0,Region
A010,5,Region
A010,6,0 = Northern Hemisphere (Europe and North America)
A010,7,1 = Southern Hemisphere (Australia)
A010,8,2 = Southern Hemisphere (South Africa and South America)
A010,9,3 = Saudi Arabia etc.
A010,10, 
A010,11,Note: Reverts back to 0 after a Software Update.
;
A011,0,Language (Voice Control)
A011,5,Language (Voice Control)
A011,6,0 = German
A011,7,1 = English (UK only)
A011,8,2 = French
A011,9,3 = Italian
A011,10,5 = Spanish
A011,11,6 = Portuguese
A011,12,7 = English (USA only)
;
A018,0,Start Screen
A018,5,Start Screen (SW US 0150+/EU 0500+)
A018,6,Modifications of the Start Screen correspond
A018,7,with the Control Module Coding.
A018,8, 
A018,9,0 = Standard Start Screen
A018,10,1 = Audi S3 (8P) Start Screen
A018,11,2 = Audi S4 (8E) Start Screen
A018,12,3 = Audi RS4 (8E) Start Screen
A018,13,4 = Audi TT (8J) Start Screen
A018,14,5 = Audi R8 (42) Start Screen
A018,15,7 = Audi TT S (8J) Start Screen
A018,16,8 = Audi TT RS (8J) Start Screen
A018,17,9 = Audi R8 GT (42) Start Screen
;
A065,0,Read Test
A065,5,Read Test
A065,6,0 = Normal Operation
A065,7,1 = Short Read Test
A065,8,2 = Full Read Test
A065,9, 
A065,10,Note: These values are only used to initiate the test and will not be stored permanently.
;
A066,0,Self Test
;
A067,0,CD/DVD Ejection
A067,5,CD/DVD Ejection
A067,6,000 = Normal
A067,7,001 = Eject CD/DVD now (will not be saved)
A067,8,255 = Eject Button locked (i.e. Rental Car)
;
A068,0,Display Test
A068,5,Display Test
A068,6,0 = No Test Pattern
A068,7,1 = Red Test Pattern
A068,8,2 = Green Test Pattern
A068,9,3 = Blue Test Pattern
A068,10,4 = White Test Pattern
A068,11,5 = Black Test Pattern
A068,12,6 = Checkerboard Test Pattern
A068,13,7 = Checkerboard Test Pattern (inverted)
A068,14,8 = 64 Gray Scales Test Pattern (vertical Bar)
A068,15,9 = Special Test Pattern
A068,16, 
A068,17,Note: These values are only used to initiate the test and will not be stored permanently.
;
A069,0,Display Mechanism
A069,5,Display Mechanism
A069,6,000 = Display closed
A069,7,001 = Display open
A069,8,200 = Display partly opened (blocked)
A069,9,255 = Unknown Display Position
;
A70,0,Display Brightness
A70,5,Display Brightness
A70,6,0 = 0 % (OFF)
A70,7,1 = 20 %
A70,8,2 = 40 %
A70,9,3 = 60 %
A70,10,4 = 80 %
A70,11,5 = 100 %
;
A097,0,Software Downgrade
A097,5,Software Downgrade
A097,6,0 = Normal (Updates only)
A097,7,1 = Forced (Downgrades possible - older DVD/CD Version required)
;
A099,0,Transport Mode
A099,5,Transport Mode
A099,6,0 = Transport Mode inactive 
A099,7,1 = Transport Mode active
A099,8, 
A099,9,Note: Only used in models without CAN-Gateway like Audi A6 (4B).
;
A111,0,System Reset
A111,5,System Reset
A111,6,To initiate a system reset (cold boot) test "1" as new value.
A111,7,Note: Stored fault codes will not be cleared.
;
A112,0,Remote Control: Audio Source
A112,5,Remote Control: Audio Source
A112,6,0 = FM
A112,7,1 = AM
A112,8,2 = CD
A112,9,3 = TV
A112,10,4 = SAT
;
A114,0,Remote Control: FM Frequency
;
A115,0,Remote Control: AM Frequency
;
A116,0,Remote Control: XM Channel
;
A117,0,Remote Control: Signal Position
A117,5,Remote Control: Signal Position
A117,6,0 = Fader Center / Balance Center
A117,7,1 = Fader Front / Balance Left
A117,8,2 = Fader Front / Balance Right
A117,9,3 = Fader Rear / Balance Left
A117,10,4 = Fader Rear / Balance Right
;
A118,0,Remote Control: FM Seek
A118,5,Remote Control: FM Seek
A118,6,1 = Seek Up
A118,7,2 = Seek Down
;
A119,0,Remote Control: AM Seek
A119,5,Remote Control: AM Seek
A119,6,1 = Seek Up
A119,7,2 = Seek Down
;
A136,0,Voice Commands - Driver Position
A136,5,Voice Commands - Driver Position
A136,6,RNS-E Basic:
A136,7,03226 = Left-Hand-Drive (LHD)
A136,8,02632 = Right-Hand-Drive (RHD)
A136,9,RNS-E High/US:
A136,10,00005 = Left-Hand-Drive (LHD)
A136,11,00013 = Right-Hand-Drive (RHD)
;
