;
; VAG-COM Label File
;
; Audi A8 (4D)
;
; Component: J502 - Tire Pressure Monitoring (#65)
;
; P/N: 4D0-907-273-???
;
; includes measuring blocks, coding and adaptation
;
; created on 28/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 28/May/2006
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Wheel Sensor 1 Status I
001,1,Wheel Sensor,Position,No Display = Not yet recognized
001,2,Wheel,Temperature,Range: -40.0...120.0 °C
001,3,Wheel Pressure,(actual),No Display = Not yet recognized
001,4,Wheel Pressure,(specified),at 20.0 °C
;
002,0,Wheel Sensor 1 Status II
002,1,Wheel Sensor,Position,No Display = Not yet recognized
002,2,Remaining,Battery Life (Month)
;
003,0,Wheel Sensor 1 Status III
003,1,Wheel Sensor,Position,No Display = Not yet recognized
003,2,Wheel Sensor,Identification
003,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
003,4,Wheel Sensor,Battery Status
;
004,0,Wheel Sensor 2 Status I
004,1,Wheel Sensor,Position,No Display = Not yet recognized
004,2,Wheel,Temperature,Range: -40.0...120.0 °C
004,3,Wheel Pressure,(actual),No Display = Not yet recognized
004,4,Wheel Pressure,(specified),at 20.0 °C
;
005,0,Wheel Sensor 2 Status II
005,1,Wheel Sensor,Position,No Display = Not yet recognized
005,2,Remaining,Battery Life (Month)
;
006,0,Wheel Sensor 2 Status II
006,1,Wheel Sensor,Position,No Display = Not yet recognized
006,2,Wheel Sensor,Identification
006,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
006,4,Wheel Sensor,Battery Status
;
007,0,Wheel Sensor 3 Status I
007,1,Wheel Sensor,Position,No Display = Not yet recognized
007,2,Wheel,Temperature,Range: -40.0...120.0 °C
007,3,Wheel Pressure,(actual),No Display = Not yet recognized
007,4,Wheel Pressure,(specified),at 20.0 °C
;
008,0,Wheel Sensor 3 Status II
008,1,Wheel Sensor,Position,No Display = Not yet recognized
008,2,Remaining,Battery Life (Month)
;
009,0,Wheel Sensor 3 Status III
009,1,Wheel Sensor,Position,No Display = Not yet recognized
009,2,Wheel Sensor,Identification
009,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
009,4,Wheel Sensor,Battery Status
;
010,0,Wheel Sensor 4 Status I
010,1,Wheel Sensor,Position,No Display = Not yet recognized
010,2,Wheel,Temperature,Range: -40.0...120.0 °C
010,3,Wheel Pressure,(actual),No Display = Not yet recognized
010,4,Wheel Pressure,(specified),at 20.0 °C
;
011,0,Wheel Sensor 4 Status II
011,1,Wheel Sensor,Position,No Display = Not yet recognized
011,2,Remaining,Battery Life (Month)
;
012,0,Wheel Sensor 4 Status III
012,1,Wheel Sensor,Position,No Display = Not yet recognized
012,2,Wheel Sensor,Identification
012,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
012,4,Wheel Sensor,Battery Status
;
013,0,Spare Tire/Wheel Sensor I
013,1,Wheel Sensor,Position,No Display = Not yet recognized
013,2,Wheel,Temperature,Range: -40.0...120.0 °C
013,3,Wheel Pressure,(actual),No Display = Not yet recognized
013,4,Wheel Pressure,(specified),at 20.0 °C
;
014,0,Spare Tire/Wheel Sensor II
014,1,Wheel Sensor,Position,No Display = Not yet recognized
014,2,Remaining,Battery Life (Month)
;
015,0,Spare Tire/Wheel Sensor III
015,1,Wheel Sensor,Position,No Display = Not yet recognized
015,2,Wheel Sensor,Identification
015,3,Wheel Sensor,Status
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
015,4,Wheel Sensor,Battery Status
;
016,0,Wheel Sensor Status (from last Received Wheel ID) I
016,1,Wheel Sensor,Identification
016,2,Wheel Sensor,Status,No Display = Not yet recognized
; Status x0h = Storage Mode
; Status x1h = Standard Sending Mode
; Status x2h = Fast Sending Mode
; Status x3h = Temperature Shut-Off
; Status x4h (and above) = Faulty
016,3,Wheel Sensor,Battery Status
016,4,Wheel Pressure,(actual)
;
017,0,General
017,1,Work Shop Code,(Last Adaptation)
017,2,Voltage,(Terminal 30)
017,3,Vehicle Status,,0 = Vehicle driving (> 5 km/h)\n1 = Vehicle standing
017,4,Vehicle Speed
;
018,0,General
018,1,Outside,Temperature
;
020,0,General
020,1,CAN-Databus,Status (Comfort),Range: 2-Wire/1-Wire\nSpecification: 2-Wire
;
021,0,Antenna Diagnosis
021,1,Diagnosis,Status,See Adaptation Channel 17
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Tire Pressure Monitoring (J502) Coding
C01,?0xxx: Manufacturer
C02,1 = Volkswagen
C03,2 = Audi
C04, 
C05,x0?xx: Variant
C06,1 = 4 Antennas / 5 Wheels / 4-Wheel Monitoring
C07,2 = 4 Antennas / 5 Wheels / 5-Wheel Monitoring ("Full Size" Spare Tire)
C08,3 = 4 Antennas / 4 Wheels / 4-Wheel Monitoring ("Space Saving" Spare Tire)
C09, 
C10,x0x?x: Spec. Pressure (partial load)
C11,0 = 2.0 bar / 1 = 2.1 bar / 2 = 2.2 bar / 3 = 2.3 bar / 4 = 2.4 bar
C12,5 = 2.5 bar / 6 = 2.6 bar / 7 = 2.7 bar / 8 = 2.8 bar / 9 = 1.9 bar
C13, 
C14,x0xx?: Spec. Pressure (full load)
C05,0 = 3.0 bar / 1 = 3.1 bar / 2 = 3.2 bar / 3 = 3.3 bar / 4 = 2.4 bar
C16,5 = 2.5 bar / 6 = 2.6 bar / 7 = 2.7 bar / 8 = 2.8 bar / 9 = 2.9 bar
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A017,0,Antenna Diagnosis
A017,5,Antenna Diagnosis
A017,6,0 = ON
A017,7,1 = OFF
A017,8, 
A017,9,See Measuring Block 021.
;
